[Strings.0804]
; Non-Localizable strings
MSFT                                 = "Microsoft"
PROVIDER_NAME                        = "Intel"
COMPANY_NAME                         = "Intel Corporation"

; Localizable strings
NIC_MPCIEX_3945ABG                 = "Intel(R) PRO/无线 3945ABG 网络连接"
NIC_MPCIEX_3945BG                  = "Intel(R) PRO/无线 3945BG 网络连接"
NIC_MPCIEX_3965ABG                 = "Intel(R) PRO/无线 3965ABG 网络连接"
NIC_MPCIEX_3965BG                  = "Intel(R) PRO/无线 3965BG 网络连接"
NIC_MPCIEX_4965AGN                 = "Intel(R) 无线 WiFi 链接 4965AGN"
NIC_MPCIEX_4965AG                  = "Intel(R) 无线 WiFi 链接 4965AG"
NIC_MPCIEX_5300AGN_3x3_MC          = "Intel(R)  WiFi 链接 5300 AGN"
NIC_MPCIEX_5300AGN_3x3_HMC         = "Intel(R)  WiFi 链接 5300 AGN"

NIC_MPCIEX_5100AGN_1x2_MC          = "Intel(R) WiFi 链接 5100 AGN"
NIC_MPCIEX_5100AGN_1x2_MC_MOW2	   = "Intel(R) WiFi 链接 5100 AGN"
NIC_MPCIEX_5100AGN_1x2_MC_KRA	   = "Intel(R) WiFi 链接 5100 AGN"
NIC_MPCIEX_5100AGN_1x2_MC_BG	   = "Intel(R) WiFi 链接 5100 BG"
NIC_MPCIEX_5100AGN_1x2_MC_BGN	   = "Intel(R) WiFi 链接 5100 BGN"
NIC_MPCIEX_5100AGN_1x2_MC_ABG	   = "Intel(R) WiFi 链接 5100 ABG"
NIC_MPCIEX_5100AGN_1x2_HMC         = "Intel(R) WiFi 链接 5100 AGN"
NIC_MPCIEX_5100AGN_1x2_HMC_MOW2	   = "Intel(R) WiFi 链接 5100 AGN"
NIC_MPCIEX_5100AGN_1x2_HMC_KRA	   = "Intel(R) WiFi 链接 5100 AGN"
NIC_MPCIEX_5100AGN_1x2_HMC_BG	   = "Intel(R) WiFi 链接 5100 BG"
NIC_MPCIEX_5100AGN_1x2_HMC_BGN	   = "Intel(R) WiFi 链接 5100 BGN"
NIC_MPCIEX_5100AGN_1x2_HMC_ABG	   = "Intel(R) WiFi 链接 5100 ABG"

NIC_MPCIEX_AdapterModel_3945ABG    = "Intel(R) PRO/无线 3945ABG 网络连接"
NIC_MPCIEX_AdapterModel_3945BG     = "Intel(R) PRO/无线 3945BG 网络连接"
NIC_MPCIEX_AdapterModel_3965ABG    = "Intel(R) PRO/无线 3965ABG 网络连接"
NIC_MPCIEX_AdapterModel_3965BG     = "Intel(R) PRO/无线 3965BG 网络连接"
NIC_MPCIEX_AdapterModel_4965AGN    = "Intel(R) 无线 WiFi 链接 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     = "Intel(R) 无线 WiFi 链接 4965AG"
NIC_MPCIEX_AdapterModel_5300AGN_3x3  = "Intel(R) WiFi 链接 5300 AGN"
NIC_MPCIEX_AdapterModel_5100AGN_1x2  = "Intel(R) WiFi 链接 5100 AGN"
NIC_MPCIEX_AdapterModel_5100AGN_1x2_MOW2  = "Intel(R) WiFi 链接 5100 AGN"
NIC_MPCIEX_AdapterModel_5100AGN_1x2_KRA  = "Intel(R) WiFi 链接 5100 AGN"
NIC_MPCIEX_AdapterModel_5100AGN_1x2_BG  = "Intel(R) WiFi 链接 5100 BG"
NIC_MPCIEX_AdapterModel_5100AGN_1x2_BGN  = "Intel(R) WiFi 链接 5100 BGN"
NIC_MPCIEX_AdapterModel_5100AGN_1x2_ABG  = "Intel(R) WiFi 链接 5100 ABG"


NIC_DriverDesc_3945ABG               = "Intel(R) 无线 WiFi 链接 3945ABG 驱动程序"
NIC_Service_DispName_3945ABG         = "Intel(R) 无线 WiFi 链接 3945ABG 适配器驱动程序 "
NIC_Service_DispName_3945ABG_VISTA   = "适用于 Windows Vista 32 位的 Intel(R) 无线 WiFi 链接 3945ABG 适配器驱动程序 "
NIC_DriverDesc_3945BG                = "Intel(R) 无线 WiFi 链接 3945BG 驱动程序"
NIC_Service_DispName_3945BG_VISTA    = "适用于 Windows Vista 32 位的 Intel(R) 无线 WiFi 链接 3945BG 适配器驱动程序 "
NIC_DriverDesc_3965ABG               = "Intel(R) 无线 WiFi 链接 3965ABG 驱动程序"
NIC_Service_DispName_3965ABG_VISTA   = "适用于 Windows Vista 32 位的 Intel(R) 无线 WiFi 链接 3965ABG 适配器驱动程序 "
NIC_DriverDesc_3965BG                = "Intel(R) 无线 WiFi 链接 3965BG 驱动程序"
NIC_Service_DispName_3965BG_VISTA    = "适用于 Windows Vista 32 位的 Intel(R) 无线 WiFi 链接 3965BG 适配器驱动程序 "
NIC_DriverDesc_4965AGN               = "Intel(R) 无线 WiFi 链接 4965AGN 驱动程序"
NIC_Service_DispName_4965AGN_VISTA   = "适用于 Windows Vista 32 位的 Intel(R) 无线 WiFi 链接 4965AGN 适配器驱动程序 "
NIC_DriverDesc_4965AG          		   = "Intel(R) 无线 WiFi 链接 4965AG 驱动程序"
NIC_Service_DispName_4965AG_VISTA    = "适用于 Windows Vista 32 位的 Intel(R) 无线 WiFi 链接 4965AG 适配器驱动程序"
NIC_DriverDesc_5300AGN_3x3      		 = "Intel(R) WiFi 链接 5300 驱动程序"
NIC_Service_DispName_5300AGN3x3_VISTA = "适用于 Windows Vista 32 位的 Intel(R) WiFi 链接 5300 适配器驱动程序 "
NIC_DriverDesc_5100AGN_1x2     		   = "Intel(R) WiFi 链接 5100 驱动程序"
NIC_Service_DispName_5100AGN1x2_VISTA = "适用于 Windows Vista 32 位的 Intel(R) WiFi 链接 5100 适配器驱动程序"
NIC_DriverDesc_5100AGN_1x2_BG     		    = "Intel(R) WiFi 链接 5100 BG 驱动程序"
NIC_Service_DispName_5100AGN1x2_BG_VISTA = "适用于 Windows Vista 32 位的 Intel(R) WiFi 链接 5100 BG 适配器驱动程序"
NIC_DriverDesc_5100AGN_1x2_BGN     		    = "Intel(R) WiFi 链接 5100 BGN 驱动程序"
NIC_Service_DispName_5100AGN1x2_BGN_VISTA = "适用于 Windows Vista 32 位的 Intel(R) WiFi 链接 5100 BGN 适配器驱动程序"
NIC_DriverDesc_5100AGN_1x2_ABG     		    = "Intel(R) WiFi 链接 5100 ABG 驱动程序"
NIC_Service_DispName_5100AGN1x2_ABG_VISTA = "适用于 Windows Vista 32 位的 Intel(R) WiFi 链接 5100 ABG 适配器驱动程序"
NIC_DriverDesc_5100ABG_1x2_ABG     		    = "Intel(R) WiFi 链接 5100 ABG 驱动程序"
NIC_Service_DispName_5100ABG1x2_VISTA = "适用于 Windows Vista 32 位的 Intel(R) WiFi 链接 5100 ABG 适配器驱动程序"

NIC_Service_DispName_VISTA							= "适用于 Windows Vista 32 位的 Intel(R) Wireless WiFi 链接 5000 系列适配器驱动程序"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	= "临时通道 802.11 b/g"
RECOMMENDED_CHANNEL52_STR 	= "临时通道 802.11 a"
RECOMMENDED_BAND          	= "临时默认无线模式"
IBSS_TX_POWER_STR           = "传输功率"
ROAMING_AGGRESSIVENESS_STR	= "漫游入侵"
ADHOC_POWER_MANAGEMENT_STR	= "临时电源管理"
ADHOC_QOS_MODE_STR          = "临时 QoS 模式"
MIXED_MODE_PROTECTION_STR   = "混合模式保护"
THROUGHPUT_ENHANCEMENT_STR  = "吞吐量增强"
WIRELESS_MODE_STR           = "无线模式"
CHANNELWIDTH52              = "波段 5.2 的 802.11n 通道宽度"
CHANNELWIDTH24              = "波段 2.4 的 802.11n 通道宽度"
TGnMode                     = "802.11n 模式"
FAT_CHANNEL_TOLERANT		= "宽通道不包容性"

LOWEST_STR					= "最低"
MEDIUM_LOW_STR				= "中低"
MEDIUM_STR					= "中等"
MEDIUM_HIGH_STR				= "中高"
HIGHEST_STR					= "最高"
DISABLED_STR				= "已禁用"
ENABLED_STR 				= "已启用"
MAXIMUM_POWER_SAVING_STR	= "最大电源节省量"
NOISY_ENVIRONMENT_STR		= "杂音环境"
WMM_STR                     = "WMM "
CTS_TO_SELF_ENABLED_STR     = "已启用 CTS 到自身"
RTS_CTS_ENABLED_STR         = "RTS/CTS 已启用"
AUTO_STR                    = "自动"
CHANNELWIDTH20ONLY          = "仅 20 MHz"
CHANNELWIDTHAUTO            = "自动"
WMM_DISABLED_STR            = "已禁用 WMM"
WMM_ENABLED_STR             = "已启用 WMM"

SOURCEDISK1                  = "Intel(R) 无线 WiFi 链接 5000 系列安装光盘"

