[Strings.0804]
MSFT                        = "Microsoft"
Realtek                      	= "Realtek Semiconductor Corp."
SSID_STR			= "SSID"
CHANNEL_STR			= "频道"
NETWORK_TYPE_STR		= "网络类型"
LED_CONTROL_STR			= "LED 控件" 
POWER_SAVE_STR			= "节能模式"
WIFI_IBSS_STR			= "IBSS 默认 11b 模式"
RATE_ADAPTIVE_STR		= "速率自适应"
QOS_STR				= "QoS"
TransmitBuffers              	= "传输缓冲区"
ReceiveBuffers               	= "接收缓冲区"
FORCE_PRIORITY_STR		= "强制优先级"
HW_PARA_STR			= "从 HwParaFile 启动"
THREE_WIRE_MODE_STR		= "三线编程模式"
BOARD_TYPE_STR			= "板类型"
PROTECTION_MODE_STR		= "保护模式"
TPC_STR				= "传输功率控制"
TPC_POLARITY_STR		= "TPC 极性选择"
HIGH_POWER_STR			= "高能机制"
INIT_GAIN_STR			= "初始增益状态"
PSP_XLINK_STR			= "PSP XLink 模式"
ANTENNA_DIVERSITY_STR		= "SW 天线分集"
INACTIVE_POWER_SAVE		= "停用节能模式"
B_MODE_INIT_GAIN_STR		= "B 模式初始增益"
WL_MODE_STR			= "无线模式"
PREAMBLE_MODE_STR		= "报头模式"
FRAGTHRESH_STR			= "分段阈值"
RTSTHRESH_STR			= "RTS 阈值"
DOT11_ENABLE_STR		= "802.11d"
CAM_STR									="CAM"
MAX_PSP_STR							="MAX_PSP"
FAST_PSP_STR						="Fast_PSP"
DISABLE_STR							="禁用"
ENABLE_STR							="启用"
AD_HOC_STR							="临时"
INFRA_STR								="基础结构"
AUTO_SELECT_STR					="自动选择"
11A_STR									="IEEE 802.11 a"
11B_STR									="IEEE 802.11 b"
11BG_STR								="IEEE 802.11 b/g"
LONG_PREAMBLE_STR				="长报头"
SHORT_PREAMBLE_STR			="短报头"
AUTO_STR								="自动"

;; Source disk name
DISKNAME			= "Realtek RTL8187SE 无线局域网 PCIE 网络适配器驱动程序磁盘"
RTL8187Se.DeviceDesc.ASUS	= "Realtek RTL8187SE 802.11b/g 无线局域网 PCIE 网络"
RTL8187Se.DeviceDesc.MSI	= "802.11b/g 微型卡无线适配器"
RTL8187Se.DeviceDesc	     	= "Realtek RTL8187SE 无线局域网 PCIE 网络适配器"
RTL8187Se.DeviceDesc.DispName   = "Realtek RTL8187SE 无线局域网 PCIE 网络适配器"
