[Strings.0804]
;localizable

Generic="SDA Standard Compliant SD Host Controller Vendor"

;
;   Device Decription strings
;
PCI\VEN_104c&DEV_ac9f.DeviceDesc="Texas Instruments Secure Digital host controller"
PCI\VEN_1679&DEV_3000.DeviceDesc="Tokyo Electron SD Standard host controller"

PCI\VEN_1180&DEV_0822&SUBSYS_C01A144D&REV_17="Ricoh Secure Digital host controller R5C841"

PCI\VEN_1106&DEV_365B.DeviceDesc="VIA Secure Digital host controller"
PCI\VEN_1106&DEV_401B.DeviceDesc="VIA Secure Digital host controller"
PCI\VEN_1106&DEV_95D0.DeviceDesc="VIA Secure Digital host controller"

PCI\CC_080500.DeviceDesc="SDA Standard Compliant SD Host Controller"
PCI\CC_080501.DeviceDesc="SDA Standard Compliant SD Host Controller"

;
;
;
SDBUSSlot = "SD 主机槽 %1!u!"

;Non-localizable
SERVICE_KERNEL_DRIVER = 1
SERVICE_BOOT_START    = 0
SERVICE_SYSTEM_START  = 1
SERVICE_DEMAND_START  = 3
SERVICE_ERROR_NORMAL  = 1
SERVICE_ERROR_IGNORE  = 0
REG_EXPAND_SZ         = 0x00020000
REG_DWORD             = 0x00010001
REG_SZ                = 0x00000000

;
;Manufacturer name strings
;

Msft="Microsoft"
TED="Tokyo Electron Device"
TI="Texas Instruments"
Ricoh="Ricoh"
VIA="VIA Technologies, Inc"
MSI="MSI"
JMicron="JMicron"
