;*****************************************
; Copyright (c) Microsoft Corporation
;
;------------------------------------------------------------------------------

;******************************************************************************
; Version Section
;------------------------------------------------------------------------------
[version]
Signature   = "$Windows NT$"
Compatible  = 1
Class       = net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %MSFT%
DriverVer=03/26/2009,12.4.1.4

;*****************************************
; Manufacturer
;-----------------------------------------

[Manufacturer]
%COMPANY_NAME% = Device, NTx86.6.1

;[ControlFlags]
;ExcludeFromSelect = \ 
;        PCI\VEN_8086&DEV_4235&SUBSYS_10018086 , \ 
;        PCI\VEN_8086&DEV_4235&SUBSYS_10048086 , \ 
;        PCI\VEN_8086&DEV_4235&SUBSYS_11018086 , \ 
;        PCI\VEN_8086&DEV_4235&SUBSYS_11048086 , \ 
;        PCI\VEN_8086&DEV_4232&SUBSYS_13018086 , \ 
;        PCI\VEN_8086&DEV_4232&SUBSYS_13048086 , \ 
;        PCI\VEN_8086&DEV_4232&SUBSYS_13058086 , \ 
;        PCI\VEN_8086&DEV_4232&SUBSYS_13068086 , \ 
;        PCI\VEN_8086&DEV_4232&SUBSYS_12018086 , \ 
;        PCI\VEN_8086&DEV_4232&SUBSYS_12048086 , \ 
;        PCI\VEN_8086&DEV_4232&SUBSYS_12058086 , \ 
;        PCI\VEN_8086&DEV_4232&SUBSYS_12068086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11008086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11018086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11028086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11038086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11048086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11058086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11068086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11078086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11008086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11018086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11028086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11038086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11048086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11058086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11068086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11078086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10008086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10018086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10028086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10038086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10048086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10058086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10068086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10078086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10008086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10018086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10028086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10038086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10048086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10008086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10018086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10028086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10038086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10048086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10308086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10318086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10328086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10338086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10058086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10348086 , \ 
;        PCI\VEN_8086&DEV_4236&SUBSYS_10118086 , \ 
;        PCI\VEN_8086&DEV_4236&SUBSYS_10148086 , \ 
;        PCI\VEN_8086&DEV_4236&SUBSYS_11118086 , \ 
;        PCI\VEN_8086&DEV_4236&SUBSYS_11148086 , \ 
;        PCI\VEN_8086&DEV_4237&SUBSYS_12118086 , \ 
;        PCI\VEN_8086&DEV_4237&SUBSYS_12148086 , \ 
;        PCI\VEN_8086&DEV_4237&SUBSYS_12158086 , \ 
;        PCI\VEN_8086&DEV_4237&SUBSYS_12168086 , \ 
;        PCI\VEN_8086&DEV_4237&SUBSYS_13118086 , \ 
;        PCI\VEN_8086&DEV_4237&SUBSYS_13148086 , \ 
;        PCI\VEN_8086&DEV_4237&SUBSYS_13158086 , \ 
;        PCI\VEN_8086&DEV_4237&SUBSYS_13168086 , \ 
;        PCI\VEN_8086&DEV_4233&SUBSYS_11108086 , \ 
;        PCI\VEN_8086&DEV_4233&SUBSYS_11118086 , \ 
;        PCI\VEN_8086&DEV_4233&SUBSYS_11128086 , \ 
;        PCI\VEN_8086&DEV_4233&SUBSYS_11138086 , \ 
;        PCI\VEN_8086&DEV_4233&SUBSYS_11148086 , \ 
;        PCI\VEN_8086&DEV_4233&SUBSYS_11158086 , \ 
;        PCI\VEN_8086&DEV_4233&SUBSYS_11168086 , \ 
;        PCI\VEN_8086&DEV_4233&SUBSYS_11178086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_11108086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_11118086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_11128086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_11138086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_11148086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_11158086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_11168086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_11178086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_10108086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_10118086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_10128086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_10138086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_10148086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_10158086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_10168086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_10178086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10108086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10118086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10128086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10138086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10148086 , \ 
;        PCI\VEN_8086&DEV_4235&SUBSYS_10218086 , \ 
;        PCI\VEN_8086&DEV_4235&SUBSYS_10248086 , \ 
;        PCI\VEN_8086&DEV_4235&SUBSYS_11218086 , \ 
;        PCI\VEN_8086&DEV_4235&SUBSYS_11248086 , \ 
;        PCI\VEN_8086&DEV_4232&SUBSYS_12218086 , \ 
;        PCI\VEN_8086&DEV_4232&SUBSYS_12248086 , \ 
;        PCI\VEN_8086&DEV_4232&SUBSYS_12258086 , \ 
;        PCI\VEN_8086&DEV_4232&SUBSYS_12268086 , \ 
;        PCI\VEN_8086&DEV_4232&SUBSYS_13218086 , \ 
;        PCI\VEN_8086&DEV_4232&SUBSYS_13248086 , \ 
;        PCI\VEN_8086&DEV_4232&SUBSYS_13258086 , \ 
;        PCI\VEN_8086&DEV_4232&SUBSYS_13268086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11208086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11218086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11228086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11238086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11248086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11258086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11268086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11278086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11208086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11218086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11228086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11238086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11248086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11258086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11268086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11278086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10208086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10218086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10228086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10238086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10248086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10258086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10268086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10278086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10208086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10218086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10228086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10238086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10248086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10208086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10218086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10228086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10238086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10248086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10408086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10418086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10428086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10438086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10448086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10408086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10418086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10428086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10438086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10448086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10508086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10518086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10528086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10538086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10548086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10508086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10518086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10528086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10538086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10548086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_135B103C , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_135C103C , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_135D103C , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_135E103C , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_135F103C , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_135B103C , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_135C103C , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_135D103C , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_135E103C , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_135F103C , \ 
;        PCI\VEN_8086&DEV_4227&SUBSYS_10108086 , \ 
;        PCI\VEN_8086&DEV_4227&SUBSYS_10118086 , \ 
;        PCI\VEN_8086&DEV_4227&SUBSYS_10128086 , \ 
;        PCI\VEN_8086&DEV_4227&SUBSYS_10138086 , \ 
;        PCI\VEN_8086&DEV_4227&SUBSYS_10148086 , \ 

;*****************************************
;Device
;-----------------------------------------

;*****************************************
;Device VISTA
;-----------------------------------------
[Device.NTx86.6.1]

; GEN_5300_AGN_3x3_MC
%NIC_MPCIEX_5300AGN_3x3_MC% = Install_MPCIEX_GEN_5300_AGN_3x3_MC_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4235&SUBSYS_10018086 ; MOW2
%NIC_MPCIEX_5300AGN_3x3_MC% = Install_MPCIEX_GEN_5300_AGN_3x3_MC_VISTA_KRA    ,   PCI\VEN_8086&DEV_4235&SUBSYS_10048086 ; KRA

; GEN_5300_AGN_3x3_HMC
%NIC_MPCIEX_5300AGN_3x3_HMC% = Install_MPCIEX_GEN_5300_AGN_3x3_HMC_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4235&SUBSYS_11018086 ; MOW2
%NIC_MPCIEX_5300AGN_3x3_HMC% = Install_MPCIEX_GEN_5300_AGN_3x3_HMC_VISTA_KRA    ,   PCI\VEN_8086&DEV_4235&SUBSYS_11048086 ; KRA

; GEN_5100_AGN_1x2_HMC
%NIC_MPCIEX_5100AGN_1x2_HMC_MOW2% = Install_MPCIEX_GEN_5100_AGN_1x2_HMC_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4232&SUBSYS_13018086 ; MOW2
%NIC_MPCIEX_5100AGN_1x2_HMC_KRA% = Install_MPCIEX_GEN_5100_AGN_1x2_HMC_VISTA_KRA    ,   PCI\VEN_8086&DEV_4232&SUBSYS_13048086 ; KRA
%NIC_MPCIEX_5100AGN_1x2_HMC_BG% = Install_MPCIEX_GEN_5100_AGN_1x2_HMC_VISTA_BG    ,   PCI\VEN_8086&DEV_4232&SUBSYS_13058086 ; BG
%NIC_MPCIEX_5100AGN_1x2_HMC_ABG% = Install_MPCIEX_GEN_5100_AGN_1x2_HMC_VISTA_ABG    ,   PCI\VEN_8086&DEV_4232&SUBSYS_13068086 ; ABG

; GEN_5100_AGN_1x2_MC
%NIC_MPCIEX_5100AGN_1x2_MC_MOW2% = Install_MPCIEX_GEN_5100_AGN_1x2_MC_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4232&SUBSYS_12018086 ; MOW2
%NIC_MPCIEX_5100AGN_1x2_MC_KRA% = Install_MPCIEX_GEN_5100_AGN_1x2_MC_VISTA_KRA    ,   PCI\VEN_8086&DEV_4232&SUBSYS_12048086 ; KRA
%NIC_MPCIEX_5100AGN_1x2_MC_BG% = Install_MPCIEX_GEN_5100_AGN_1x2_MC_VISTA_BG    ,   PCI\VEN_8086&DEV_4232&SUBSYS_12058086 ; BG
%NIC_MPCIEX_5100AGN_1x2_MC_ABG% = Install_MPCIEX_GEN_5100_AGN_1x2_MC_VISTA_ABG    ,   PCI\VEN_8086&DEV_4232&SUBSYS_12068086 ; ABG

; GEN_4965_AGN_C
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_C_VISTA_MOW1    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11008086 ; MOW1
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_C_VISTA_MOW2    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11018086 ; MOW2
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_C_VISTA_RoW    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11028086 ; RoW
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_C_VISTA_JPN    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11038086 ; JPN
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_C_VISTA_KRA    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11048086 ; KRA
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_C_VISTA_SP1    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11058086 ; SP1
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_C_VISTA_SP2    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11068086 ; SP2
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_C_VISTA_SP3    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11078086 ; SP3

; GEN_4965_AGN
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11008086 ; MOW1
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11018086 ; MOW2
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_VISTA_RoW    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11028086 ; RoW
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_VISTA_JPN    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11038086 ; JPN
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_VISTA_KRA    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11048086 ; KRA
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_VISTA_SP1    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11058086 ; SP1
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_VISTA_SP2    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11068086 ; SP2
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_VISTA_SP3    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11078086 ; SP3

; GEN_4965_AG
%NIC_MPCIEX_4965AG% = Install_MPCIEX_GEN_4965_AG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10008086 ; MOW1
%NIC_MPCIEX_4965AG% = Install_MPCIEX_GEN_4965_AG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10018086 ; MOW2
%NIC_MPCIEX_4965AG% = Install_MPCIEX_GEN_4965_AG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10028086 ; RoW
%NIC_MPCIEX_4965AG% = Install_MPCIEX_GEN_4965_AG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10038086 ; JPN
%NIC_MPCIEX_4965AG% = Install_MPCIEX_GEN_4965_AG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10048086 ; KRA
%NIC_MPCIEX_4965AG% = Install_MPCIEX_GEN_4965_AG_VISTA_SP1    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10058086 ; SP1
%NIC_MPCIEX_4965AG% = Install_MPCIEX_GEN_4965_AG_VISTA_SP2    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10068086 ; SP2
%NIC_MPCIEX_4965AG% = Install_MPCIEX_GEN_4965_AG_VISTA_SP3    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10078086 ; SP3

; GEN_3965_ABG
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_GEN_3965_ABG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10008086 ; MOW1
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_GEN_3965_ABG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10018086 ; MOW2
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_GEN_3965_ABG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10028086 ; RoW
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_GEN_3965_ABG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10038086 ; JPN
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_GEN_3965_ABG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10048086 ; KRA

; GEN_3945_ABG
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_GEN_3945_ABG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10008086 ; MOW1
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_GEN_3945_ABG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10018086 ; MOW2
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_GEN_3945_ABG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10028086 ; RoW
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_GEN_3945_ABG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10038086 ; JPN
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_GEN_3945_ABG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10048086 ; KRA

; GEN_3945_ABG_SP1
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_GEN_3945_ABG_SP1_VISTA    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10308086 ;

; GEN_3945_ABG_SP2
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_GEN_3945_ABG_SP2_VISTA    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10318086 ;

; GEN_3945_ABG_SP3
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_GEN_3945_ABG_SP3_VISTA    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10328086 ;

; GEN_3945_ABG_SP4
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_GEN_3945_ABG_SP4_VISTA    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10338086 ;

; GEN_3945_BG
%NIC_MPCIEX_3945BG% = Install_MPCIEX_GEN_3945_BG_VISTA    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10058086 ;

; GEN_3945_BGX
%NIC_MPCIEX_3945BG% = Install_MPCIEX_GEN_3945_BGX_VISTA    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10348086 ;

; Lenovo_5300_AGN_3x3_MC
%NIC_MPCIEX_5300AGN_3x3_MC% = Install_MPCIEX_Lenovo_5300_AGN_3x3_MC_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4236&SUBSYS_10118086 ; MOW2
%NIC_MPCIEX_5300AGN_3x3_MC% = Install_MPCIEX_Lenovo_5300_AGN_3x3_MC_VISTA_KRA    ,   PCI\VEN_8086&DEV_4236&SUBSYS_10148086 ; KRA

; Lenovo_5300_AGN_3x3_HMC
%NIC_MPCIEX_5300AGN_3x3_HMC% = Install_MPCIEX_Lenovo_5300_AGN_3x3_HMC_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4236&SUBSYS_11118086 ; MOW2
%NIC_MPCIEX_5300AGN_3x3_HMC% = Install_MPCIEX_Lenovo_5300_AGN_3x3_HMC_VISTA_KRA    ,   PCI\VEN_8086&DEV_4236&SUBSYS_11148086 ; KRA

; Lenovo_5100_AGN_1x2_MC
%NIC_MPCIEX_5100AGN_1x2_MC_MOW2% = Install_MPCIEX_Lenovo_5100_AGN_1x2_MC_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4237&SUBSYS_12118086 ; MOW2
%NIC_MPCIEX_5100AGN_1x2_MC_KRA% = Install_MPCIEX_Lenovo_5100_AGN_1x2_MC_VISTA_KRA    ,   PCI\VEN_8086&DEV_4237&SUBSYS_12148086 ; KRA
%NIC_MPCIEX_5100AGN_1x2_MC_BG% = Install_MPCIEX_Lenovo_5100_AGN_1x2_MC_VISTA_BG    ,   PCI\VEN_8086&DEV_4237&SUBSYS_12158086 ; BG
%NIC_MPCIEX_5100AGN_1x2_MC_ABG% = Install_MPCIEX_Lenovo_5100_AGN_1x2_MC_VISTA_ABG    ,   PCI\VEN_8086&DEV_4237&SUBSYS_12168086 ; ABG

; Lenovo_5100_AGN_1x2_HMC
%NIC_MPCIEX_5100AGN_1x2_HMC_MOW2% = Install_MPCIEX_Lenovo_5100_AGN_1x2_HMC_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4237&SUBSYS_13118086 ; MOW2
%NIC_MPCIEX_5100AGN_1x2_HMC_KRA% = Install_MPCIEX_Lenovo_5100_AGN_1x2_HMC_VISTA_KRA    ,   PCI\VEN_8086&DEV_4237&SUBSYS_13148086 ; KRA
%NIC_MPCIEX_5100AGN_1x2_HMC_BG% = Install_MPCIEX_Lenovo_5100_AGN_1x2_HMC_VISTA_BG    ,   PCI\VEN_8086&DEV_4237&SUBSYS_13158086 ; BG
%NIC_MPCIEX_5100AGN_1x2_HMC_ABG% = Install_MPCIEX_Lenovo_5100_AGN_1x2_HMC_VISTA_ABG    ,   PCI\VEN_8086&DEV_4237&SUBSYS_13168086 ; ABG

; Lenovo_4965_AGN_C
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4233&SUBSYS_11108086 ; MOW1
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4233&SUBSYS_11118086 ; MOW2
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_RoW    ,   PCI\VEN_8086&DEV_4233&SUBSYS_11128086 ; RoW
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_JPN    ,   PCI\VEN_8086&DEV_4233&SUBSYS_11138086 ; JPN
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_KRA    ,   PCI\VEN_8086&DEV_4233&SUBSYS_11148086 ; KRA
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_SP1    ,   PCI\VEN_8086&DEV_4233&SUBSYS_11158086 ; SP1
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_SP2    ,   PCI\VEN_8086&DEV_4233&SUBSYS_11168086 ; SP2
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_SP3    ,   PCI\VEN_8086&DEV_4233&SUBSYS_11178086 ; SP3

; Lenovo_4965_AGN
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4230&SUBSYS_11108086 ; MOW1
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4230&SUBSYS_11118086 ; MOW2
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_VISTA_RoW    ,   PCI\VEN_8086&DEV_4230&SUBSYS_11128086 ; RoW
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_VISTA_JPN    ,   PCI\VEN_8086&DEV_4230&SUBSYS_11138086 ; JPN
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_VISTA_KRA    ,   PCI\VEN_8086&DEV_4230&SUBSYS_11148086 ; KRA
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_VISTA_SP1    ,   PCI\VEN_8086&DEV_4230&SUBSYS_11158086 ; SP1
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_VISTA_SP2    ,   PCI\VEN_8086&DEV_4230&SUBSYS_11168086 ; SP2
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_VISTA_SP3    ,   PCI\VEN_8086&DEV_4230&SUBSYS_11178086 ; SP3

; Lenovo_4965_AG
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Lenovo_4965_AG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4230&SUBSYS_10108086 ; MOW1
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Lenovo_4965_AG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4230&SUBSYS_10118086 ; MOW2
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Lenovo_4965_AG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4230&SUBSYS_10128086 ; RoW
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Lenovo_4965_AG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4230&SUBSYS_10138086 ; JPN
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Lenovo_4965_AG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4230&SUBSYS_10148086 ; KRA
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Lenovo_4965_AG_VISTA_SP1    ,   PCI\VEN_8086&DEV_4230&SUBSYS_10158086 ; SP1
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Lenovo_4965_AG_VISTA_SP2    ,   PCI\VEN_8086&DEV_4230&SUBSYS_10168086 ; SP2
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Lenovo_4965_AG_VISTA_SP3    ,   PCI\VEN_8086&DEV_4230&SUBSYS_10178086 ; SP3

; Lenovo_3965_ABG
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Lenovo_3965_ABG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10108086 ; MOW1
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Lenovo_3965_ABG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10118086 ; MOW2
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Lenovo_3965_ABG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10128086 ; RoW
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Lenovo_3965_ABG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10138086 ; JPN
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Lenovo_3965_ABG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10148086 ; KRA

; Dell_5300_AGN_3x3_MC
%NIC_MPCIEX_5300AGN_3x3_MC% = Install_MPCIEX_Dell_5300_AGN_3x3_MC_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4235&SUBSYS_10218086 ; MOW2
%NIC_MPCIEX_5300AGN_3x3_MC% = Install_MPCIEX_Dell_5300_AGN_3x3_MC_VISTA_KRA    ,   PCI\VEN_8086&DEV_4235&SUBSYS_10248086 ; KRA

; Dell_5300_AGN_3x3_HMC
%NIC_MPCIEX_5300AGN_3x3_HMC% = Install_MPCIEX_Dell_5300_AGN_3x3_HMC_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4235&SUBSYS_11218086 ; MOW2
%NIC_MPCIEX_5300AGN_3x3_HMC% = Install_MPCIEX_Dell_5300_AGN_3x3_HMC_VISTA_KRA    ,   PCI\VEN_8086&DEV_4235&SUBSYS_11248086 ; KRA

; Dell_5100_AGN_1x2_MC
%NIC_MPCIEX_5100AGN_1x2_MC_MOW2% = Install_MPCIEX_Dell_5100_AGN_1x2_MC_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4232&SUBSYS_12218086 ; MOW2
%NIC_MPCIEX_5100AGN_1x2_MC_KRA% = Install_MPCIEX_Dell_5100_AGN_1x2_MC_VISTA_KRA    ,   PCI\VEN_8086&DEV_4232&SUBSYS_12248086 ; KRA
%NIC_MPCIEX_5100AGN_1x2_MC_BG% = Install_MPCIEX_Dell_5100_AGN_1x2_MC_VISTA_BG    ,   PCI\VEN_8086&DEV_4232&SUBSYS_12258086 ; BG
%NIC_MPCIEX_5100AGN_1x2_MC_ABG% = Install_MPCIEX_Dell_5100_AGN_1x2_MC_VISTA_ABG    ,   PCI\VEN_8086&DEV_4232&SUBSYS_12268086 ; ABG

; Dell_5100_AGN_1x2_HMC
%NIC_MPCIEX_5100AGN_1x2_HMC_MOW2% = Install_MPCIEX_Dell_5100_AGN_1x2_HMC_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4232&SUBSYS_13218086 ; MOW2
%NIC_MPCIEX_5100AGN_1x2_HMC_KRA% = Install_MPCIEX_Dell_5100_AGN_1x2_HMC_VISTA_KRA    ,   PCI\VEN_8086&DEV_4232&SUBSYS_13248086 ; KRA
%NIC_MPCIEX_5100AGN_1x2_HMC_BG% = Install_MPCIEX_Dell_5100_AGN_1x2_HMC_VISTA_BG    ,   PCI\VEN_8086&DEV_4232&SUBSYS_13258086 ; BG
%NIC_MPCIEX_5100AGN_1x2_HMC_ABG% = Install_MPCIEX_Dell_5100_AGN_1x2_HMC_VISTA_ABG    ,   PCI\VEN_8086&DEV_4232&SUBSYS_13268086 ; ABG

; Dell_4965_AGN_C
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_C_VISTA_MOW1    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11208086 ; MOW1
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_C_VISTA_MOW2    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11218086 ; MOW2
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_C_VISTA_RoW    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11228086 ; RoW
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_C_VISTA_JPN    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11238086 ; JPN
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_C_VISTA_KRA    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11248086 ; KRA
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_C_VISTA_SP1    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11258086 ; SP1
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_C_VISTA_SP2    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11268086 ; SP2
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_C_VISTA_SP3    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11278086 ; SP3

; Dell_4965_AGN
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11208086 ; MOW1
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11218086 ; MOW2
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_VISTA_RoW    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11228086 ; RoW
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_VISTA_JPN    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11238086 ; JPN
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_VISTA_KRA    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11248086 ; KRA
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_VISTA_SP1    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11258086 ; SP1
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_VISTA_SP2    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11268086 ; SP2
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_VISTA_SP3    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11278086 ; SP3

; Dell_4965_AG
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Dell_4965_AG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10208086 ; MOW1
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Dell_4965_AG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10218086 ; MOW2
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Dell_4965_AG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10228086 ; RoW
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Dell_4965_AG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10238086 ; JPN
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Dell_4965_AG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10248086 ; KRA
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Dell_4965_AG_VISTA_SP1    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10258086 ; SP1
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Dell_4965_AG_VISTA_SP2    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10268086 ; SP2
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Dell_4965_AG_VISTA_SP3    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10278086 ; SP3

; Dell_3965_ABG
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Dell_3965_ABG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10208086 ; MOW1
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Dell_3965_ABG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10218086 ; MOW2
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Dell_3965_ABG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10228086 ; RoW
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Dell_3965_ABG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10238086 ; JPN
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Dell_3965_ABG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10248086 ; KRA

; Dell_3945_ABG
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Dell_3945_ABG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10208086 ; MOW1
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Dell_3945_ABG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10218086 ; MOW2
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Dell_3945_ABG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10228086 ; RoW
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Dell_3945_ABG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10238086 ; JPN
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Dell_3945_ABG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10248086 ; KRA

; Toshiba_3965_ABG
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Toshiba_3965_ABG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10408086 ; MOW1
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Toshiba_3965_ABG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10418086 ; MOW2
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Toshiba_3965_ABG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10428086 ; RoW
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Toshiba_3965_ABG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10438086 ; JPN
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Toshiba_3965_ABG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10448086 ; KRA

; Toshiba_3945_ABG
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Toshiba_3945_ABG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10408086 ; MOW1
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Toshiba_3945_ABG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10418086 ; MOW2
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Toshiba_3945_ABG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10428086 ; RoW
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Toshiba_3945_ABG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10438086 ; JPN

; Toshiba_3945_BGX
%NIC_MPCIEX_3945BG% = Install_MPCIEX_Toshiba_3945_BGX_VISTA    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10448086 ;

; Sony_3965_ABG
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Sony_3965_ABG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10508086 ; MOW1
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Sony_3965_ABG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10518086 ; MOW2
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Sony_3965_ABG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10528086 ; RoW
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Sony_3965_ABG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10538086 ; JPN
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Sony_3965_ABG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10548086 ; KRA

; Sony_3945_ABG
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Sony_3945_ABG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10508086 ; MOW1
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Sony_3945_ABG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10518086 ; MOW2
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Sony_3945_ABG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10528086 ; RoW
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Sony_3945_ABG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10538086 ; JPN
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Sony_3945_ABG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10548086 ; KRA

; HP_3965_ABG
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_HP_3965_ABG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4228&SUBSYS_135B103C ; MOW1
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_HP_3965_ABG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4228&SUBSYS_135C103C ; MOW2
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_HP_3965_ABG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4228&SUBSYS_135D103C ; RoW
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_HP_3965_ABG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4228&SUBSYS_135E103C ; JPN
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_HP_3965_ABG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4228&SUBSYS_135F103C ; KRA

; HP_3945_ABG
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_HP_3945_ABG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4222&SUBSYS_135B103C ; MOW1
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_HP_3945_ABG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4222&SUBSYS_135C103C ; MOW2
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_HP_3945_ABG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4222&SUBSYS_135D103C ; RoW
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_HP_3945_ABG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4222&SUBSYS_135E103C ; JPN
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_HP_3945_ABG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4222&SUBSYS_135F103C ; KRA

; IBM_3945_ABG
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_IBM_3945_ABG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4227&SUBSYS_10108086 ; MOW1
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_IBM_3945_ABG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4227&SUBSYS_10118086 ; MOW2
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_IBM_3945_ABG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4227&SUBSYS_10128086 ; RoW
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_IBM_3945_ABG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4227&SUBSYS_10138086 ; JPN

; IBM_3945_BG
%NIC_MPCIEX_3945BG% = Install_MPCIEX_IBM_3945_BG_VISTA    ,   PCI\VEN_8086&DEV_4227&SUBSYS_10148086 ;



;*****************************************
;INSTALL VISTA
;-----------------------------------------


;-----------------------------------------
; Intel  VISTA GEN_5300_AGN_3x3_MC
;-----------------------------------------

[Install_MPCIEX_GEN_5300_AGN_3x3_MC_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_GEN_5300_AGN_3x3_MC, Reg_GEN_5300_AGN_3x3_MC_MOW2, Reg_MPCIEX_5300AGN_3x3_MC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_5300_AGN_3x3_MC_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_5300_AGN_3x3_MC_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_5300_AGN_3x3_MC_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_GEN_5300_AGN_3x3_MC, Reg_GEN_5300_AGN_3x3_MC_KRA, Reg_MPCIEX_5300AGN_3x3_MC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_5300_AGN_3x3_MC_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_5300_AGN_3x3_MC_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA GEN_5300_AGN_3x3_HMC
;-----------------------------------------

[Install_MPCIEX_GEN_5300_AGN_3x3_HMC_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_GEN_5300_AGN_3x3_HMC, Reg_GEN_5300_AGN_3x3_HMC_MOW2, Reg_MPCIEX_5300AGN_3x3_HMC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_5300_AGN_3x3_HMC_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_5300_AGN_3x3_HMC_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_5300_AGN_3x3_HMC_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_GEN_5300_AGN_3x3_HMC, Reg_GEN_5300_AGN_3x3_HMC_KRA, Reg_MPCIEX_5300AGN_3x3_HMC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_5300_AGN_3x3_HMC_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_5300_AGN_3x3_HMC_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA GEN_5100_AGN_1x2_HMC
;-----------------------------------------

[Install_MPCIEX_GEN_5100_AGN_1x2_HMC_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_GEN_5100_AGN_1x2_HMC, Reg_GEN_5100_AGN_1x2_HMC_MOW2, Reg_MPCIEX_5100AGN_1x2_HMC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_5100_AGN_1x2_HMC_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_5100_AGN_1x2_HMC_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_5100_AGN_1x2_HMC_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_GEN_5100_AGN_1x2_HMC, Reg_GEN_5100_AGN_1x2_HMC_KRA, Reg_MPCIEX_5100AGN_1x2_HMC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_5100_AGN_1x2_HMC_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_5100_AGN_1x2_HMC_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_5100_AGN_1x2_HMC_VISTA_BG]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_BG, Reg_GEN_5100_AGN_1x2_HMC, Reg_GEN_5100_AGN_1x2_HMC_BG, Reg_MPCIEX_5100AGN_1x2_HMC, Reg_NDIS_VISTA, Reg_CoInstaller32
DelReg         = Reg_WirelessMode_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_5100_AGN_1x2_HMC_VISTA_BG.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_5100_AGN_1x2_HMC_VISTA_BG.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_5100_AGN_1x2_HMC_VISTA_ABG]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_GEN_5100_AGN_1x2_HMC, Reg_GEN_5100_AGN_1x2_HMC_ABG, Reg_MPCIEX_5100AGN_1x2_HMC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_5100_AGN_1x2_HMC_VISTA_ABG.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_5100_AGN_1x2_HMC_VISTA_ABG.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA GEN_5100_AGN_1x2_MC
;-----------------------------------------

[Install_MPCIEX_GEN_5100_AGN_1x2_MC_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_GEN_5100_AGN_1x2_MC, Reg_GEN_5100_AGN_1x2_MC_MOW2, Reg_MPCIEX_5100AGN_1x2_MC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_5100_AGN_1x2_MC_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_5100_AGN_1x2_MC_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_5100_AGN_1x2_MC_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_GEN_5100_AGN_1x2_MC, Reg_GEN_5100_AGN_1x2_MC_KRA, Reg_MPCIEX_5100AGN_1x2_MC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_5100_AGN_1x2_MC_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_5100_AGN_1x2_MC_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_5100_AGN_1x2_MC_VISTA_BG]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_BG, Reg_GEN_5100_AGN_1x2_MC, Reg_GEN_5100_AGN_1x2_MC_BG, Reg_MPCIEX_5100AGN_1x2_MC, Reg_NDIS_VISTA, Reg_CoInstaller32
DelReg         = Reg_WirelessMode_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_5100_AGN_1x2_MC_VISTA_BG.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_5100_AGN_1x2_MC_VISTA_BG.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_5100_AGN_1x2_MC_VISTA_ABG]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_GEN_5100_AGN_1x2_MC, Reg_GEN_5100_AGN_1x2_MC_ABG, Reg_MPCIEX_5100AGN_1x2_MC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_5100_AGN_1x2_MC_VISTA_ABG.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_5100_AGN_1x2_MC_VISTA_ABG.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA GEN_4965_AGN_C
;-----------------------------------------

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN_C, Reg_GEN_4965_AGN_C_MOW1, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_C_VISTA_MOW1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN_C, Reg_GEN_4965_AGN_C_MOW2, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_C_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN_C, Reg_GEN_4965_AGN_C_RoW, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_C_VISTA_RoW.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN_C, Reg_GEN_4965_AGN_C_JPN, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_C_VISTA_JPN.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN_C, Reg_GEN_4965_AGN_C_KRA, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_C_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_SP1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN_C, Reg_GEN_4965_AGN_C_SP1, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_SP1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_C_VISTA_SP1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_SP2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN_C, Reg_GEN_4965_AGN_C_SP2, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_SP2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_C_VISTA_SP2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_SP3]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN_C, Reg_GEN_4965_AGN_C_SP3, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_SP3.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_C_VISTA_SP3.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA GEN_4965_AGN
;-----------------------------------------

[Install_MPCIEX_GEN_4965_AGN_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN, Reg_GEN_4965_AGN_MOW1, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_VISTA_MOW1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN, Reg_GEN_4965_AGN_MOW2, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN, Reg_GEN_4965_AGN_RoW, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_VISTA_RoW.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN, Reg_GEN_4965_AGN_JPN, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_VISTA_JPN.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN, Reg_GEN_4965_AGN_KRA, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_VISTA_SP1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN, Reg_GEN_4965_AGN_SP1, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_VISTA_SP1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_VISTA_SP1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_VISTA_SP2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN, Reg_GEN_4965_AGN_SP2, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_VISTA_SP2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_VISTA_SP2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_VISTA_SP3]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN, Reg_GEN_4965_AGN_SP3, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_VISTA_SP3.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_VISTA_SP3.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA GEN_4965_AG
;-----------------------------------------

[Install_MPCIEX_GEN_4965_AG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AG, Reg_GEN_4965_AG_MOW1, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AG_VISTA_MOW1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AG, Reg_GEN_4965_AG_MOW2, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AG_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AG, Reg_GEN_4965_AG_RoW, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AG_VISTA_RoW.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AG, Reg_GEN_4965_AG_JPN, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AG_VISTA_JPN.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AG, Reg_GEN_4965_AG_KRA, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AG_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AG_VISTA_SP1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AG, Reg_GEN_4965_AG_SP1, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AG_VISTA_SP1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AG_VISTA_SP1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AG_VISTA_SP2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AG, Reg_GEN_4965_AG_SP2, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AG_VISTA_SP2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AG_VISTA_SP2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AG_VISTA_SP3]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AG, Reg_GEN_4965_AG_SP3, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AG_VISTA_SP3.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AG_VISTA_SP3.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA GEN_3965_ABG
;-----------------------------------------

[Install_MPCIEX_GEN_3965_ABG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3965_ABG, Reg_GEN_3965_ABG_MOW1, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3965_ABG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_GEN_3965_ABG_VISTA_MOW1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_3965_ABG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3965_ABG, Reg_GEN_3965_ABG_MOW2, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3965_ABG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_GEN_3965_ABG_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_3965_ABG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3965_ABG, Reg_GEN_3965_ABG_RoW, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3965_ABG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_GEN_3965_ABG_VISTA_RoW.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_3965_ABG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3965_ABG, Reg_GEN_3965_ABG_JPN, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3965_ABG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_GEN_3965_ABG_VISTA_JPN.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_3965_ABG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3965_ABG, Reg_GEN_3965_ABG_KRA, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3965_ABG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_GEN_3965_ABG_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA GEN_3945_ABG
;-----------------------------------------

[Install_MPCIEX_GEN_3945_ABG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3945_ABG, Reg_GEN_3945_ABG_MOW1, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3945_ABG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_GEN_3945_ABG_VISTA_MOW1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_3945_ABG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3945_ABG, Reg_GEN_3945_ABG_MOW2, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3945_ABG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_GEN_3945_ABG_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_3945_ABG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3945_ABG, Reg_GEN_3945_ABG_RoW, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3945_ABG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_GEN_3945_ABG_VISTA_RoW.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_3945_ABG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3945_ABG, Reg_GEN_3945_ABG_JPN, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3945_ABG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_GEN_3945_ABG_VISTA_JPN.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_3945_ABG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3945_ABG, Reg_GEN_3945_ABG_KRA, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3945_ABG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_GEN_3945_ABG_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA GEN_3945_ABG_SP1
;-----------------------------------------

[Install_MPCIEX_GEN_3945_ABG_SP1_VISTA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3945_ABG_SP1, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3945_ABG_SP1_VISTA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_3945_ABG_SP1_VISTA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA GEN_3945_ABG_SP2
;-----------------------------------------

[Install_MPCIEX_GEN_3945_ABG_SP2_VISTA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3945_ABG_SP2, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3945_ABG_SP2_VISTA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_3945_ABG_SP2_VISTA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA GEN_3945_ABG_SP3
;-----------------------------------------

[Install_MPCIEX_GEN_3945_ABG_SP3_VISTA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3945_ABG_SP3, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3945_ABG_SP3_VISTA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_3945_ABG_SP3_VISTA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA GEN_3945_ABG_SP4
;-----------------------------------------

[Install_MPCIEX_GEN_3945_ABG_SP4_VISTA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3945_ABG_SP4, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3945_ABG_SP4_VISTA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_3945_ABG_SP4_VISTA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA GEN_3945_BG
;-----------------------------------------

[Install_MPCIEX_GEN_3945_BG_VISTA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3945_BG, Reg_MPCIEX_3945BG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_BG
DelReg				 = Reg_Loudon_Obsolete , Reg_WirelessMode_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3945_BG_VISTA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_3945_BG_VISTA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA GEN_3945_BGX
;-----------------------------------------

[Install_MPCIEX_GEN_3945_BGX_VISTA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3945_BGX, Reg_MPCIEX_3945BG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_BG
DelReg				 = Reg_Loudon_Obsolete , Reg_WirelessMode_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3945_BGX_VISTA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_3945_BGX_VISTA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA Lenovo_5300_AGN_3x3_MC
;-----------------------------------------

[Install_MPCIEX_Lenovo_5300_AGN_3x3_MC_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_Lenovo_5300_AGN_3x3_MC, Reg_Lenovo_5300_AGN_3x3_MC_MOW2, Reg_MPCIEX_5300AGN_3x3_MC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_5300_AGN_3x3_MC_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_5300_AGN_3x3_MC_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_5300_AGN_3x3_MC_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_Lenovo_5300_AGN_3x3_MC, Reg_Lenovo_5300_AGN_3x3_MC_KRA, Reg_MPCIEX_5300AGN_3x3_MC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_5300_AGN_3x3_MC_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_5300_AGN_3x3_MC_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA


;-----------------------------------------
; Intel  VISTA Lenovo_5300_AGN_3x3_HMC
;-----------------------------------------

[Install_MPCIEX_Lenovo_5300_AGN_3x3_HMC_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_Lenovo_5300_AGN_3x3_HMC, Reg_Lenovo_5300_AGN_3x3_HMC_MOW2, Reg_MPCIEX_5300AGN_3x3_HMC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_5300_AGN_3x3_HMC_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_5300_AGN_3x3_HMC_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_5300_AGN_3x3_HMC_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_Lenovo_5300_AGN_3x3_HMC, Reg_Lenovo_5300_AGN_3x3_HMC_KRA, Reg_MPCIEX_5300AGN_3x3_HMC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_5300_AGN_3x3_HMC_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_5300_AGN_3x3_HMC_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA Lenovo_5100_AGN_1x2_MC
;-----------------------------------------

[Install_MPCIEX_Lenovo_5100_AGN_1x2_MC_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_Lenovo_5100_AGN_1x2_MC, Reg_Lenovo_5100_AGN_1x2_MC_MOW2, Reg_MPCIEX_5100AGN_1x2_MC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_5100_AGN_1x2_MC_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_5100_AGN_1x2_MC_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_5100_AGN_1x2_MC_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_Lenovo_5100_AGN_1x2_MC, Reg_Lenovo_5100_AGN_1x2_MC_KRA, Reg_MPCIEX_5100AGN_1x2_MC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_5100_AGN_1x2_MC_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_5100_AGN_1x2_MC_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_5100_AGN_1x2_MC_VISTA_BG]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_BG, Reg_Lenovo_5100_AGN_1x2_MC, Reg_Lenovo_5100_AGN_1x2_MC_BG, Reg_MPCIEX_5100AGN_1x2_MC, Reg_NDIS_VISTA, Reg_CoInstaller32
DelReg         = Reg_WirelessMode_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_5100_AGN_1x2_MC_VISTA_BG.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_5100_AGN_1x2_MC_VISTA_BG.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_5100_AGN_1x2_MC_VISTA_ABG]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_Lenovo_5100_AGN_1x2_MC, Reg_Lenovo_5100_AGN_1x2_MC_ABG, Reg_MPCIEX_5100AGN_1x2_MC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_5100_AGN_1x2_MC_VISTA_ABG.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_5100_AGN_1x2_MC_VISTA_ABG.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA Lenovo_5100_AGN_1x2_HMC
;-----------------------------------------

[Install_MPCIEX_Lenovo_5100_AGN_1x2_HMC_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_Lenovo_5100_AGN_1x2_HMC, Reg_Lenovo_5100_AGN_1x2_HMC_MOW2, Reg_MPCIEX_5100AGN_1x2_HMC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_5100_AGN_1x2_HMC_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_5100_AGN_1x2_HMC_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_5100_AGN_1x2_HMC_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_Lenovo_5100_AGN_1x2_HMC, Reg_Lenovo_5100_AGN_1x2_HMC_KRA, Reg_MPCIEX_5100AGN_1x2_HMC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_5100_AGN_1x2_HMC_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_5100_AGN_1x2_HMC_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_5100_AGN_1x2_HMC_VISTA_BG]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_BG, Reg_Lenovo_5100_AGN_1x2_HMC, Reg_Lenovo_5100_AGN_1x2_HMC_BG, Reg_MPCIEX_5100AGN_1x2_HMC, Reg_NDIS_VISTA, Reg_CoInstaller32
DelReg         = Reg_WirelessMode_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_5100_AGN_1x2_HMC_VISTA_BG.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_5100_AGN_1x2_HMC_VISTA_BG.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_5100_AGN_1x2_HMC_VISTA_ABG]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_Lenovo_5100_AGN_1x2_HMC, Reg_Lenovo_5100_AGN_1x2_HMC_ABG, Reg_MPCIEX_5100AGN_1x2_HMC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_5100_AGN_1x2_HMC_VISTA_ABG.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_5100_AGN_1x2_HMC_VISTA_ABG.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA Lenovo_4965_AGN_C
;-----------------------------------------

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN_C, Reg_Lenovo_4965_AGN_C_MOW1, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_MOW1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN_C, Reg_Lenovo_4965_AGN_C_MOW2, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN_C, Reg_Lenovo_4965_AGN_C_RoW, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_RoW.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN_C, Reg_Lenovo_4965_AGN_C_JPN, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_JPN.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN_C, Reg_Lenovo_4965_AGN_C_KRA, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_SP1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN_C, Reg_Lenovo_4965_AGN_C_SP1, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_SP1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_SP1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_SP2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN_C, Reg_Lenovo_4965_AGN_C_SP2, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_SP2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_SP2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_SP3]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN_C, Reg_Lenovo_4965_AGN_C_SP3, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_SP3.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_SP3.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA Lenovo_4965_AGN
;-----------------------------------------

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN, Reg_Lenovo_4965_AGN_MOW1, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_VISTA_MOW1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN, Reg_Lenovo_4965_AGN_MOW2, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN, Reg_Lenovo_4965_AGN_RoW, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_VISTA_RoW.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN, Reg_Lenovo_4965_AGN_JPN, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_VISTA_JPN.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN, Reg_Lenovo_4965_AGN_KRA, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_SP1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN, Reg_Lenovo_4965_AGN_SP1, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_SP1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_VISTA_SP1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_SP2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN, Reg_Lenovo_4965_AGN_SP2, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_SP2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_VISTA_SP2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_SP3]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN, Reg_Lenovo_4965_AGN_SP3, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_SP3.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_VISTA_SP3.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA Lenovo_4965_AG
;-----------------------------------------

[Install_MPCIEX_Lenovo_4965_AG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AG, Reg_Lenovo_4965_AG_MOW1, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AG_VISTA_MOW1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AG, Reg_Lenovo_4965_AG_MOW2, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AG_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AG, Reg_Lenovo_4965_AG_RoW, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AG_VISTA_RoW.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AG, Reg_Lenovo_4965_AG_JPN, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AG_VISTA_JPN.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AG, Reg_Lenovo_4965_AG_KRA, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AG_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AG_VISTA_SP1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AG, Reg_Lenovo_4965_AG_SP1, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AG_VISTA_SP1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AG_VISTA_SP1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AG_VISTA_SP2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AG, Reg_Lenovo_4965_AG_SP2, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AG_VISTA_SP2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AG_VISTA_SP2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AG_VISTA_SP3]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AG, Reg_Lenovo_4965_AG_SP3, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AG_VISTA_SP3.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AG_VISTA_SP3.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA Lenovo_3965_ABG
;-----------------------------------------

[Install_MPCIEX_Lenovo_3965_ABG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_3965_ABG, Reg_Lenovo_3965_ABG_MOW1, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_3965_ABG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Lenovo_3965_ABG_VISTA_MOW1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_3965_ABG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_3965_ABG, Reg_Lenovo_3965_ABG_MOW2, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_3965_ABG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Lenovo_3965_ABG_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_3965_ABG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_3965_ABG, Reg_Lenovo_3965_ABG_RoW, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_3965_ABG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Lenovo_3965_ABG_VISTA_RoW.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_3965_ABG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_3965_ABG, Reg_Lenovo_3965_ABG_JPN, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_3965_ABG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Lenovo_3965_ABG_VISTA_JPN.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_3965_ABG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_3965_ABG, Reg_Lenovo_3965_ABG_KRA, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_3965_ABG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Lenovo_3965_ABG_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA


;-----------------------------------------
; Intel  VISTA Dell_5300_AGN_3x3_MC
;-----------------------------------------

[Install_MPCIEX_Dell_5300_AGN_3x3_MC_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_Dell_5300_AGN_3x3_MC, Reg_Dell_5300_AGN_3x3_MC_MOW2, Reg_MPCIEX_5300AGN_3x3_MC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_5300_AGN_3x3_MC_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_5300_AGN_3x3_MC_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_5300_AGN_3x3_MC_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_Dell_5300_AGN_3x3_MC, Reg_Dell_5300_AGN_3x3_MC_KRA, Reg_MPCIEX_5300AGN_3x3_MC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_5300_AGN_3x3_MC_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_5300_AGN_3x3_MC_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA Dell_5300_AGN_3x3_HMC
;-----------------------------------------

[Install_MPCIEX_Dell_5300_AGN_3x3_HMC_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_Dell_5300_AGN_3x3_HMC, Reg_Dell_5300_AGN_3x3_HMC_MOW2, Reg_MPCIEX_5300AGN_3x3_HMC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_5300_AGN_3x3_HMC_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_5300_AGN_3x3_HMC_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_5300_AGN_3x3_HMC_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_Dell_5300_AGN_3x3_HMC, Reg_Dell_5300_AGN_3x3_HMC_KRA, Reg_MPCIEX_5300AGN_3x3_HMC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_5300_AGN_3x3_HMC_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_5300_AGN_3x3_HMC_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA Dell_5100_AGN_1x2_MC
;-----------------------------------------

[Install_MPCIEX_Dell_5100_AGN_1x2_MC_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_Dell_5100_AGN_1x2_MC, Reg_Dell_5100_AGN_1x2_MC_MOW2, Reg_MPCIEX_5100AGN_1x2_MC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_5100_AGN_1x2_MC_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_5100_AGN_1x2_MC_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_5100_AGN_1x2_MC_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_Dell_5100_AGN_1x2_MC, Reg_Dell_5100_AGN_1x2_MC_KRA, Reg_MPCIEX_5100AGN_1x2_MC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_5100_AGN_1x2_MC_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_5100_AGN_1x2_MC_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_5100_AGN_1x2_MC_VISTA_BG]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_BG, Reg_Dell_5100_AGN_1x2_MC, Reg_Dell_5100_AGN_1x2_MC_BG, Reg_MPCIEX_5100AGN_1x2_MC, Reg_NDIS_VISTA, Reg_CoInstaller32
DelReg         = Reg_WirelessMode_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_5100_AGN_1x2_MC_VISTA_BG.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_5100_AGN_1x2_MC_VISTA_BG.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_5100_AGN_1x2_MC_VISTA_ABG]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_Dell_5100_AGN_1x2_MC, Reg_Dell_5100_AGN_1x2_MC_ABG, Reg_MPCIEX_5100AGN_1x2_MC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_5100_AGN_1x2_MC_VISTA_ABG.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_5100_AGN_1x2_MC_VISTA_ABG.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA Dell_5100_AGN_1x2_HMC
;-----------------------------------------

[Install_MPCIEX_Dell_5100_AGN_1x2_HMC_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_Dell_5100_AGN_1x2_HMC, Reg_Dell_5100_AGN_1x2_HMC_MOW2, Reg_MPCIEX_5100AGN_1x2_HMC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_5100_AGN_1x2_HMC_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_5100_AGN_1x2_HMC_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_5100_AGN_1x2_HMC_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_Dell_5100_AGN_1x2_HMC, Reg_Dell_5100_AGN_1x2_HMC_KRA, Reg_MPCIEX_5100AGN_1x2_HMC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_5100_AGN_1x2_HMC_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_5100_AGN_1x2_HMC_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_5100_AGN_1x2_HMC_VISTA_BG]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_BG, Reg_Dell_5100_AGN_1x2_HMC, Reg_Dell_5100_AGN_1x2_HMC_BG, Reg_MPCIEX_5100AGN_1x2_HMC, Reg_NDIS_VISTA, Reg_CoInstaller32
DelReg         = Reg_WirelessMode_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_5100_AGN_1x2_HMC_VISTA_BG.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_5100_AGN_1x2_HMC_VISTA_BG.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_5100_AGN_1x2_HMC_VISTA_ABG]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_SHP, Reg_NDI, Reg_NDI_SHP, Reg_NDI_ABG, Reg_Dell_5100_AGN_1x2_HMC, Reg_Dell_5100_AGN_1x2_HMC_ABG, Reg_MPCIEX_5100AGN_1x2_HMC, Reg_NDIS_VISTA, Reg_CoInstaller32
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_5100_AGN_1x2_HMC_VISTA_ABG.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_5100_AGN_1x2_HMC_VISTA_ABG.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA Dell_4965_AGN_C
;-----------------------------------------

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN_C, Reg_Dell_4965_AGN_C_MOW1, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_C_VISTA_MOW1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN_C, Reg_Dell_4965_AGN_C_MOW2, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_C_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN_C, Reg_Dell_4965_AGN_C_RoW, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_C_VISTA_RoW.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN_C, Reg_Dell_4965_AGN_C_JPN, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_C_VISTA_JPN.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN_C, Reg_Dell_4965_AGN_C_KRA, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_C_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_SP1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN_C, Reg_Dell_4965_AGN_C_SP1, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_SP1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_C_VISTA_SP1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_SP2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN_C, Reg_Dell_4965_AGN_C_SP2, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_SP2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_C_VISTA_SP2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_SP3]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN_C, Reg_Dell_4965_AGN_C_SP3, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_SP3.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_C_VISTA_SP3.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA Dell_4965_AGN
;-----------------------------------------

[Install_MPCIEX_Dell_4965_AGN_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN, Reg_Dell_4965_AGN_MOW1, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_VISTA_MOW1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN, Reg_Dell_4965_AGN_MOW2, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN, Reg_Dell_4965_AGN_RoW, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_VISTA_RoW.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN, Reg_Dell_4965_AGN_JPN, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_VISTA_JPN.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN, Reg_Dell_4965_AGN_KRA, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_VISTA_SP1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN, Reg_Dell_4965_AGN_SP1, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_VISTA_SP1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_VISTA_SP1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_VISTA_SP2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN, Reg_Dell_4965_AGN_SP2, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_VISTA_SP2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_VISTA_SP2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_VISTA_SP3]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN, Reg_Dell_4965_AGN_SP3, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_VISTA_SP3.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_VISTA_SP3.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA Dell_4965_AG
;-----------------------------------------

[Install_MPCIEX_Dell_4965_AG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AG, Reg_Dell_4965_AG_MOW1, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AG_VISTA_MOW1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AG, Reg_Dell_4965_AG_MOW2, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AG_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AG, Reg_Dell_4965_AG_RoW, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AG_VISTA_RoW.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AG, Reg_Dell_4965_AG_JPN, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AG_VISTA_JPN.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AG, Reg_Dell_4965_AG_KRA, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AG_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AG_VISTA_SP1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AG, Reg_Dell_4965_AG_SP1, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AG_VISTA_SP1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AG_VISTA_SP1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AG_VISTA_SP2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AG, Reg_Dell_4965_AG_SP2, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AG_VISTA_SP2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AG_VISTA_SP2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AG_VISTA_SP3]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AG, Reg_Dell_4965_AG_SP3, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR, Reg_NDI_ABG
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AG_VISTA_SP3.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AG_VISTA_SP3.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA Dell_3965_ABG
;-----------------------------------------

[Install_MPCIEX_Dell_3965_ABG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_3965_ABG, Reg_Dell_3965_ABG_MOW1, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_3965_ABG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Dell_3965_ABG_VISTA_MOW1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_3965_ABG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_3965_ABG, Reg_Dell_3965_ABG_MOW2, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_3965_ABG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Dell_3965_ABG_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_3965_ABG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_3965_ABG, Reg_Dell_3965_ABG_RoW, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_3965_ABG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Dell_3965_ABG_VISTA_RoW.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_3965_ABG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_3965_ABG, Reg_Dell_3965_ABG_JPN, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_3965_ABG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Dell_3965_ABG_VISTA_JPN.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_3965_ABG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_3965_ABG, Reg_Dell_3965_ABG_KRA, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_3965_ABG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Dell_3965_ABG_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA Dell_3945_ABG
;-----------------------------------------

[Install_MPCIEX_Dell_3945_ABG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_3945_ABG, Reg_Dell_3945_ABG_MOW1, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_3945_ABG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Dell_3945_ABG_VISTA_MOW1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_3945_ABG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_3945_ABG, Reg_Dell_3945_ABG_MOW2, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_3945_ABG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Dell_3945_ABG_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_3945_ABG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_3945_ABG, Reg_Dell_3945_ABG_RoW, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_3945_ABG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Dell_3945_ABG_VISTA_RoW.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_3945_ABG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_3945_ABG, Reg_Dell_3945_ABG_JPN, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_3945_ABG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Dell_3945_ABG_VISTA_JPN.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_3945_ABG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_3945_ABG, Reg_Dell_3945_ABG_KRA, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_3945_ABG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Dell_3945_ABG_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA Toshiba_3965_ABG
;-----------------------------------------

[Install_MPCIEX_Toshiba_3965_ABG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Toshiba_3965_ABG, Reg_Toshiba_3965_ABG_MOW1, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Toshiba_3965_ABG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Toshiba_3965_ABG_VISTA_MOW1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Toshiba_3965_ABG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Toshiba_3965_ABG, Reg_Toshiba_3965_ABG_MOW2, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Toshiba_3965_ABG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Toshiba_3965_ABG_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Toshiba_3965_ABG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Toshiba_3965_ABG, Reg_Toshiba_3965_ABG_RoW, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Toshiba_3965_ABG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Toshiba_3965_ABG_VISTA_RoW.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Toshiba_3965_ABG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Toshiba_3965_ABG, Reg_Toshiba_3965_ABG_JPN, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Toshiba_3965_ABG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Toshiba_3965_ABG_VISTA_JPN.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Toshiba_3965_ABG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Toshiba_3965_ABG, Reg_Toshiba_3965_ABG_KRA, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Toshiba_3965_ABG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Toshiba_3965_ABG_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA Toshiba_3945_ABG
;-----------------------------------------

[Install_MPCIEX_Toshiba_3945_ABG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Toshiba_3945_ABG, Reg_Toshiba_3945_ABG_MOW1, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Toshiba_3945_ABG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Toshiba_3945_ABG_VISTA_MOW1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Toshiba_3945_ABG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Toshiba_3945_ABG, Reg_Toshiba_3945_ABG_MOW2, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Toshiba_3945_ABG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Toshiba_3945_ABG_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Toshiba_3945_ABG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Toshiba_3945_ABG, Reg_Toshiba_3945_ABG_RoW, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Toshiba_3945_ABG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Toshiba_3945_ABG_VISTA_RoW.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Toshiba_3945_ABG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Toshiba_3945_ABG, Reg_Toshiba_3945_ABG_JPN, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Toshiba_3945_ABG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Toshiba_3945_ABG_VISTA_JPN.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA Toshiba_3945_BGX
;-----------------------------------------

[Install_MPCIEX_Toshiba_3945_BGX_VISTA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Toshiba_3945_BGX, Reg_MPCIEX_3945BG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_BG
DelReg				 = Reg_Loudon_Obsolete , Reg_WirelessMode_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Toshiba_3945_BGX_VISTA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Toshiba_3945_BGX_VISTA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA Sony_3965_ABG
;-----------------------------------------

[Install_MPCIEX_Sony_3965_ABG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Sony_3965_ABG, Reg_Sony_3965_ABG_MOW1, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Sony_3965_ABG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Sony_3965_ABG_VISTA_MOW1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Sony_3965_ABG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Sony_3965_ABG, Reg_Sony_3965_ABG_MOW2, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Sony_3965_ABG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Sony_3965_ABG_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Sony_3965_ABG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Sony_3965_ABG, Reg_Sony_3965_ABG_RoW, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Sony_3965_ABG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Sony_3965_ABG_VISTA_RoW.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Sony_3965_ABG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Sony_3965_ABG, Reg_Sony_3965_ABG_JPN, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Sony_3965_ABG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Sony_3965_ABG_VISTA_JPN.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Sony_3965_ABG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Sony_3965_ABG, Reg_Sony_3965_ABG_KRA, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Sony_3965_ABG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Sony_3965_ABG_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA Sony_3945_ABG
;-----------------------------------------

[Install_MPCIEX_Sony_3945_ABG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Sony_3945_ABG, Reg_Sony_3945_ABG_MOW1, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Sony_3945_ABG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Sony_3945_ABG_VISTA_MOW1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Sony_3945_ABG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Sony_3945_ABG, Reg_Sony_3945_ABG_MOW2, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Sony_3945_ABG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Sony_3945_ABG_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Sony_3945_ABG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Sony_3945_ABG, Reg_Sony_3945_ABG_RoW, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Sony_3945_ABG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Sony_3945_ABG_VISTA_RoW.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Sony_3945_ABG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Sony_3945_ABG, Reg_Sony_3945_ABG_JPN, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Sony_3945_ABG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Sony_3945_ABG_VISTA_JPN.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Sony_3945_ABG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Sony_3945_ABG, Reg_Sony_3945_ABG_KRA, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Sony_3945_ABG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Sony_3945_ABG_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA HP_3965_ABG
;-----------------------------------------

[Install_MPCIEX_HP_3965_ABG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_HP_3965_ABG, Reg_HP_3965_ABG_MOW1, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_HP_3965_ABG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_HP_3965_ABG_VISTA_MOW1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_HP_3965_ABG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_HP_3965_ABG, Reg_HP_3965_ABG_MOW2, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_HP_3965_ABG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_HP_3965_ABG_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_HP_3965_ABG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_HP_3965_ABG, Reg_HP_3965_ABG_RoW, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_HP_3965_ABG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_HP_3965_ABG_VISTA_RoW.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_HP_3965_ABG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_HP_3965_ABG, Reg_HP_3965_ABG_JPN, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_HP_3965_ABG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_HP_3965_ABG_VISTA_JPN.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_HP_3965_ABG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_HP_3965_ABG, Reg_HP_3965_ABG_KRA, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_HP_3965_ABG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_HP_3965_ABG_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA HP_3945_ABG
;-----------------------------------------

[Install_MPCIEX_HP_3945_ABG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_HP_3945_ABG, Reg_HP_3945_ABG_MOW1, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_HP_3945_ABG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_HP_3945_ABG_VISTA_MOW1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_HP_3945_ABG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_HP_3945_ABG, Reg_HP_3945_ABG_MOW2, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_HP_3945_ABG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_HP_3945_ABG_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_HP_3945_ABG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_HP_3945_ABG, Reg_HP_3945_ABG_RoW, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_HP_3945_ABG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_HP_3945_ABG_VISTA_RoW.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_HP_3945_ABG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_HP_3945_ABG, Reg_HP_3945_ABG_JPN, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_HP_3945_ABG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_HP_3945_ABG_VISTA_JPN.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_HP_3945_ABG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_HP_3945_ABG, Reg_HP_3945_ABG_KRA, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_HP_3945_ABG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_HP_3945_ABG_VISTA_KRA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA IBM_3945_ABG
;-----------------------------------------

[Install_MPCIEX_IBM_3945_ABG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_IBM_3945_ABG, Reg_IBM_3945_ABG_MOW1, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_IBM_3945_ABG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_IBM_3945_ABG_VISTA_MOW1.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_IBM_3945_ABG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_IBM_3945_ABG, Reg_IBM_3945_ABG_MOW2, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_IBM_3945_ABG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_IBM_3945_ABG_VISTA_MOW2.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_IBM_3945_ABG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_IBM_3945_ABG, Reg_IBM_3945_ABG_RoW, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_IBM_3945_ABG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_IBM_3945_ABG_VISTA_RoW.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_IBM_3945_ABG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_IBM_3945_ABG, Reg_IBM_3945_ABG_JPN, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_ABG
DelReg				 = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_IBM_3945_ABG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_IBM_3945_ABG_VISTA_JPN.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  VISTA IBM_3945_BG
;-----------------------------------------

[Install_MPCIEX_IBM_3945_BG_VISTA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_IBM_3945_BG, Reg_MPCIEX_3945BG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM, Reg_NDI_BG
DelReg				 = Reg_Loudon_Obsolete , Reg_WirelessMode_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_IBM_3945_BG_VISTA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_IBM_3945_BG_VISTA.Services]
AddService      = netw5v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Reg_Loudon_Obsolete]
HKR,,RfKillSKU
HKR,,FixedSupportedRates
HKR,,PowerIndex

[Reg_WirelessMode_Obsolete]
HKR, Ndi\Params\WirelessMode,               ParamDesc,  0, %WIRELESS_MODE_STR%
HKR, Ndi\Params\WirelessMode,               Type,       0, "enum",
HKR, Ndi\params\WirelessMode,      			    Default,   	0, "34" ;abg
HKR, Ndi\Params\WirelessMode,               Optional,   0, "0"
HKR, Ndi\params\WirelessMode\enum, 			    "17",       0, "1. 802.11a"
HKR, Ndi\params\WirelessMode\enum, 			    "0",        0, "2. 802.11b"
HKR, Ndi\params\WirelessMode\enum, 			    "16",       0, "3. 802.11g"
HKR, Ndi\params\WirelessMode\enum, 			    "32",       0, "4. 802.11b/g"
HKR, Ndi\params\WirelessMode\enum, 			    "18",       0, "5. 802.11a/g"
HKR, Ndi\params\WirelessMode\enum, 			    "34",       0, "6. 802.11a/b/g"

[Reg_Common]
HKR,,ApsdTriggerQueues,0x10001,0x0
HKR,,BTEnableFlags,0x10001,0x3
HKR,,BcsSupport,0x10003,0x0
HKR,,CardType,0x00010001,2
HKR,,CCXv4FeatureSet,0x10001,0x0
HKR,,CcxSdkActive,0x10003,0x1
HKR,,CcxVersion,0x10003,0x4
HKR,,ConfigurationName,0,"PR0W1RELE55"
HKR,,ConnectionPriority,0,"2"
HKR,,DesiredAuthenticationMode,0x10003,0x0
HKR,,DesiredCipher,0x10003,0x1
HKR,,DesiredDefaultKeyId,0x10003,0x1
HKR,,DesiredPortType,0x10003,0x1
HKR,,DesiredPSKey1,0x2,""
HKR,,DesiredPSKey2,0x2,""
HKR,,DesiredPSKey3,0x2,""
HKR,,DesiredPSKey4,0x2,""
HKR,,DlsEnabled,0x10003,0x0
HKR,,DlsResponseTimeout,0x10003,0x0
HKR,,DlsTimeoutCounter,0x10003,0x0
HKR,,ExternalImage,0x10001,0x0
HKR,,FixedLongPreamble,0x10001,0x0
HKR,,FixedSupportedRates,0x10001,0xFFF
HKR,,ModulationType,2,"2"
HKR,,NdisEnvironment,0x10001,0
HKR,,NetType,0,"WLAN"
HKR,,PibssShortSlot,0x10001,0x1
HKR,,Provider,0,%PROVIDER_NAME%
HKR,,RadioEnable,0x10003,0x1
HKR,,RecommendedBeaconInterval,0x10001,0x64
HKR,,SlsDecisionPeriod,0x10003,0x0
HKR,,SlsEnabled,0x10003,0x0
HKR,,SlsEnabledOnRecipient,0x10003,0x0
HKR,,SlsForcedToDirect,0x10003,0x0
HKR,,BTOnThreshold,0x10001,0x4
HKR,,FastResumeReconnect,0x10001,0x1
HKR,,ManagementPacketFilterAdjustment,0x10001,0x1

; following registry keys define the Advanced Property Page (NDI) values. they are common, and the defult values vary between the different reg sections.
[Reg_NDI_BG]
HKR, Ndi\Params\WirelessMode,				ParamDesc,  0, %WIRELESS_MODE_STR%
HKR, Ndi\Params\WirelessMode, 			Type, 		  0, "enum",
HKR, Ndi\params\WirelessMode, 			Default, 		0, "32" ;bg
HKR, Ndi\Params\WirelessMode, 			Optional, 	0, "0"
HKR, Ndi\params\WirelessMode\enum, 	"0",  			0, "1. 802.11b"
HKR, Ndi\params\WirelessMode\enum, 	"16", 			0, "2. 802.11g"
HKR, Ndi\params\WirelessMode\enum, 	"32", 			0, "3. 802.11b/g"

[Reg_NDI_ABG]
HKR, Ndi\Params\WirelessMode,               ParamDesc,  0, %WIRELESS_MODE_STR%
HKR, Ndi\Params\WirelessMode,               Type,       0, "enum",
HKR, Ndi\params\WirelessMode,      			    Default,   	0, "34" ;abg
HKR, Ndi\Params\WirelessMode,               Optional,   0, "0"
HKR, Ndi\params\WirelessMode\enum, 			    "17",       0, "1. 802.11a"
HKR, Ndi\params\WirelessMode\enum, 			    "0",        0, "2. 802.11b"
HKR, Ndi\params\WirelessMode\enum, 			    "16",       0, "3. 802.11g"
HKR, Ndi\params\WirelessMode\enum, 			    "32",       0, "4. 802.11b/g"
HKR, Ndi\params\WirelessMode\enum, 			    "18",       0, "5. 802.11a/g"
HKR, Ndi\params\WirelessMode\enum, 			    "34",       0, "6. 802.11a/b/g"

[Reg_NDI]
HKR, Ndi\params\RecommendedChannel24,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL24_STR%
HKR, Ndi\params\RecommendedChannel24,      	Type,       0x00000002, "int"
HKR, Ndi\params\RecommendedChannel24,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel24,      	Min,	    0x00000002, "1"
HKR, Ndi\params\RecommendedChannel24,      	Step,	   	0x00000002, "1"

HKR, Ndi\params\IbssTxPower,      			    ParamDesc, 	0x00000000, %IBSS_TX_POWER_STR%
HKR, Ndi\params\IbssTxPower,      			    Type,      	0x00000002, "enum"
HKR, Ndi\params\IbssTxPower,      			    Default,   	0x00000002, "100"
HKR, Ndi\params\IbssTxPower,      			    Optional,  	0x00000002, "0"
HKR, Ndi\params\IbssTxPower\enum, 			    "0",       	0x00000000, "1. "%LOWEST_STR%
HKR, Ndi\params\IbssTxPower\enum, 			    "25",       0x00000000, "2. "%MEDIUM_LOW_STR%
HKR, Ndi\params\IbssTxPower\enum, 			    "50",       0x00000000, "3. "%MEDIUM_STR%
HKR, Ndi\params\IbssTxPower\enum, 			    "75",       0x00000000, "4. "%MEDIUM_HIGH_STR%
HKR, Ndi\params\IbssTxPower\enum, 			    "100",      0x00000000, "5. "%HIGHEST_STR%

HKR, Ndi\params\RoamAggressiveness,     	  ParamDesc, 	0x00000000, %ROAMING_AGGRESSIVENESS_STR%
HKR, Ndi\params\RoamAggressiveness,     	  Type,      	0x00000002, "enum"
HKR, Ndi\params\RoamAggressiveness,     	  Default,   	0x00000002, "2"
HKR, Ndi\params\RoamAggressiveness,     	  Optional,  	0x00000002, "0"
HKR, Ndi\params\RoamAggressiveness\enum,	  "0",       	0x00000000, "1. "%LOWEST_STR%
HKR, Ndi\params\RoamAggressiveness\enum,	  "1",       	0x00000000, "2. "%MEDIUM_LOW_STR%
HKR, Ndi\params\RoamAggressiveness\enum,	  "2",     	0x00000000, "3. "%MEDIUM_STR%
HKR, Ndi\params\RoamAggressiveness\enum,	  "3", 	    	0x00000000, "4. "%MEDIUM_HIGH_STR%
HKR, Ndi\params\RoamAggressiveness\enum,    	  "4",          0x00000000, "5. "%HIGHEST_STR%

HKR, Ndi\params\RecommendedAtimWindow, 				ParamDesc, 	0x00000000, %ADHOC_POWER_MANAGEMENT_STR%
HKR, Ndi\params\RecommendedAtimWindow, 				Type,  			0x00000002, "enum"
HKR, Ndi\params\RecommendedAtimWindow, 				Default, 		0x00000002, "0"
HKR, Ndi\params\RecommendedAtimWindow, 				Optional,  	0x00000002, "0"
HKR, Ndi\params\RecommendedAtimWindow\enum,  	"0", 				0x00000000, %DISABLED_STR%
HKR, Ndi\params\RecommendedAtimWindow\enum,  	"3", 				0x00000000, %MAXIMUM_POWER_SAVING_STR%
HKR, Ndi\params\RecommendedAtimWindow\enum,  	"10", 				0x00000000, %NOISY_ENVIRONMENT_STR%

HKR, Ndi\params\IbssQosEnabled,			  ParamDesc, 	0x00000000, %ADHOC_QOS_MODE_STR%
HKR, Ndi\params\IbssQosEnabled,			  Type,  			0x00000002, "enum"
HKR, Ndi\params\IbssQosEnabled,			  Default, 		0x00000002, "0"
HKR, Ndi\params\IbssQosEnabled,			  Optional,  	0x00000002, "0"
HKR, Ndi\params\IbssQosEnabled\enum,  "0",  			0x00000000, %WMM_DISABLED_STR%
HKR, Ndi\params\IbssQosEnabled\enum,  "1",  			0x00000000, %WMM_ENABLED_STR%

HKR, Ndi\params\CtsToItself,		  ParamDesc, 			0x00000000, %MIXED_MODE_PROTECTION_STR%
HKR, Ndi\params\CtsToItself,		  Type,  					0x00000002, "enum"
HKR, Ndi\params\CtsToItself,		  Default, 				0x00000002, "1"
HKR, Ndi\params\CtsToItself,		  Optional,  			0x00000002, "0"
HKR, Ndi\params\CtsToItself\enum, "0",  					0x00000000, %RTS_CTS_ENABLED_STR%
HKR, Ndi\params\CtsToItself\enum, "1",  					0x00000000, %CTS_TO_SELF_ENABLED_STR%

HKR, Ndi\params\PropPacketBurstEnabled,		ParamDesc, 	0x00000000, %THROUGHPUT_ENHANCEMENT_STR%
HKR, Ndi\params\PropPacketBurstEnabled,		Type,  			0x00000002, "enum"
HKR, Ndi\params\PropPacketBurstEnabled,		Default, 		0x00000002, "0"
HKR, Ndi\params\PropPacketBurstEnabled,		Optional,  	0x00000002, "0"
HKR, Ndi\params\PropPacketBurstEnabled\enum, "0", 		0x00000000, %DISABLED_STR%
HKR, Ndi\params\PropPacketBurstEnabled\enum, "1", 		0x00000000, %ENABLED_STR%

[Reg_NDI_ECP]
HKR,,CLSGUID,0,"{FB326D29-7731-4ece-83C0-D47F8D1BF0FF}"

[Reg_NDI_SHP]
HKR,,CLSGUID,0,"{09F89A23-8DEB-4ec1-A674-9C8A1C1E00F6}"

[Reg_NDI_KDR]
HKR,,CLSGUID,0,"{4E82578B-20D2-4709-B663-CC9C3EA9C74A}"

[Reg_NDI_ALM]
HKR,,CLSGUID,0,"{AA7636EC-77CB-4e5a-9C1C-43950899EAAA}"


[Reg_NDIS_VISTA]
HKR, Ndi\Interfaces,  UpperRange,   0, "ndis5,wifipro"
HKR, Ndi\Interfaces,  LowerRange,   0, "ethernet,wlan"
HKR, Ndi,             Service,      0, "netw5v32"

; Registry settings by HW
; =========================

[Reg_ECP]
HKR,,FeatureSet,0x10001,0xA1920001
HKR,,ScanWhenAssociated,0x10001,0x1
HKR,,WoWLanEnable,0x10001,0x1

[Reg_SHP]
HKR,,FeatureSet,0x10001,0xA1920001
HKR,,CalibrationActive,0x10001,0x22BB
HKR,,ActivateDisconnectedAntennaOnly,0x10001,0x0
HKR,,ScanWhenAssociated,0x10001,0x1
HKR,,WoWLanEnable,0x10001,0x1

[Reg_KDR]
HKR,,FeatureSet,0x10001,0xA1928001
HKR,,ScanMode,0x10001,0x18
HKR,,WatchDogEnabled,0x10001,0x1
HKR,,CalibrationActive,0x10001,0x000032f7
HKR,,rlcChainSettings,0x10001,0x0
HKR,,ScanChainSelection,0x10001,0x37
HKR,,WoWLanEnable,0x10001,0x1
HKR,,DefaultTtl,0x10001,0xFFFFFFFF


[Reg_ALM]
HKR,,FeatureSet,0x10001,0xA192A001
HKR,,CalibrationActive,0x10001,0x00000037
HKR,,IEEE11nMode,0x00000002,0x0
HKR,,WoWLanEnable,0x10001,0x1
HKR,,DefaultTtl,0x10001,0xFFFFFFFF



; Registry settings by OS
; =========================

[Reg_Common_VISTA]
HKR,,TGeEnableBits,0x10001,0x27
HKR,,MinidumpCallbackSupported,0x10001,0x0


; Registry settings by SKU
; =========================

[Reg_GEN_5300_AGN_3x3_MC]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,LedMode,0x10001,0x1
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_GEN_5300_AGN_3x3_MC_MOW2]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"

[Reg_GEN_5300_AGN_3x3_MC_KRA]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	    0x00000002, "13"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_GEN_5300_AGN_3x3_HMC]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,LedMode,0x10001,0x1
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_GEN_5300_AGN_3x3_HMC_MOW2]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"

[Reg_GEN_5300_AGN_3x3_HMC_KRA]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	    0x00000002, "13"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

;GEN_5100_AGN_1x2 skus
[Reg_GEN_5100_AGN_1x2_MC]
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,LedMode,0x10001,0x1
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"
HKR,,tlcValidAntenna,0x10001,0x2

[Reg_GEN_5100_AGN_1x2_MC_MOW2]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5100AGN_1x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_5100AGN_1x2%
HKR,,BandType,0x10003,0x2
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"

[Reg_GEN_5100_AGN_1x2_MC_KRA]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5100AGN_1x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_5100AGN_1x2%
HKR,,BandType,0x10003,0x2
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	    0x00000002, "13"

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_GEN_5100_AGN_1x2_MC_BG]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5100AGN_1x2_BG%
HKR,,DriverDesc,0,%NIC_DriverDesc_5100AGN_1x2_BG%
HKR,,BandType,0x10003,0x0
HKR,,JPNLegacyChannels,0x10003,0x0
HKR,,IEEE11nMode,0x10001,0x00000000
HKR,,ChannelWidth52,0x10001,0x0
HKR,,ChannelWidth24,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"

[Reg_GEN_5100_AGN_1x2_MC_ABG]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5100AGN_1x2_ABG%
HKR,,DriverDesc,0,%NIC_DriverDesc_5100AGN_1x2_ABG%
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,LedMode,0x10001,0x1
HKR,,IEEE11nMode,0x10001,0x00000000
HKR,,ChannelWidth52,0x10001,0x0
HKR,,ChannelWidth24,0x10001,0x0 
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

HKR,,BandType,0x10003,0x2
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	    0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_GEN_5100_AGN_1x2_HMC]
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,LedMode,0x10001,0x1
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"
HKR,,tlcValidAntenna,0x10001,0x2

[Reg_GEN_5100_AGN_1x2_HMC_MOW2]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5100AGN_1x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_5100AGN_1x2%
HKR,,BandType,0x10003,0x2
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_GEN_5100_AGN_1x2_HMC_KRA]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5100AGN_1x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_5100AGN_1x2%
HKR,,BandType,0x10003,0x2
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	    0x00000002, "13"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_GEN_5100_AGN_1x2_HMC_BG]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5100AGN_1x2_BG%
HKR,,DriverDesc,0,%NIC_DriverDesc_5100AGN_1x2_BG%
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,IEEE11nMode,0x10001,0x00000000
HKR,,LedMode,0x10001,0x1
HKR,,BandType,0x10003,0x0
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

;GEN_5100_ABG_1x2 skus
[Reg_GEN_5100_AGN_1x2_HMC_ABG]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5100AGN_1x2_ABG%
HKR,,DriverDesc,0,%NIC_DriverDesc_5100AGN_1x2_ABG%
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,LedMode,0x10001,0x1
HKR,,IEEE11nMode,0x10001,0x00000000
HKR,,ChannelWidth52,0x10001,0x0
HKR,,ChannelWidth24,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

HKR,,BandType,0x10003,0x2
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	    0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

;Lenovo_5300_AGN_3x3 skus
[Reg_Lenovo_5300_AGN_3x3_MC]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"WXYZ"
HKR,,LedMode,0x10001,0x3
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Lenovo_5300_AGN_3x3_MC_MOW2]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"

[Reg_Lenovo_5300_AGN_3x3_MC_KRA]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	    0x00000002, "13"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_5300_AGN_3x3_HMC]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"WXYZ"
HKR,,LedMode,0x10001,0x3
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Lenovo_5300_AGN_3x3_HMC_MOW2]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"

[Reg_Lenovo_5300_AGN_3x3_HMC_KRA]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	    0x00000002, "13"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

;Lenovo_5100_AGN_1x2 skus
[Reg_Lenovo_5100_AGN_1x2_MC]
HKR,,DesiredSsid,0x00000002,"WXYZ"
HKR,,LedMode,0x10001,0x3
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"
HKR,,tlcValidAntenna,0x10001,0x2

[Reg_Lenovo_5100_AGN_1x2_MC_MOW2]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5100AGN_1x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_5100AGN_1x2%
HKR,,BandType,0x10003,0x2
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"

[Reg_Lenovo_5100_AGN_1x2_MC_KRA]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5100AGN_1x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_5100AGN_1x2%
HKR,,BandType,0x10003,0x2
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	    0x00000002, "13"

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_5100_AGN_1x2_MC_BG]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5100AGN_1x2_BG%
HKR,,DriverDesc,0,%NIC_DriverDesc_5100AGN_1x2_BG%
HKR,,BandType,0x10003,0x0
HKR,,IEEE11nMode,0x10001,0x00000000
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

HKR,,ChannelWidth52,0x10001,0x0
HKR,,ChannelWidth24,0x10001,0x0
HKR,,FatChannelIntolerant, 0x10001, 0x0

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"

[Reg_Lenovo_5100_AGN_1x2_MC_ABG]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5100AGN_1x2_ABG%
HKR,,DriverDesc,0,%NIC_DriverDesc_5100AGN_1x2_ABG%
HKR,,DesiredSsid,0x00000002,"WXYZ"
HKR,,LedMode,0x10001,0x3
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"
HKR,,IEEE11nMode,0x10001,0x00000000
HKR,,ChannelWidth52,0x10001,0x0
HKR,,ChannelWidth24,0x10001,0x0
HKR,,FatChannelIntolerant, 0x10001, 0x0


HKR,,BandType,0x10003,0x2
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	    0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_5100_AGN_1x2_HMC]
HKR,,DesiredSsid,0x00000002,"WXYZ"
HKR,,LedMode,0x10001,0x3
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"
HKR,,tlcValidAntenna,0x10001,0x2

[Reg_Lenovo_5100_AGN_1x2_HMC_MOW2]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5100AGN_1x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_5100AGN_1x2%
HKR,,BandType,0x10003,0x2
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"

[Reg_Lenovo_5100_AGN_1x2_HMC_KRA]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5100AGN_1x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_5100AGN_1x2%
HKR,,BandType,0x10003,0x2
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	    0x00000002, "13"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Lenovo_5100_AGN_1x2_HMC_BG]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5100AGN_1x2_BG%
HKR,,DriverDesc,0,%NIC_DriverDesc_5100AGN_1x2_BG%
HKR,,IEEE11nMode,0x10001,0x00000000
HKR,,BandType,0x10003,0x0
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"
HKR,,ChannelWidth52,0x10001,0x0
HKR,,ChannelWidth24,0x10001,0x0
HKR,,FatChannelIntolerant, 0x10001, 0x0

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"

;Lenovo_5100_ABG_1x2 skus
[Reg_Lenovo_5100_AGN_1x2_HMC_ABG]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5100AGN_1x2_ABG%
HKR,,DriverDesc,0,%NIC_DriverDesc_5100AGN_1x2_ABG%
HKR,,DesiredSsid,0x00000002,"WXYZ"
HKR,,LedMode,0x10001,0x3
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"
HKR,,IEEE11nMode,0x10001,0x00000000
HKR,,ChannelWidth52,0x10001,0x0
HKR,,ChannelWidth24,0x10001,0x0

HKR,,BandType,0x10003,0x2
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	    0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


;Dell_5300_AGN_3x3 skus
[Reg_Dell_5300_AGN_3x3_MC]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"101"
HKR,,LedMode,0x10001,0x2
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "1"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Dell_5300_AGN_3x3_MC_MOW2]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"


[Reg_Dell_5300_AGN_3x3_MC_KRA]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	    0x00000002, "13"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"




;Dell_5300_AGN_3x3 skus
[Reg_Dell_5300_AGN_3x3_HMC]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"101"
HKR,,LedMode,0x10001,0x2
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "1"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Dell_5300_AGN_3x3_HMC_MOW2]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"


[Reg_Dell_5300_AGN_3x3_HMC_KRA]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	    0x00000002, "13"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

;Dell_5100_AGN_1x2 skus
[Reg_Dell_5100_AGN_1x2_MC]
HKR,,DesiredSsid,0x00000002,"101"
HKR,,LedMode,0x10001,0x2
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "1"
HKR,,tlcValidAntenna,0x10001,0x2

[Reg_Dell_5100_AGN_1x2_MC_MOW2]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5100AGN_1x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_5100AGN_1x2%
HKR,,BandType,0x10003,0x2
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"

[Reg_Dell_5100_AGN_1x2_MC_KRA]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5100AGN_1x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_5100AGN_1x2%
HKR,,BandType,0x10003,0x2
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	    0x00000002, "13"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_5100_AGN_1x2_MC_BG]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5100AGN_1x2_BG%
HKR,,DriverDesc,0,%NIC_DriverDesc_5100AGN_1x2_BG%
HKR,,IEEE11nMode,0x10001,0x00000000
HKR,,BandType,0x10003,0x0
HKR,,JPNLegacyChannels,0x10003,0x0
HKR,,ChannelWidth52,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"
HKR,,ChannelWidth52,0x10001,0x0
HKR,,ChannelWidth24,0x10001,0x0
HKR,,FatChannelIntolerant, 0x10001, 0x0

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"

[Reg_Dell_5100_AGN_1x2_MC_ABG]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5100AGN_1x2_ABG%
HKR,,DriverDesc,0,%NIC_DriverDesc_5100AGN_1x2_ABG%
HKR,,DesiredSsid,0x00000002,"101"
HKR,,LedMode,0x10001,0x2
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "1"
HKR,,IEEE11nMode,0x10001,0x00000000
HKR,,ChannelWidth52,0x10001,0x0
HKR,,ChannelWidth24,0x10001,0x0

HKR,,BandType,0x10003,0x2
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	    0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"



[Reg_Dell_5100_AGN_1x2_HMC]
HKR,,DesiredSsid,0x00000002,"101"
HKR,,LedMode,0x10001,0x2
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "1"
HKR,,tlcValidAntenna,0x10001,0x2

[Reg_Dell_5100_AGN_1x2_HMC_MOW2]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5100AGN_1x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_5100AGN_1x2%
HKR,,BandType,0x10003,0x2
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"

[Reg_Dell_5100_AGN_1x2_HMC_KRA]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5100AGN_1x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_5100AGN_1x2%
HKR,,BandType,0x10003,0x2
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	    0x00000002, "13"

HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\ChannelWidth24,				ParamDesc, 	0, %CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth24,				Default,   	0, "0"
HKR, Ndi\params\ChannelWidth24,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth24\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_5100_AGN_1x2_HMC_BG]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5100AGN_1x2_BG%
HKR,,DriverDesc,0,%NIC_DriverDesc_5100AGN_1x2_BG%
HKR,,BandType,0x10003,0x0
HKR,,IEEE11nMode,0x10001,0x00000000
HKR,,JPNLegacyChannels,0x10003,0x0
HKR,,ChannelWidth52,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"
HKR,,ChannelWidth24,0x10001,0x0
HKR,,FatChannelIntolerant, 0x10001, 0x0

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"


;Dell_5100_ABG_1x2 skus
[Reg_Dell_5100_AGN_1x2_HMC_ABG]
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5100AGN_1x2_ABG%
HKR,,DriverDesc,0,%NIC_DriverDesc_5100AGN_1x2_ABG%
HKR,,DesiredSsid,0x00000002,"101"
HKR,,LedMode,0x10001,0x2
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "1"
HKR,,IEEE11nMode,0x10001,0x00000000
HKR,,ChannelWidth52,0x10001,0x0
HKR,,ChannelWidth24,0x10001,0x0

HKR,,BandType,0x10003,0x2
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	    0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"



[Reg_GEN_4965_AGN]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,LedMode,0x10001,0x1
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_GEN_4965_AGN_MOW1]
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"


[Reg_GEN_4965_AGN_MOW2]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	    0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_GEN_4965_AGN_RoW]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_GEN_4965_AGN_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_GEN_4965_AGN_KRA]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	    0x00000002, "13"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_GEN_4965_AGN_C]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,LedMode,0x10001,0x1
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_GEN_4965_AGN_C_MOW1]
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"


[Reg_GEN_4965_AGN_C_MOW2]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	    0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_GEN_4965_AGN_C_RoW]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_GEN_4965_AGN_C_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_GEN_4965_AGN_C_KRA]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	    0x00000002, "13"


[Reg_GEN_4965_AG]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,LedMode,0x10001,0x1
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

[Reg_GEN_4965_AG_MOW1]
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

[Reg_GEN_4965_AG_MOW2]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	    0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"



[Reg_GEN_4965_AG_RoW]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"



[Reg_GEN_4965_AG_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_GEN_4965_AG_KRA]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_GEN_3965_ABG]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,LedMode,0x10001,0x1
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

[Reg_GEN_3965_ABG_MOW1]
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

[Reg_GEN_3965_ABG_MOW2]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	     	0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"



[Reg_GEN_3965_ABG_RoW]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"



[Reg_GEN_3965_ABG_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_GEN_3965_ABG_KRA]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_GEN_3945_ABG]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,LedMode,0x10001,0x1
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

[Reg_GEN_3945_ABG_MOW1]
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

[Reg_GEN_3945_ABG_MOW2]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_GEN_3945_ABG_RoW]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	    	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_GEN_3945_ABG_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_GEN_3945_ABG_KRA]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_GEN_3945_BG]
HKR,,BandType,0x10003,0x0
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,LedMode,0x10001,0x1
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_GEN_3945_BGX]
HKR,,BandType,0x10003,0x0
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,LedMode,0x10001,0x3
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_Lenovo_4965_AGN]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"WXYZ"
HKR,,LedMode,0x10001,0x3
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Lenovo_4965_AGN_MOW1]
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"


[Reg_Lenovo_4965_AGN_MOW2]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_Lenovo_4965_AGN_RoW]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	     	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_Lenovo_4965_AGN_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_4965_AGN_KRA]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_4965_AGN_C]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"WXYZ"
HKR,,LedMode,0x10001,0x3
HKR, Ndi\params\RecommendedChannel24,  	Default,  0x00000002, "11"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,  	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default, 	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",  0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",  0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Lenovo_4965_AGN_C_MOW1]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"


[Reg_Lenovo_4965_AGN_C_MOW2]
HKR, Ndi\params\RecommendedChannel52,  	Default,  0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,  	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,  	Type, 0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,  	Optional, 0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	  0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	  0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	 	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	 	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	 	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_4965_AGN_C_RoW]
HKR, Ndi\params\RecommendedChannel52,  	Default,  0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52,  	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,  	Type, 0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,  	Optional, 0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	 	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	  0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	  0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	 	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	 	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_4965_AGN_C_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,  	Default,  0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,  	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,  	Type, 0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,  	Optional, 0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	 	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	  0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	  0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	 	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	 	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "13"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_4965_AGN_C_KRA]
HKR, Ndi\params\RecommendedChannel52,  	Default,  0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,  	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,  	Type, 0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,  	Optional, 0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	 	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	  0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	  0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	 	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	 	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	  0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	  0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	 	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	 	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24, Max,	  0x00000002, "13"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_4965_AG]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"WXYZ"
HKR,,LedMode,0x10001,0x3
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

[Reg_Lenovo_4965_AG_MOW1]
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_Lenovo_4965_AG_MOW2]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_4965_AG_RoW]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	    	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_4965_AG_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_Lenovo_4965_AG_KRA]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_3965_ABG]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"WXYZ"
HKR,,LedMode,0x10001,0x3
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

[Reg_Lenovo_3965_ABG_MOW1]
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

[Reg_Lenovo_3965_ABG_MOW2]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_3965_ABG_RoW]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	     	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_Lenovo_3965_ABG_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_3965_ABG_KRA]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_4965_AGN]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"101"
HKR,,LedMode,0x10001,0x2
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "1"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Dell_4965_AGN_MOW1]
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"


[Reg_Dell_4965_AGN_MOW2]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_4965_AGN_RoW]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_4965_AGN_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_4965_AGN_KRA]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_4965_AGN_C]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"101"
HKR,,LedMode,0x10001,0x2
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "1"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth52,				ParamDesc, 	0, %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth52,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth52,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth52\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Dell_4965_AGN_C_MOW1]
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"


[Reg_Dell_4965_AGN_C_MOW2]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_4965_AGN_C_RoW]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_4965_AGN_C_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_4965_AGN_C_KRA]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"

HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_4965_AG]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"101"
HKR,,LedMode,0x10001,0x2
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "1"

[Reg_Dell_4965_AG_MOW1]
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_Dell_4965_AG_MOW2]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_4965_AG_RoW]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_Dell_4965_AG_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_4965_AG_KRA]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_3965_ABG]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"101"
HKR,,LedMode,0x10001,0x2
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "1"

[Reg_Dell_3965_ABG_MOW1]
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_Dell_3965_ABG_MOW2]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_3965_ABG_RoW]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_Dell_3965_ABG_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_3965_ABG_KRA]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_3945_ABG]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"101"
HKR,,LedMode,0x10001,0x2
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "1"

[Reg_Dell_3945_ABG_MOW1]
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_Dell_3945_ABG_MOW2]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_3945_ABG_RoW]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_Dell_3945_ABG_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_3945_ABG_KRA]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Toshiba_3965_ABG]
HKR,,BandType,0x10003,0x2
HKR,,LedMode,0x10001,0x1
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "10"

[Reg_Toshiba_3965_ABG_MOW1]
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

[Reg_Toshiba_3965_ABG_MOW2]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Toshiba_3965_ABG_RoW]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_Toshiba_3965_ABG_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Toshiba_3965_ABG_KRA]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Toshiba_3945_ABG]
HKR,,BandType,0x10003,0x2
HKR,,LedMode,0x10001,0x1
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "10"

[Reg_Toshiba_3945_ABG_MOW1]
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_Toshiba_3945_ABG_MOW2]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Toshiba_3945_ABG_RoW]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_Toshiba_3945_ABG_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Toshiba_3945_BGX]
HKR,,BandType,0x10003,0x0
HKR,,LedMode,0x10001,0x1
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "10"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_Sony_3965_ABG]
HKR,,BandType,0x10003,0x2
HKR,,LedMode,0x10001,0x2
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

[Reg_Sony_3965_ABG_MOW1]
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

[Reg_Sony_3965_ABG_MOW2]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Sony_3965_ABG_RoW]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	    	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_Sony_3965_ABG_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Sony_3965_ABG_KRA]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Sony_3945_ABG]
HKR,,BandType,0x10003,0x2
HKR,,LedMode,0x10001,0x2
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

[Reg_Sony_3945_ABG_MOW1]
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_Sony_3945_ABG_MOW2]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Sony_3945_ABG_RoW]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_Sony_3945_ABG_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Sony_3945_ABG_KRA]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_HP_3965_ABG]
HKR,,LedMode,0x10001,0x2
HKR,,BandType,0x10003,0x2
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

[Reg_HP_3965_ABG_MOW1]
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_HP_3965_ABG_MOW2]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_HP_3965_ABG_RoW]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_HP_3965_ABG_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 	0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_HP_3965_ABG_KRA]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_HP_3945_ABG]
HKR,,BandType,0x10003,0x2
HKR,,LedMode,0x10001,0x2
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

[Reg_HP_3945_ABG_MOW1]
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_HP_3945_ABG_MOW2]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11" 
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_HP_3945_ABG_RoW]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_HP_3945_ABG_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_HP_3945_ABG_KRA]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_IBM_3945_ABG]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"WXYZ"
HKR,,LedMode,0x10001,0x3
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

[Reg_IBM_3945_ABG_MOW1]
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_IBM_3945_ABG_MOW2]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_IBM_3945_ABG_RoW]
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_IBM_3945_ABG_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_IBM_3945_BG]
HKR,,BandType,0x10003,0x0
HKR,,DesiredSsid,0x00000002,"WXYZ"
HKR,,LedMode,0x10001,0x3
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_MPCIEX_3965ABG]
HKR,,Diversity11a,0x10003,0x3
HKR,,Diversity11b,0x10003,0x3
HKR,,Diversity11g,0x10003,0x3
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_3965ABG%
HKR,,DriverDesc,0,%NIC_DriverDesc_3965ABG%

[Reg_MPCIEX_3945ABG]
HKR,,Diversity11a,0x10003,0x0
HKR,,Diversity11b,0x10003,0x0
HKR,,Diversity11g,0x10003,0x0
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_3945ABG%
HKR,,DriverDesc,0,%NIC_DriverDesc_3945ABG%

[Reg_MPCIEX_3945BG]
HKR,,Diversity11a,0x10003,0x0
HKR,,Diversity11b,0x10003,0x0
HKR,,Diversity11g,0x10003,0x0
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_3945BG%
HKR,,DriverDesc,0,%NIC_DriverDesc_3945BG%

[Reg_MPCIEX_4965AGN] 
HKR,,Diversity11a,0x10003,0x0
HKR,,Diversity11b,0x10003,0x0
HKR,,Diversity11g,0x10003,0x0 
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_4965AGN%
HKR,,DriverDesc,0,%NIC_DriverDesc_4965AGN%

[Reg_MPCIEX_4965AG] 
HKR,,Diversity11a,0x10003,0x0
HKR,,Diversity11b,0x10003,0x0
HKR,,Diversity11g,0x10003,0x0 
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_4965AG%
HKR,,DriverDesc,0,%NIC_DriverDesc_4965AG%

[Reg_MPCIEX_5300AGN_3x3_MC]  
HKR,,Diversity11a,0x10003,0x0
HKR,,Diversity11b,0x10003,0x0
HKR,,Diversity11g,0x10003,0x0
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5300AGN_3x3%
HKR,,DriverDesc,0,%NIC_DriverDesc_5300AGN_3x3%
HKR,,rlcChainSettings,0x10001,0xE

[Reg_MPCIEX_5300AGN_3x3_HMC]  
HKR,,Diversity11a,0x10003,0x0
HKR,,Diversity11b,0x10003,0x0
HKR,,Diversity11g,0x10003,0x0
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_5300AGN_3x3%
HKR,,DriverDesc,0,%NIC_DriverDesc_5300AGN_3x3%
HKR,,rlcChainSettings,0x10001,0xE


[Reg_MPCIEX_5100AGN_1x2_MC]  
HKR,,Diversity11a,0x10003,0x0
HKR,,Diversity11b,0x10003,0x0
HKR,,Diversity11g,0x10003,0x0
HKR,,rlcChainSettings,0x10001,0x6
HKR,,tlcValidAntenna,0x10001,0x2


[Reg_MPCIEX_5100AGN_1x2_HMC]  
HKR,,Diversity11a,0x10003,0x0
HKR,,Diversity11b,0x10003,0x0
HKR,,Diversity11g,0x10003,0x0
HKR,,rlcChainSettings,0x10001,0x6
HKR,,tlcValidAntenna,0x10001,0x2



; Registry settings for Binding
; =============================

[Reg_CoInstaller32]

[MSI_NDIS.reg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 1


; Registry settings for EventLogs
; ===============================

[Common_EventLog_VISTA]
AddReg = Reg_CommonAddEventLog_VISTA

[Reg_CommonAddEventLog_VISTA]
HKR,, EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\Drivers\netw5v32.sys"
HKR,, TypesSupported,   0x00010001, 7

[Reg_GEN_3945_ABG_SP1]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

[Reg_GEN_3945_ABG_SP2]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

[Reg_GEN_3945_ABG_SP3]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

[Reg_GEN_3945_ABG_SP4]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

[Reg_GEN_4965_AGN_C_SP1]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"


[Reg_GEN_4965_AGN_C_SP2]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"


[Reg_GEN_4965_AGN_C_SP3]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"


[Reg_GEN_4965_AGN_SP1]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"


[Reg_GEN_4965_AGN_SP2]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"


[Reg_GEN_4965_AGN_SP3]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"


[Reg_GEN_4965_AG_SP1]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

[Reg_GEN_4965_AG_SP2]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

[Reg_GEN_4965_AG_SP3]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

[Reg_Lenovo_4965_AGN_C_SP1]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"


[Reg_Lenovo_4965_AGN_C_SP2]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"


[Reg_Lenovo_4965_AGN_C_SP3]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"


[Reg_Lenovo_4965_AGN_SP1]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"


[Reg_Lenovo_4965_AGN_SP2]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"


[Reg_Lenovo_4965_AGN_SP3]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"


[Reg_Lenovo_4965_AG_SP1]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

[Reg_Lenovo_4965_AG_SP2]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

[Reg_Lenovo_4965_AG_SP3]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

[Reg_Dell_4965_AGN_C_SP1]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"


[Reg_Dell_4965_AGN_C_SP2]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"


[Reg_Dell_4965_AGN_C_SP3]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"


[Reg_Dell_4965_AGN_SP1]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"


[Reg_Dell_4965_AGN_SP2]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"


[Reg_Dell_4965_AGN_SP3]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"


[Reg_Dell_4965_AG_SP1]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

[Reg_Dell_4965_AG_SP2]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

[Reg_Dell_4965_AG_SP3]
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"


[NIC_Service_VISTA]
DisplayName = %NIC_Service_DispName_VISTA%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary = %12%\netw5v32.sys
LoadOrderGroup  = NDIS

[Common_EventLog_VISTA]
AddReg = Reg_CommonAddEventLog_VISTA

;-----------------------------------------
; DestinationDirs

[CopyFiles_Driver_VISTA]
netw5v32.sys,,,2


[CopyFiles_NCPA32]

[SourceDisksNames]
1=%SOURCEDISK1%,,

[SourceDisksFiles]
netw5v32.sys   = 1,,

[DestinationDirs]
DefaultDestDir            = 11 ; Windows\System32
CopyFiles_Driver_VISTA=12;Windows\System32\Drivers
CopyFiles_NCPA32          = 11 ; Windows\System32

[Strings]
; Non-Localizable strings
MSFT                                 = "Microsoft"
PROVIDER_NAME                        = "Intel"
COMPANY_NAME                         = "Intel Corporation"

; Localizable strings
NIC_MPCIEX_3945ABG                 = "Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  = "Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 = "Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  = "Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 = "Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  = "Intel(R) Wireless WiFi Link 4965AG"
NIC_MPCIEX_5300AGN_3x3_MC          = "Intel(R)  WiFi Link 5300 AGN"
NIC_MPCIEX_5300AGN_3x3_HMC         = "Intel(R)  WiFi Link 5300 AGN"

NIC_MPCIEX_5100AGN_1x2_MC          = "Intel(R) WiFi Link 5100 AGN"
NIC_MPCIEX_5100AGN_1x2_MC_MOW2	   = "Intel(R) WiFi Link 5100 AGN"
NIC_MPCIEX_5100AGN_1x2_MC_KRA	   = "Intel(R) WiFi Link 5100 AGN"
NIC_MPCIEX_5100AGN_1x2_MC_BG	   = "Intel(R) WiFi Link 5100 BG"
NIC_MPCIEX_5100AGN_1x2_MC_BGN	   = "Intel(R) WiFi Link 5100 BGN"
NIC_MPCIEX_5100AGN_1x2_MC_ABG	   = "Intel(R) WiFi Link 5100 ABG"
NIC_MPCIEX_5100AGN_1x2_HMC         = "Intel(R) WiFi Link 5100 AGN"
NIC_MPCIEX_5100AGN_1x2_HMC_MOW2	   = "Intel(R) WiFi Link 5100 AGN"
NIC_MPCIEX_5100AGN_1x2_HMC_KRA	   = "Intel(R) WiFi Link 5100 AGN"
NIC_MPCIEX_5100AGN_1x2_HMC_BG	   = "Intel(R) WiFi Link 5100 BG"
NIC_MPCIEX_5100AGN_1x2_HMC_BGN	   = "Intel(R) WiFi Link 5100 BGN"
NIC_MPCIEX_5100AGN_1x2_HMC_ABG	   = "Intel(R) WiFi Link 5100 ABG"

NIC_MPCIEX_AdapterModel_3945ABG    = "Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     = "Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    = "Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     = "Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    = "Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     = "Intel(R) Wireless WiFi Link 4965AG"
NIC_MPCIEX_AdapterModel_5300AGN_3x3  = "Intel(R) WiFi Link 5300 AGN"
NIC_MPCIEX_AdapterModel_5100AGN_1x2  = "Intel(R) WiFi Link 5100 AGN"
NIC_MPCIEX_AdapterModel_5100AGN_1x2_MOW2  = "Intel(R) WiFi Link 5100 AGN"
NIC_MPCIEX_AdapterModel_5100AGN_1x2_KRA  = "Intel(R) WiFi Link 5100 AGN"
NIC_MPCIEX_AdapterModel_5100AGN_1x2_BG  = "Intel(R) WiFi Link 5100 BG"
NIC_MPCIEX_AdapterModel_5100AGN_1x2_BGN  = "Intel(R) WiFi Link 5100 BGN"
NIC_MPCIEX_AdapterModel_5100AGN_1x2_ABG  = "Intel(R) WiFi Link 5100 ABG"


NIC_DriverDesc_3945ABG               = "Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         = "Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   = "Intel(R) Wireless WiFi Link 3945ABG Adapter Driver for Windows Vista 32 Bit"
NIC_DriverDesc_3945BG                = "Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    = "Intel(R) Wireless WiFi Link 3945BG Adapter Driver for Windows Vista 32 Bit"
NIC_DriverDesc_3965ABG               = "Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   = "Intel(R) Wireless WiFi Link 3965ABG Adapter Driver for Windows Vista 32 Bit"
NIC_DriverDesc_3965BG                = "Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    = "Intel(R) Wireless WiFi Link 3965BG Adapter Driver for Windows Vista 32 Bit"
NIC_DriverDesc_4965AGN               = "Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   = "Intel(R) Wireless WiFi Link 4965AGN Adapter Driver for Windows Vista 32 Bit"
NIC_DriverDesc_4965AG          		   = "Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    = "Intel(R) Wireless WiFi Link 4965AG Adapter Driver for Windows Vista 32 Bit"
NIC_DriverDesc_5300AGN_3x3      		 = "Intel(R) WiFi Link 5300 Driver"
NIC_Service_DispName_5300AGN3x3_VISTA = "Intel(R) WiFi Link 5300 Adapter Driver for Windows Vista 32 Bit"
NIC_DriverDesc_5100AGN_1x2     		   = "Intel(R) WiFi Link 5100 Driver"
NIC_Service_DispName_5100AGN1x2_VISTA = "Intel(R) WiFi Link 5100 Adapter Driver for Windows Vista 32 Bit"
NIC_DriverDesc_5100AGN_1x2_BG     		    = "Intel(R) WiFi Link 5100 BG Driver"
NIC_Service_DispName_5100AGN1x2_BG_VISTA = "Intel(R) WiFi Link 5100 BG Adapter Driver for Windows Vista 32 Bit"
NIC_DriverDesc_5100AGN_1x2_BGN     		    = "Intel(R) WiFi Link 5100 BGN Driver"
NIC_Service_DispName_5100AGN1x2_BGN_VISTA = "Intel(R) WiFi Link 5100 BGN Adapter Driver for Windows Vista 32 Bit"
NIC_DriverDesc_5100AGN_1x2_ABG     		    = "Intel(R) WiFi Link 5100 ABG Driver"
NIC_Service_DispName_5100AGN1x2_ABG_VISTA = "Intel(R) WiFi Link 5100 ABG Adapter Driver for Windows Vista 32 Bit"
NIC_DriverDesc_5100ABG_1x2_ABG     		    = "Intel(R) WiFi Link 5100 ABG Driver"
NIC_Service_DispName_5100ABG1x2_VISTA = "Intel(R) WiFi Link 5100 ABG Adapter Driver for Windows Vista 32 Bit"

NIC_Service_DispName_VISTA							= "Intel(R) Wireless WiFi Link 5000 Series Adapter Driver for Windows Vista 32 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	= "Ad Hoc Channel 802.11 b/g"
RECOMMENDED_CHANNEL52_STR 	= "Ad Hoc Channel 802.11 a"
RECOMMENDED_BAND          	= "Ad Hoc Default Wireless Mode"
IBSS_TX_POWER_STR           = "Transmit Power"
ROAMING_AGGRESSIVENESS_STR	= "Roaming Aggressiveness"
ADHOC_POWER_MANAGEMENT_STR	= "Ad Hoc Power Management"
ADHOC_QOS_MODE_STR          = "Ad Hoc QoS Mode"
MIXED_MODE_PROTECTION_STR   = "Mixed Mode Protection"
THROUGHPUT_ENHANCEMENT_STR  = "Throughput Enhancement"
WIRELESS_MODE_STR           = "Wireless Mode"
CHANNELWIDTH52              = "802.11n Channel Width for band 5.2"
CHANNELWIDTH24              = "802.11n Channel Width for band 2.4"
TGnMode                     = "802.11n Mode"
FAT_CHANNEL_TOLERANT		= "Fat Channel Intolerant"

LOWEST_STR					= "Lowest"
MEDIUM_LOW_STR				= "Medium-low"
MEDIUM_STR					= "Medium"
MEDIUM_HIGH_STR				= "Medium-High"
HIGHEST_STR					= "Highest"
DISABLED_STR				= "Disabled"
ENABLED_STR 				= "Enabled"
MAXIMUM_POWER_SAVING_STR	= "Maximum Power Savings"
NOISY_ENVIRONMENT_STR		= "Noisy Environment"
WMM_STR                     = "WMM "
CTS_TO_SELF_ENABLED_STR     = "CTS-to-self Enabled"
RTS_CTS_ENABLED_STR         = "RTS/CTS Enabled"
AUTO_STR                    = "Auto"
CHANNELWIDTH20ONLY          = "20 MHz Only"
CHANNELWIDTHAUTO            = "Auto"
WMM_DISABLED_STR            = "WMM Disabled"
WMM_ENABLED_STR             = "WMM Enabled"

SOURCEDISK1                  = "Intel(R) Wireless WiFi Link 5000 Series Install Disk"

