; Copyright (c) Microsoft Corporation.  All rights reserved.

[Version]
Signature="$WINDOWS NT$"
Class=System
ClassGuid={4D36E97D-E325-11CE-BFC1-08002BE10318}
Provider=%MSFT%
DriverVer=06/21/2006,6.1.7601.17514

[SignatureAttributes]
swenum.sys=SignatureAttributes.DRM

[SignatureAttributes.DRM]
DRMLevel=1300

[SourceDisksNames]
3426=windows cd

[SourceDisksFiles]
alim1541.sys    = 3426
viaagp.sys      = 3426
amdagp.sys      = 3426
sisagp.sys      = 3426
nv_agp.sys    = 3426
uliagpkx.sys  = 3426
swenum.sys         = 3426
pci.sys            = 3426
agp440.sys    = 3426
volmgr.sys         = 3426
streamci.dll       = 3426
termdd.sys         = 3426
mssmbios.sys       = 3426
msisadrv.sys       = 3426
isapnp.sys         = 3426
vdrvroot.sys       = 3426

[DestinationDirs]
SWENUM.CoInstallers.CopyFiles = 11 ; %windir%\System32
DefaultDestDir = 12                ; DIRID_DRIVERS

[ControlFlags]
BasicDriverOk=*
ExcludeFromSelect=*

[Manufacturer]
%GENDEV_MFG%=GENDEV_SYS,NTx86
%ACC_MFG%=ACC_SYS,NTx86
%ACER_MFG%=ACER_SYS,NTx86
%ALI_MFG%=ALI_SYS,NTx86
%AMD_MFG%=AMD_SYS,NTx86
%ATI_MFG%=ATI_SYS,NTx86
%COMPAQ_MFG%=COMPAQ_SYS,NTx86
%CONTAQ_MFG%=CONTAQ_SYS,NTx86
%CYRIX_MFG%=CYRIX_SYS,NTx86
%DEC_MFG%=DEC_SYS,NTx86
%HITACHI_MFG%=HITACHI_SYS,NTx86
%HP_MFG%=HP_SYS,NTx86
%IBM_MFG%=IBM_SYS,NTx86
%INTEL_MFG%=INTEL_SYS,NTx86
%MICRON_MFG%=MICRON_SYS,NTx86

%NATSEMI_MFG%=NATSEMI_SYS,NTx86
%NEC_MFG%=NEC_SYS,NTx86
%NVIDIA_MFG%=NVIDIA_SYS,NTx86
%OPTI_MFG%=OPTI_SYS,NTx86
%SERVERWORKS_MFG%=SERVERWORKS_SYS,NTx86
%SIS_MFG%=SIS_SYS,NTx86
%SMSC_MFG%=SMSC_SYS,NTx86
%TEXAS_MFG%=TEXAS_SYS,NTx86
%TOSHIBA_MFG%=TOSHIBA_SYS,NTx86
%ULI_MFG%=ULI_SYS,NTx86
%UMC_MFG%=UMC_SYS,NTx86
%VIA_MFG%=VIA_SYS,NTx86
%VLSI_MFG%=VLSI_SYS,NTx86

[GENDEV_SYS.NTx86]
%*PNP0A00.DeviceDesc%          = MSISADRV, *PNP0A00          ; ISA BUS
%*PNP0A01.DeviceDesc%          = MSISADRV, *PNP0A01          ; EISA BUS
%*PNP0A04.DeviceDesc%          = MSISADRV, *PNP0A04          ; VL BUS
%*PNP0A03.DeviceDesc%          = PCI_DRV_ROOT, *PNP0A03      ; ROOT PCI BUS
%PCI\CC_0604.DeviceDesc%       = PCI_DRV, PCI\CC_0604        ; PCI-PCI BRIDGE
%PCI\CC_0604&DT_4.DeviceDesc%  = PCI_DRV, PCI\CC_0604&DT_4   ; PCI Express Root Port
%PCI\CC_0604&DT_5.DeviceDesc%  = PCI_DRV, PCI\CC_0604&DT_5   ; PCI Express Upstream Switch Port
%PCI\CC_0604&DT_6.DeviceDesc%  = PCI_DRV, PCI\CC_0604&DT_6   ; PCI Express Downstream Switch Port
%PCI\CC_0604&DT_7.DeviceDesc%  = PCI_DRV, PCI\CC_0604&DT_7   ; PCI Express to PCI(-X) Bridge
%PCI\CC_0604&DT_8.DeviceDesc%  = PCI_DRV, PCI\CC_0604&DT_8   ; PCI(-X) to PCI Express Bridge
%PCI\CC_0601.DeviceDesc%       = MSISADRV, PCI\CC_0601       ; PCI-ISA BRIDGE
%PCI\CC_0602.DeviceDesc%       = MSISADRV, PCI\CC_0602       ; PCI-EISA BRIDGE
%PCI\CC_0600.DeviceDesc%       = NO_DRV, PCI\CC_0600         ; HOST PCI BRIDGE
%PCI\CC_0500.DeviceDesc%       = NO_DRV,PCI\CC_0500          ; RAM Controller
%Volmgr.DeviceDesc%            = Volmgr, Root\VOLMGR         ; Volume Manager
%SWENUM.DeviceDesc%            = SWENUM, ROOT\SWENUM         ; Software Bus
%Root\MSSMBios.DeviceDesc%     = MSSMBIOS_DRV, Root\MSSMBios ; MSSMBios Driver
%LPTENUM\MicrosoftRawPort958A.DeviceDesc% = NO_DRV, LPTENUM\MicrosoftRawPort958A ; Printer Port Logical Interface
%RDP_MOU.DeviceDesc%           = RDP_MOU,ROOT\RDP_MOU        ; RDP Remote Mouse
%RDP_KBD.DeviceDesc%           = RDP_KBD,ROOT\RDP_KBD        ; RDP Remote Keyboard
%VDRVROOT.DeviceDesc%          = VDRVROOT, Root\VDRVROOT     ; Virtual Drive Enumerator


%ACPI0004.DeviceDesc%   = NO_DRV_X_PNP, *ACPI0004  ; Generic ACPI Bus - Module Device
%ACPI0004.DeviceDesc%   = NO_DRV_X_PNP, ACPI0004   ; Generic ACPI Bus - Module Device
%*PNP0000.DeviceDesc%   = NO_DRV_PIC, *PNP0000     ; PIC
%*PNP0001.DeviceDesc%   = NO_DRV_PIC, *PNP0001     ; EISA PIC
%*PNP0003.DeviceDesc%   = NO_DRV_PIC, *PNP0003     ; APIC
%*PNP0004.DeviceDesc%   = NO_DRV_PIC, *PNP0004     ; Cyrix SLiC MPIC
%*PNP0100.DeviceDesc%   = NO_DRV_X, *PNP0100       ; System Timer
%*PNP0101.DeviceDesc%   = NO_DRV_X, *PNP0101       ; EISA System Timer
%*PNP0103.DeviceDesc%   = NO_DRV_HPET, *PNP0103    ; HPET
%*PNP0200.DeviceDesc%   = NO_DRV_X, *PNP0200       ; DMA
%*PNP0201.DeviceDesc%   = NO_DRV_X, *PNP0201       ; EISA DMA
%*PNP0800.DeviceDesc%   = NO_DRV_X, *PNP0800       ; System Speaker
%*PNP0B00.DeviceDesc%   = NO_DRV_X, *PNP0B00       ; Real Time Clock
%*PNP0A05.DeviceDesc%   = NO_DRV_X_PNP, *PNP0A05   ; Generic ACPI Bus
%*PNP0A06.DeviceDesc%   = NO_DRV_X_PNP, *PNP0A06   ; Extended IO Bus
%*PNP0C00.DeviceDesc%   = NO_DRV_X, *PNP0C00       ; PnP BIOS
%*PNP0C01.DeviceDesc%   = NO_DRV_MBRES, *PNP0C01   ; System board
%*PNP0C02.DeviceDesc%   = NO_DRV_MBRES, *PNP0C02   ; Motherboard resources
%*PNP0C04.DeviceDesc%   = NO_DRV_X, *PNP0C04       ; Numeric processor
;%*PNP0C05.DeviceDesc%  = NO_DRV, *PNP0C05         ; APM BIOS
%*PNP0C09.DeviceDesc%   = NO_DRV, *PNP0C09         ; Embedded Controller
;%*PNP0C0A.DeviceDesc%  = NO_DRV, *PNP0C0A         ; APM Battery
%*PNP0C0B.DeviceDesc%   = NO_DRV, *PNP0C0B         ; APM FAN
%*PNP0C0C.DeviceDesc%   = NO_DRV, *PNP0C0C         ; APM Power Button
%*PNP0C0D.DeviceDesc%   = NO_DRV, *PNP0C0D         ; APM Lid
%*PNP0C0E.DeviceDesc%   = NO_DRV, *PNP0C0E         ; APM Sleep Button
;%*PNP0C0F.DeviceDesc%  = NO_DRV, *PNP0C0F         ; ACPI IRQ Holder
;%*PNP0C13.DeviceDesc%  = NO_DRV, *PNP0C13         ; PnP BIOS in ACPI fail safe
%*PNP0C15.DeviceDesc%   = NO_DRV, *PNP0C15         ; Docking Station
%*PNP0C32.DeviceDesc%   = NO_DRV, *PNP0C32         ; Direct Application Launch Button
%ACPI\FixedButton.DeviceDesc%    = NO_DRV, ACPI\FixedButton ; ACPI Fixed Feature Button
%ACPI\ThermalZone.DeviceDesc%    = NO_DRV, ACPI\ThermalZone ; ACPI Thermal Zone
%ACPI\DockDevice.DeviceDesc%     = NO_DRV, ACPI\DockDevice  ; ACPI Dock Device
%ACPI\DockDevice.DeviceDesc%     = MS_TPDOCK, ACPI\DockDevice&_SB_.PCI_.OAK_       ; ACPI Dock Device (TP 570 Dock)
%ACPI\DockDevice.DeviceDesc%     = MS_TPSLICE, ACPI\DockDevice&_SB_.PCI_.ISA_.SLCE ; ACPI Dock Device (TP 570 Slice)
%*LEGACYISAPNP.DeviceDesc%       = LEGACY_ISAPNP_DRV, *LEGACYISAPNP                ; References LEGACY_ISAPNP_DRV files
%ISAPNP\ReadDataPort.DeviceDesc% = NO_DRV, ISAPNP\ReadDataPort

[ACC_SYS.NTx86]
%PCI\VEN_10AA&DEV_0000.DeviceDesc% = MSISADRV, PCI\VEN_10AA&DEV_0000

[ACER_SYS.NTx86]
%PCI\VEN_1025&DEV_1435.DeviceDesc% = MSISADRV, PCI\VEN_1025&DEV_1435

[ALI_SYS.NTx86]
%PCI\VEN_10B9&DEV_1445.DeviceDesc% = MSISADRV, PCI\VEN_10B9&DEV_1445
%PCI\VEN_10B9&DEV_1449.DeviceDesc% = MSISADRV, PCI\VEN_10B9&DEV_1449
%PCI\VEN_10B9&DEV_1451.DeviceDesc% = NO_DRV, PCI\VEN_10B9&DEV_1451
%PCI\VEN_10B9&DEV_1489.DeviceDesc% = MSISADRV, PCI\VEN_10B9&DEV_1489
%PCI\VEN_10B9&DEV_1521.DeviceDesc% = NO_DRV, PCI\VEN_10B9&DEV_1521
%PCI\VEN_10B9&DEV_1523.DeviceDesc% = MSISADRV, PCI\VEN_10B9&DEV_1523
%PCI\VEN_10B9&DEV_1531.DeviceDesc% = NO_DRV, PCI\VEN_10B9&DEV_1531
%PCI\VEN_10B9&DEV_1533.DeviceDesc% = MSISADRV, PCI\VEN_10B9&DEV_1533
%PCI\VEN_10B9&DEV_1541.DeviceDesc% = NO_DRV, PCI\VEN_10B9&DEV_1541
%PCI\VEN_10B9&DEV_1621.DeviceDesc% = NO_DRV, PCI\VEN_10B9&DEV_1621
%PCI\VEN_10B9&DEV_1647.DeviceDesc% = NO_DRV, PCI\VEN_10B9&DEV_1647
%PCI\VEN_10B9&DEV_1651.DeviceDesc% = NO_DRV, PCI\VEN_10B9&DEV_1651
%PCI\VEN_10B9&DEV_5243.DeviceDesc% = AGPALi_Install,PCI\VEN_10B9&DEV_5243        ; ALi 1541
%PCI\VEN_10B9&DEV_5247.DeviceDesc% = AGPALi_Install,PCI\VEN_10B9&DEV_5247        ; ALi 1621
%PCI\VEN_10B9&DEV_7101.DeviceDesc% = NO_DRV, PCI\VEN_10B9&DEV_7101

[AMD_SYS.NTx86]
%PCI\VEN_1002&DEV_5A23.DeviceDesc% = NO_DRV,PCI\VEN_1002&DEV_5A23
 ; AMD IOMMU
%PCI\VEN_1022&DEV_1100.DeviceDesc% = NO_DRV,PCI\VEN_1022&DEV_1100                ; AMD HyperTransport Configuration
%PCI\VEN_1022&DEV_1101.DeviceDesc% = NO_DRV,PCI\VEN_1022&DEV_1101                ; AMD Address Map Configuration
%PCI\VEN_1022&DEV_1102.DeviceDesc% = NO_DRV,PCI\VEN_1022&DEV_1102                ; AMD DRAM & Trace Mode Configuration
%PCI\VEN_1022&DEV_1103.DeviceDesc% = NO_DRV,PCI\VEN_1022&DEV_1103                ; AMD Miscellaneous Configuration
%PCI\VEN_1022&DEV_7007.DeviceDesc% = AMDAGP_Install,PCI\VEN_1022&DEV_7007        ; AMD 751
%PCI\VEN_1022&DEV_700D.DeviceDesc% = AMDAGP_Install,PCI\VEN_1022&DEV_700D        ; AMD 762
%PCI\VEN_1022&DEV_700F.DeviceDesc% = AMDAGP_Install,PCI\VEN_1022&DEV_700F        ; AMD 761
%PCI\VEN_1022&DEV_740B.DeviceDesc% = NO_DRV, PCI\VEN_1022&DEV_740B               ; 756 Power Management Controller
%PCI\VEN_1022&DEV_7413.DeviceDesc% = NO_DRV,PCI\VEN_1022&DEV_7413                ; 766 Power Management Controller
%PCI\VEN_1022&DEV_7443.DeviceDesc% = NO_DRV,PCI\VEN_1022&DEV_7443                ; 768 Power Management Controller
%PCI\VEN_1022&DEV_7451.DeviceDesc% = NO_DRV,PCI\VEN_1022&DEV_7451                ; 8131 I/O APIC
%PCI\VEN_1022&DEV_7459.DeviceDesc% = NO_DRV,PCI\VEN_1022&DEV_7459                ; 8132 I/O APIC
%PCI\VEN_1022&DEV_746A.DeviceDesc% = NO_DRV,PCI\VEN_1022&DEV_746A                ; 8111 SMBus 2.0 Controller
%PCI\VEN_1022&DEV_746B.DeviceDesc% = NO_DRV,PCI\VEN_1022&DEV_746B                ; 8111 System Management Controller

[ATI_SYS.NTx86]
%PCI\VEN_1002&DEV_4371.DeviceDesc% = PCI_DRV,PCI\VEN_1002&DEV_4371               ; ATI I/O Communications Processor PCI Bus Controller
%PCI\VEN_1002&DEV_4372.DeviceDesc% = NO_DRV,PCI\VEN_1002&DEV_4372                ; ATI I/O Communications Processor SMBus Controller
%PCI\VEN_1002&DEV_4377.DeviceDesc% = MSISADRV,PCI\VEN_1002&DEV_4377              ; ATI I/O Communications Processor LPC Controller
%PCI\VEN_1002&DEV_4384.DeviceDesc% = PCI_DRV,PCI\VEN_1002&DEV_4384               ; ATI I/O Communications Processor PCI Bus Controller
%PCI\VEN_1002&DEV_4385.DeviceDesc% = NO_DRV_MEM,PCI\VEN_1002&DEV_4385            ; ATI I/O Communications Processor SMBus Controller
                                                                                 ;
                                                                                 ;   The HPET is contained in a BAR on this device.  It
                                                                                 ;   conflicts with the HAL's attempt to claim the HPET
                                                                                 ;   resources and is thus marked NO_DRV_MEM.
                                                                                 ;
%PCI\VEN_1002&DEV_438D.DeviceDesc% = MSISADRV,PCI\VEN_1002&DEV_438D              ; ATI I/O Communications Processor LPC Controller

[COMPAQ_SYS.NTx86]
%PCI\VEN_0E11&DEV_0001.DeviceDesc%         = MSISADRV, PCI\VEN_0E11&DEV_0001
%PCI\VEN_0E11&DEV_0002.DeviceDesc%         = MSISADRV, PCI\VEN_0E11&DEV_0002
%PCI\VEN_0E11&DEV_1000.DeviceDesc%         = NO_DRV, PCI\VEN_0E11&DEV_1000
%PCI\VEN_0E11&DEV_2000.DeviceDesc%         = NO_DRV, PCI\VEN_0E11&DEV_2000
%PCI\VEN_0E11&DEV_AE29.DeviceDesc%         = MSISADRV, PCI\VEN_0E11&DEV_AE29
%PCI\VEN_0E11&DEV_AE2B.DeviceDesc%         = MSISADRV, PCI\VEN_0E11&DEV_AE2B
%PCI\VEN_0E11&DEV_A0F0.DeviceDesc%         = NO_DRV, PCI\VEN_0E11&DEV_A0F0
%PCI\VEN_0E11&DEV_A0F3.DeviceDesc%         = MSISADRV, PCI\VEN_0E11&DEV_A0F3
%PCI\VEN_0E11&DEV_A0F7.DeviceDesc%         = NO_DRV, PCI\VEN_0E11&DEV_A0F7
%PCI\VEN_0E11&DEV_AE2A.DeviceDesc%         = NO_DRV, PCI\VEN_0E11&DEV_AE2A
%PCI\VEN_0E11&DEV_AE31.DeviceDesc%         = NO_DRV, PCI\VEN_0E11&DEV_AE31
%PCI\VEN_0E11&DEV_AE69.DeviceDesc%         = MSISADRV, PCI\VEN_0E11&DEV_AE69
%PCI\VEN_0E11&DEV_AE6C&CC_0600.DeviceDesc% = NO_DRV, PCI\VEN_0E11&DEV_AE6C&CC_0600
%PCI\VEN_0E11&DEV_AE6C&CC_0604.DeviceDesc% = PCI_DRV, PCI\VEN_0E11&DEV_AE6C&CC_0604
%PCI\VEN_0E11&DEV_AE6D.DeviceDesc%         = NO_DRV, PCI\VEN_0E11&DEV_AE6D
%PCI\VEN_8086&DEV_123F&SUBSYS_A2F90E11.DeviceDesc% = NO_DRV, PCI\VEN_8086&DEV_123F&SUBSYS_A2F90E11
%*CPQA0EF.DeviceDesc%                      = NO_DRV,, *CPQA0EF       ; Deskpro thermal sensor
%*CPQAE08.DeviceDesc%                      = NO_DRV,, *CPQAE08       ; Deskpro thermal sensor
%*CPQAE30.DeviceDesc%                      = NO_DRV, *CPQAE30
%*CPQAE3B.DeviceDesc%                      = NO_DRV, *CPQAE3B
%*CPQAE3C.DeviceDesc%                      = NO_DRV, *CPQAE3C
%*CPQAE4A.DeviceDesc%                      = NO_DRV, *CPQAE4A
%*CPQAE4B.DeviceDesc%                      = NO_DRV, *CPQAE4B
%*CPQAE4C.DeviceDesc%                      = NO_DRV, *CPQAE4C
%*CPQAE4D.DeviceDesc%                      = NO_DRV, *CPQAE4D
%*CPQAE53.DeviceDesc%                      = NO_DRV, *CPQAE53
%*CPQAE54.DeviceDesc%                      = NO_DRV, *CPQAE54
%*CPQAE55.DeviceDesc%                      = NO_DRV, *CPQAE55
%*CPQB05F.DeviceDesc%                      = NO_DRV, *CPQB05F
%*CPQB118.DeviceDesc%                      = NO_DRV, *CPQB118
%*CPQB119.DeviceDesc%                      = NO_DRV, *CPQB119
%*CPQB11A.DeviceDesc%                      = NO_DRV, *CPQB11A
%*CPQFA1B.DeviceDesc%                      = NO_DRV, *CPQFA1B        ; Compaq memory board

[CONTAQ_SYS.NTx86]
%PCI\VEN_1080&DEV_0600.DeviceDesc% = MSISADRV, PCI\VEN_1080&DEV_0600

[CYRIX_SYS.NTx86]
%PCI\VEN_1078&DEV_0000.DeviceDesc% = MSISADRV,PCI\VEN_1078&DEV_0000
%PCI\VEN_1078&DEV_0002.DeviceDesc% = MSISADRV,PCI\VEN_1078&DEV_0002

[DEC_SYS.NTx86]
%PCI\VEN_1011&DEV_0001.DeviceDesc% = PCI_DRV, PCI\VEN_1011&DEV_0001
%PCI\VEN_1011&DEV_0021.DeviceDesc% = PCI_DRV, PCI\VEN_1011&DEV_0021
%PCI\VEN_1011&DEV_0022.DeviceDesc% = PCI_DRV, PCI\VEN_1011&DEV_0022
%PCI\VEN_1011&DEV_0024.DeviceDesc% = PCI_DRV, PCI\VEN_1011&DEV_0024
%PCI\VEN_1011&DEV_0025.DeviceDesc% = PCI_DRV, PCI\VEN_1011&DEV_0025
%PCI\VEN_1011&DEV_0026.DeviceDesc% = PCI_DRV, PCI\VEN_1011&DEV_0026

[HITACHI_SYS.NTx86]
%PCI\VEN_1054&DEV_3005.DeviceDesc%         = NO_DRV, PCI\VEN_1054&DEV_3005
%PCI\VEN_1054&DEV_3006.DeviceDesc%         = NO_DRV, PCI\VEN_1054&DEV_3006

[HP_SYS.NTx86]
%PCI\VEN_103C&DEV_10C1.DeviceDesc% = NO_DRV, PCI\VEN_103C&DEV_10C1
%PCI\VEN_103C&DEV_10ED.DeviceDesc% = NO_DRV, PCI\VEN_103C&DEV_10ED
%PCI\VEN_103C&DEV_1219.DeviceDesc% = NO_DRV, PCI\VEN_103C&DEV_1219
%PCI\VEN_103C&DEV_121A.DeviceDesc% = NO_DRV, PCI\VEN_103C&DEV_121A
%PCI\VEN_103C&DEV_121B.DeviceDesc% = NO_DRV, PCI\VEN_103C&DEV_121B
%PCI\VEN_103C&DEV_121C.DeviceDesc% = NO_DRV, PCI\VEN_103C&DEV_121C
%HWPC209.DeviceDesc%               = NO_DRV, *HWPC209

[IBM_SYS.NTx86]
%PCI\VEN_1014&DEV_000A.DeviceDesc%        = MSISADRV, PCI\VEN_1014&DEV_000A
%PCI\VEN_1014&DEV_0017.DeviceDesc%        = NO_DRV, PCI\VEN_1014&DEV_0017
%PCI\VEN_1014&DEV_0022&REV_00.DeviceDesc% = PCI_DRV, PCI\VEN_1014&DEV_0022&REV_00
%PCI\VEN_1014&DEV_0022.DeviceDesc%        = PCI_DRV, PCI\VEN_1014&DEV_0022
%PCI\VEN_1014&DEV_0095.DeviceDesc%        = PCI_DRV, PCI\VEN_1014&DEV_0095
%*IBM006A.DeviceDesc%                     = NO_DRV, *IBM006A

[INTEL_SYS.NTx86]
%*INT0800.DeviceDesc%                      = NO_DRV_MEM, *INT0800
%PCI\VEN_8086&DEV_0008.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_0008
%PCI\VEN_8086&DEV_0040.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_0040
%PCI\VEN_8086&DEV_0041.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_0041
%PCI\VEN_8086&DEV_0050.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_0050
%PCI\VEN_8086&DEV_0051.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_0051
%PCI\VEN_8086&DEV_0326.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_0326
%PCI\VEN_8086&DEV_0327.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_0327
%PCI\VEN_8086&DEV_0329.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_0329
%PCI\VEN_8086&DEV_032A.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_032A
%PCI\VEN_8086&DEV_032C.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_032C
%PCI\VEN_8086&DEV_0330.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_0330
%PCI\VEN_8086&DEV_0331.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_0331
%PCI\VEN_8086&DEV_0332.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_0332
%PCI\VEN_8086&DEV_0333.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_0333
%PCI\VEN_8086&DEV_0334.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_0334
%PCI\VEN_8086&DEV_0370.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_0370
%PCI\VEN_8086&DEV_0371.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_0371
%PCI\VEN_8086&DEV_0372.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_0372
%PCI\VEN_8086&DEV_0373.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_0373
%PCI\VEN_8086&DEV_0374.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_0374
%PCI\VEN_8086&DEV_0482.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_0482           ; INTEL PCI V1 PCI-EISA bridge
%PCI\VEN_8086&DEV_0483.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_0483
%PCI\VEN_8086&DEV_0484.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_0484           ; INTEL PCI V1 PCI-ISA bridge
%PCI\VEN_8086&DEV_0486.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_0486           ; INTEL i486 PCIset with ISA bridge
%PCI\VEN_8086&DEV_04A3_OLD.DeviceDesc%     = NO_DRV,PCI\VEN_8086&DEV_04A3&REV_00
%PCI\VEN_8086&DEV_04A3_OLD.DeviceDesc%     = NO_DRV,PCI\VEN_8086&DEV_04A3&REV_01
%PCI\VEN_8086&DEV_04A3_OLD.DeviceDesc%     = NO_DRV,PCI\VEN_8086&DEV_04A3&REV_02
%PCI\VEN_8086&DEV_04A3_OLD.DeviceDesc%     = NO_DRV,PCI\VEN_8086&DEV_04A3&REV_03
%PCI\VEN_8086&DEV_04A3.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_04A3
%PCI\VEN_8086&DEV_1130.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_1130             ; 815, 815E, 815EM
%PCI\VEN_8086&DEV_1131.DeviceDesc%   = AGP440_Install, PCI\VEN_8086&DEV_1131     ; 815, 815E, 815EM
%PCI\VEN_8086&DEV_1161.DeviceDesc%         = NO_DRV_MEM, PCI\VEN_8086&DEV_1161         ; 82840-1161
%PCI\VEN_8086&DEV_1225.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_1225
%PCI\VEN_8086&DEV_122D.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_122D
%PCI\VEN_8086&DEV_122E.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_122E           ; INTEL PCI-ISA bridge
%PCI\VEN_8086&DEV_1234.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_1234           ; INTEL PCI-ISA bridge
%PCI\VEN_8086&DEV_1235.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_1235
%PCI\VEN_8086&DEV_1237.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_1237
%PCI\VEN_8086&DEV_123B.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_123B            ; INTEL PCI-PCI docking bridge
%PCI\VEN_8086&DEV_123C.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_123C           ; INTEL PCI-ISA docking bridge
%PCI\VEN_8086&DEV_123D.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_123D             ; INTEL 683053 PIC
%PCI\VEN_8086&DEV_123F.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_123F             ; INTEL Hot plug PCI controller
%PCI\VEN_8086&DEV_124B.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_124B            ; INTEL PCI-PCI docking bridge
%PCI\VEN_8086&DEV_1250.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_1250
%PCI\VEN_8086&DEV_1360.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_1360            ; 82840-1360
%PCI\VEN_8086&DEV_1361.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_1361             ; 82840-1361
%PCI\VEN_8086&DEV_1460.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_1460            ; Hub Interface to PCI Bridges
%PCI\VEN_8086&DEV_1461.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_1461             ; I/OxAPIC Interrupt Controllers
%PCI\VEN_8086&DEV_1462.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_1462             ; Intel Hot Plug PCI controller
%PCI\VEN_8086&DEV_1A21.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_1A21             ; 82840-1A21
%PCI\VEN_8086&DEV_1A23.DeviceDesc%         = AGP840_Install,PCI\VEN_8086&DEV_1A23      ; 82840-1A23
%PCI\VEN_8086&DEV_1A24.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_1A24            ; 82840-1A24
%PCI\VEN_8086&DEV_1A30.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_1A30
%PCI\VEN_8086&DEV_1A31.DeviceDesc%         = AGP440_Install,PCI\VEN_8086&DEV_1A31      ; 82845-1A31
%PCI\VEN_8086&DEV_1A38.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_1A38
%PCI\VEN_8086&DEV_2410.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_2410           ; INTEL PCI-ISA bridge
%PCI\VEN_8086&DEV_2413.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2413
%PCI\VEN_8086&DEV_2418.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2418
%PCI\VEN_8086&DEV_2420.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_2420           ; INTEL PCI-ISA bridge
%PCI\VEN_8086&DEV_2423.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2423
%PCI\VEN_8086&DEV_2428.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2428
%PCI\VEN_8086&DEV_2440.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_2440           ; INTEL PCI-ISA bridge
%PCI\VEN_8086&DEV_2443.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2443
%PCI\VEN_8086&DEV_2448.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2448            ;Intel 82801
%PCI\VEN_8086&DEV_244C.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_244C           ; INTEL PCI-ISA bridge
%PCI\VEN_8086&DEV_244E.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_244E
%PCI\VEN_8086&DEV_2480.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_2480           ; INTEL 82801BA LPC Interface Controller
%PCI\VEN_8086&DEV_2483.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2483             ;Intel 82801
%PCI\VEN_8086&DEV_248C.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_248C           ;Intel 82801
%PCI\VEN_8086&DEV_24C0.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_24C0           ; INTEL 82801DB LPC Interface Controller
%PCI\VEN_8086&DEV_24C3.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_24C3
%PCI\VEN_8086&DEV_24CC.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_24CC           ; INTEL 82801DB LPC Interface Controller
%PCI\VEN_8086&DEV_24D0.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_24D0
%PCI\VEN_8086&DEV_24D3.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_24D3
%PCI\VEN_8086&DEV_24DC.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_24DC
%PCI\VEN_8086&DEV_2500.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2500
%PCI\VEN_8086&DEV_2501.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2501             ; 82820-2501
%PCI\VEN_8086&DEV_250B.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_250B             ; 82820-250B
%PCI\VEN_8086&DEV_250F.DeviceDesc%         = AGP440_Install,PCI\VEN_8086&DEV_250F      ; 828820
%PCI\VEN_8086&DEV_2530.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2530               ; 850
%PCI\VEN_8086&DEV_2531.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2531               ; 860
%PCI\VEN_8086&DEV_2532.DeviceDesc%         = AGP440_Install,PCI\VEN_8086&DEV_2532
%PCI\VEN_8086&DEV_2533.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2533
%PCI\VEN_8086&DEV_2534.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2534
%PCI\VEN_8086&DEV_2540.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2540
%PCI\VEN_8086&DEV_2541.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2541
%PCI\VEN_8086&DEV_2543.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2543
%PCI\VEN_8086&DEV_2544.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2544
%PCI\VEN_8086&DEV_2545.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2545
%PCI\VEN_8086&DEV_2546.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2546
%PCI\VEN_8086&DEV_2547.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2547
%PCI\VEN_8086&DEV_2548.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2548
%PCI\VEN_8086&DEV_254C.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_254C
%PCI\VEN_8086&DEV_2550.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2550
%PCI\VEN_8086&DEV_2551.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2551
%PCI\VEN_8086&DEV_2552.DeviceDesc% = AGP440_Install, PCI\VEN_8086&DEV_2552
%PCI\VEN_8086&DEV_2553.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2553
%PCI\VEN_8086&DEV_2554.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2554
%PCI\VEN_8086&DEV_255D.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_255D
%PCI\VEN_8086&DEV_2560.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2560
%PCI\VEN_8086&DEV_2561.DeviceDesc%   = AGP440_Install,PCI\VEN_8086&DEV_2561       ; 845G
%PCI\VEN_8086&DEV_2570.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2570
%PCI\VEN_8086&DEV_2571.DeviceDesc% = AGP440_Install, PCI\VEN_8086&DEV_2571      ; 82865G\PE\P Processor to AGP Controller
%PCI\VEN_8086&DEV_2573.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2573
%PCI\VEN_8086&DEV_2576.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2576
%PCI\VEN_8086&DEV_2578.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2578
%PCI\VEN_8086&DEV_2579.DeviceDesc% = AGP440_Install, PCI\VEN_8086&DEV_2579
%PCI\VEN_8086&DEV_257B.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_257B
%PCI\VEN_8086&DEV_257E.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_257E
%PCI\VEN_8086&DEV_2580.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2580
%PCI\VEN_8086&DEV_2581.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2581
%PCI\VEN_8086&DEV_2584.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2584
%PCI\VEN_8086&DEV_2585.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2585
%PCI\VEN_8086&DEV_2588.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2588
%PCI\VEN_8086&DEV_2589.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2589
%PCI\VEN_8086&DEV_2590.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2590
%PCI\VEN_8086&DEV_2591.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2591
%PCI\VEN_8086&DEV_25A1.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_25A1
%PCI\VEN_8086&DEV_25A4.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_25A4
%PCI\VEN_8086&DEV_25AB.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_25AB
%PCI\VEN_8086&DEV_25AC.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_25AC
%PCI\VEN_8086&DEV_25AE.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_25AE
%PCI\VEN_8086&DEV_25C0.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_25C0
%PCI\VEN_8086&DEV_25D0.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_25D0
%PCI\VEN_8086&DEV_25D4.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_25D4
%PCI\VEN_8086&DEV_25D8.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_25D8
%PCI\VEN_8086&DEV_25E2.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_25E2
%PCI\VEN_8086&DEV_25E3.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_25E3
%PCI\VEN_8086&DEV_25E4.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_25E4
%PCI\VEN_8086&DEV_25E5.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_25E5
%PCI\VEN_8086&DEV_25E6.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_25E6
%PCI\VEN_8086&DEV_25E7.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_25E7
%PCI\VEN_8086&DEV_25F0.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_25F0
%PCI\VEN_8086&DEV_25F1.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_25F1
%PCI\VEN_8086&DEV_25F3.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_25F3
%PCI\VEN_8086&DEV_25F5.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_25F5
%PCI\VEN_8086&DEV_25F6.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_25F6
%PCI\VEN_8086&DEV_25F7.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_25F7
%PCI\VEN_8086&DEV_25F8.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_25F8
%PCI\VEN_8086&DEV_25F9.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_25F9
%PCI\VEN_8086&DEV_25FA.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_25FA
%PCI\VEN_8086&DEV_2600.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2600
%PCI\VEN_8086&DEV_2601.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2601
%PCI\VEN_8086&DEV_2602.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2602
%PCI\VEN_8086&DEV_2603.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2603
%PCI\VEN_8086&DEV_2604.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2604
%PCI\VEN_8086&DEV_2605.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2605
%PCI\VEN_8086&DEV_2606.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2606
%PCI\VEN_8086&DEV_2607.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2607
%PCI\VEN_8086&DEV_2608.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2608
%PCI\VEN_8086&DEV_2609.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2609
%PCI\VEN_8086&DEV_260A.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_260A
%PCI\VEN_8086&DEV_260C.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_260C
%PCI\VEN_8086&DEV_2610.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2610
%PCI\VEN_8086&DEV_2611.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2611
%PCI\VEN_8086&DEV_2612.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2612
%PCI\VEN_8086&DEV_2613.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2613
%PCI\VEN_8086&DEV_2614.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2614
%PCI\VEN_8086&DEV_2615.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2615
%PCI\VEN_8086&DEV_2617.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2617
%PCI\VEN_8086&DEV_2618.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2618
%PCI\VEN_8086&DEV_2619.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2619
%PCI\VEN_8086&DEV_261A.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_261A
%PCI\VEN_8086&DEV_261B.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_261B
%PCI\VEN_8086&DEV_261C.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_261C
%PCI\VEN_8086&DEV_261D.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_261D
%PCI\VEN_8086&DEV_261E.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_261E
%PCI\VEN_8086&DEV_2620.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2620
%PCI\VEN_8086&DEV_2621.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2621
%PCI\VEN_8086&DEV_2622.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2622
%PCI\VEN_8086&DEV_2623.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2623
%PCI\VEN_8086&DEV_2624.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2624
%PCI\VEN_8086&DEV_2625.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2625
%PCI\VEN_8086&DEV_2626.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2626
%PCI\VEN_8086&DEV_2627.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2627
%PCI\VEN_8086&DEV_2640.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_2640
%PCI\VEN_8086&DEV_2641.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_2641
%PCI\VEN_8086&DEV_2642.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_2642
%PCI\VEN_8086&DEV_2660.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2660
%PCI\VEN_8086&DEV_2662.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2662
%PCI\VEN_8086&DEV_2664.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2664
%PCI\VEN_8086&DEV_2666.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2666
%PCI\VEN_8086&DEV_266A.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_266A
%PCI\VEN_8086&DEV_2670.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_2670
%PCI\VEN_8086&DEV_2690.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2690
%PCI\VEN_8086&DEV_2692.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2692
%PCI\VEN_8086&DEV_2694.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2694
%PCI\VEN_8086&DEV_2696.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2696
%PCI\VEN_8086&DEV_269B.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_269B
%PCI\VEN_8086&DEV_2770.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2770
%PCI\VEN_8086&DEV_2771.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2771
%PCI\VEN_8086&DEV_2774.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2774
%PCI\VEN_8086&DEV_2775.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2775
%PCI\VEN_8086&DEV_2778.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2778
%PCI\VEN_8086&DEV_2779.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2779
%PCI\VEN_8086&DEV_277C.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_277C
%PCI\VEN_8086&DEV_277A.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_277A
%PCI\VEN_8086&DEV_277D.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_277D
%PCI\VEN_8086&DEV_27A0.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_27A0
%PCI\VEN_8086&DEV_27A1.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_27A1
%PCI\VEN_8086&DEV_27AC.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_27AC
%PCI\VEN_8086&DEV_27AD.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_27AD
%PCI\VEN_8086&DEV_27B0.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_27B0
%PCI\VEN_8086&DEV_27B8.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_27B8
%PCI\VEN_8086&DEV_27B9.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_27B9
%PCI\VEN_8086&DEV_27BC.DeviceDesc%         = MSISADRV,PCI\VEN_8086&DEV_27BC
%PCI\VEN_8086&DEV_27BD.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_27BD
%PCI\VEN_8086&DEV_27DA.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_27DA
%PCI\VEN_8086&DEV_27D0.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_27D0
%PCI\VEN_8086&DEV_27D2.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_27D2
%PCI\VEN_8086&DEV_27D4.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_27D4
%PCI\VEN_8086&DEV_27D6.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_27D6
%PCI\VEN_8086&DEV_27E0.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_27E0
%PCI\VEN_8086&DEV_27E2.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_27E2
%PCI\VEN_8086&DEV_2810.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_2810
%PCI\VEN_8086&DEV_2811.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_2811
%PCI\VEN_8086&DEV_2812.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_2812
%PCI\VEN_8086&DEV_2814.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_2814
%PCI\VEN_8086&DEV_2815.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_2815
%PCI\VEN_8086&DEV_283E.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_283E
%PCI\VEN_8086&DEV_283F.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_283F
%PCI\VEN_8086&DEV_2841.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2841
%PCI\VEN_8086&DEV_2843.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2843
%PCI\VEN_8086&DEV_2845.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2845
%PCI\VEN_8086&DEV_2847.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2847
%PCI\VEN_8086&DEV_2849.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2849
%PCI\VEN_8086&DEV_284F.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_284F
%PCI\VEN_8086&DEV_2910.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_2910
%PCI\VEN_8086&DEV_2911.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_2911
%PCI\VEN_8086&DEV_2912.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_2912
%PCI\VEN_8086&DEV_2914.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_2914
%PCI\VEN_8086&DEV_2916.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_2916
%PCI\VEN_8086&DEV_2917.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_2917
%PCI\VEN_8086&DEV_2918.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_2918
%PCI\VEN_8086&DEV_2919.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_2919
%PCI\VEN_8086&DEV_2930.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2930
%PCI\VEN_8086&DEV_2932.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2932
%PCI\VEN_8086&DEV_2940.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2940
%PCI\VEN_8086&DEV_2942.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2942
%PCI\VEN_8086&DEV_2944.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2944
%PCI\VEN_8086&DEV_2946.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2946
%PCI\VEN_8086&DEV_2948.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2948
%PCI\VEN_8086&DEV_294A.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_294A
%PCI\VEN_8086&DEV_2970.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2970
%PCI\VEN_8086&DEV_2971.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2971
%PCI\VEN_8086&DEV_2980.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2980
%PCI\VEN_8086&DEV_2981.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_2981
%PCI\VEN_8086&DEV_2990.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2990
%PCI\VEN_8086&DEV_2991.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2991
%PCI\VEN_8086&DEV_29A0.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_29A0
%PCI\VEN_8086&DEV_29A1.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_29A1
%PCI\VEN_8086&DEV_29B0.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_29B0
%PCI\VEN_8086&DEV_29B1.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_29B1
%PCI\VEN_8086&DEV_29C0.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_29C0
%PCI\VEN_8086&DEV_29C1.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_29C1
%PCI\VEN_8086&DEV_29D0.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_29D0
%PCI\VEN_8086&DEV_29D1.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_29D1
%PCI\VEN_8086&DEV_29E0.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_29E0
%PCI\VEN_8086&DEV_29E1.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_29E1
%PCI\VEN_8086&DEV_29E9.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_29E9
%PCI\VEN_8086&DEV_29F0.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_29F0
%PCI\VEN_8086&DEV_29F1.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_29F1
%PCI\VEN_8086&DEV_29F9.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_29F9
%PCI\VEN_8086&DEV_2A00.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2A00
%PCI\VEN_8086&DEV_2A01.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2A01
%PCI\VEN_8086&DEV_2A09.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2A09
%PCI\VEN_8086&DEV_2A10.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2A10
%PCI\VEN_8086&DEV_2A11.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2A11
%PCI\VEN_8086&DEV_2A19.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2A19
%PCI\VEN_8086&DEV_2A29.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2A29
%PCI\VEN_8086&DEV_2A39.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2A39
%PCI\VEN_8086&DEV_2A40.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2A40
%PCI\VEN_8086&DEV_2A41.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2A41
%PCI\VEN_8086&DEV_2A49.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2A49
%PCI\VEN_8086&DEV_2A59.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2A59
%PCI\VEN_8086&DEV_2A69.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2A69
%PCI\VEN_8086&DEV_2A79.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2A79
%PCI\VEN_8086&DEV_2A89.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2A89
%PCI\VEN_8086&DEV_2A99.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2A99
%PCI\VEN_8086&DEV_2AA9.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2AA9
%PCI\VEN_8086&DEV_2AB9.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2AB9
%PCI\VEN_8086&DEV_2AC9.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2AC9
%PCI\VEN_8086&DEV_2AD9.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2AD9
%PCI\VEN_8086&DEV_2AE9.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2AE9
%PCI\VEN_8086&DEV_2AF9.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2AF9
%PCI\VEN_8086&DEV_2B00.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B00
%PCI\VEN_8086&DEV_2B02.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B02
%PCI\VEN_8086&DEV_2B68.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B68
%PCI\VEN_8086&DEV_2B6A.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B6A
%PCI\VEN_8086&DEV_2B04.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B04
%PCI\VEN_8086&DEV_2B08.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B08
%PCI\VEN_8086&DEV_2B0C.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B0C
%PCI\VEN_8086&DEV_2B10.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B10
%PCI\VEN_8086&DEV_2B14.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B14
%PCI\VEN_8086&DEV_2B16.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B16
%PCI\VEN_8086&DEV_2B13.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B13
%PCI\VEN_8086&DEV_2B18.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B18
%PCI\VEN_8086&DEV_2B1C.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B1C
%PCI\VEN_8086&DEV_2B1E.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B1E
%PCI\VEN_8086&DEV_2B1B.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B1B
%PCI\VEN_8086&DEV_2B20.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B20
%PCI\VEN_8086&DEV_2B24.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B24
%PCI\VEN_8086&DEV_2B28.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B28
%PCI\VEN_8086&DEV_2B2C.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B2C
%PCI\VEN_8086&DEV_2B30.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B30
%PCI\VEN_8086&DEV_2B34.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B34
%PCI\VEN_8086&DEV_2B38.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B38
%PCI\VEN_8086&DEV_2B3C.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B3C
%PCI\VEN_8086&DEV_2B40.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B40
%PCI\VEN_8086&DEV_2B42.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B42
%PCI\VEN_8086&DEV_2B44.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B44
%PCI\VEN_8086&DEV_2B46.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B46
%PCI\VEN_8086&DEV_2B48.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B48
%PCI\VEN_8086&DEV_2B4C.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B4C
%PCI\VEN_8086&DEV_2B50.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B50
%PCI\VEN_8086&DEV_2B52.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B52
%PCI\VEN_8086&DEV_2B54.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B54
%PCI\VEN_8086&DEV_2B56.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B56
%PCI\VEN_8086&DEV_2B58.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B58
%PCI\VEN_8086&DEV_2B5A.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B5A
%PCI\VEN_8086&DEV_2B5C.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B5C
%PCI\VEN_8086&DEV_2B5E.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B5E
%PCI\VEN_8086&DEV_2B60.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B60
%PCI\VEN_8086&DEV_2B62.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B62
%PCI\VEN_8086&DEV_2B64.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B64
%PCI\VEN_8086&DEV_2B66.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2B66
%PCI\VEN_8086&DEV_2C01.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C01
%PCI\VEN_8086&DEV_2C10.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C10
%PCI\VEN_8086&DEV_2C11.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C11
%PCI\VEN_8086&DEV_2C14.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C14
%PCI\VEN_8086&DEV_2C15.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C15
%PCI\VEN_8086&DEV_2C18.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C18
%PCI\VEN_8086&DEV_2C19.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C19
%PCI\VEN_8086&DEV_2C1A.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C1A
%PCI\VEN_8086&DEV_2C1C.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C1C
%PCI\VEN_8086&DEV_2C20.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C20
%PCI\VEN_8086&DEV_2C21.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C21
%PCI\VEN_8086&DEV_2C22.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C22
%PCI\VEN_8086&DEV_2C23.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C23
%PCI\VEN_8086&DEV_2C28.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C28
%PCI\VEN_8086&DEV_2C29.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C29
%PCI\VEN_8086&DEV_2C2A.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C2A
%PCI\VEN_8086&DEV_2C2B.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C2B
%PCI\VEN_8086&DEV_2C30.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C30
%PCI\VEN_8086&DEV_2C31.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C31
%PCI\VEN_8086&DEV_2C32.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C32
%PCI\VEN_8086&DEV_2C33.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C33
%PCI\VEN_8086&DEV_2C40.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C40
%PCI\VEN_8086&DEV_2C41.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C41
%PCI\VEN_8086&DEV_2C50.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C50
%PCI\VEN_8086&DEV_2C51.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C51
%PCI\VEN_8086&DEV_2C52.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C52
%PCI\VEN_8086&DEV_2C53.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C53
%PCI\VEN_8086&DEV_2C54.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C54
%PCI\VEN_8086&DEV_2C55.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C55
%PCI\VEN_8086&DEV_2C56.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C56
%PCI\VEN_8086&DEV_2C57.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C57
%PCI\VEN_8086&DEV_2C81.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C81
%PCI\VEN_8086&DEV_2C90.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C90
%PCI\VEN_8086&DEV_2C91.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C91
%PCI\VEN_8086&DEV_2C98.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C98
%PCI\VEN_8086&DEV_2C99.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C99
%PCI\VEN_8086&DEV_2C9C.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2C9C
%PCI\VEN_8086&DEV_2CA0.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2CA0
%PCI\VEN_8086&DEV_2CA1.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2CA1
%PCI\VEN_8086&DEV_2CA2.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2CA2
%PCI\VEN_8086&DEV_2CA3.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2CA3
%PCI\VEN_8086&DEV_2CA8.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2CA8
%PCI\VEN_8086&DEV_2CA9.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2CA9
%PCI\VEN_8086&DEV_2CAA.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2CAA
%PCI\VEN_8086&DEV_2CAB.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2CAB
%PCI\VEN_8086&DEV_2E00.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2E00
%PCI\VEN_8086&DEV_2E01.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2E01
%PCI\VEN_8086&DEV_2E08.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2E08
%PCI\VEN_8086&DEV_2E09.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2E09
%PCI\VEN_8086&DEV_2E10.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2E10
%PCI\VEN_8086&DEV_2E11.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2E11
%PCI\VEN_8086&DEV_2E18.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2E18
%PCI\VEN_8086&DEV_2E19.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2E19
%PCI\VEN_8086&DEV_2E20.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2E20
%PCI\VEN_8086&DEV_2E21.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2E21
%PCI\VEN_8086&DEV_2E28.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2E28
%PCI\VEN_8086&DEV_2E29.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2E29
%PCI\VEN_8086&DEV_2E30.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2E30
%PCI\VEN_8086&DEV_2E31.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2E31
%PCI\VEN_8086&DEV_2E38.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2E38
%PCI\VEN_8086&DEV_2E40.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2E40
%PCI\VEN_8086&DEV_2E41.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2E41
%PCI\VEN_8086&DEV_2E48.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2E48
%PCI\VEN_8086&DEV_2E58.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2E58
%PCI\VEN_8086&DEV_2E68.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2E68
%PCI\VEN_8086&DEV_2E78.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2E78
%PCI\VEN_8086&DEV_2E88.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2E88
%PCI\VEN_8086&DEV_2E90.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_2E90
%PCI\VEN_8086&DEV_2E91.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_2E91
%PCI\VEN_8086&DEV_2E98.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2E98
%PCI\VEN_8086&DEV_2EA8.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2EA8
%PCI\VEN_8086&DEV_2EB8.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2EB8
%PCI\VEN_8086&DEV_2EC8.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2EC8
%PCI\VEN_8086&DEV_2ED8.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2ED8
%PCI\VEN_8086&DEV_2EE8.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2EE8
%PCI\VEN_8086&DEV_2EF8.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_2EF8
%PCI\VEN_8086&DEV_3340.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3340
%PCI\VEN_8086&DEV_3341.DeviceDesc%   = AGP440_Install,PCI\VEN_8086&DEV_3341
%PCI\VEN_8086&DEV_3400.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3400
%PCI\VEN_8086&DEV_3401.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3401
%PCI\VEN_8086&DEV_3402.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3402
%PCI\VEN_8086&DEV_3403.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3403
%PCI\VEN_8086&DEV_3404.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3404
%PCI\VEN_8086&DEV_3405.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3405
%PCI\VEN_8086&DEV_3406.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3406
%PCI\VEN_8086&DEV_3407.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3407
%PCI\VEN_8086&DEV_3408.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3408
%PCI\VEN_8086&DEV_3409.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3409
%PCI\VEN_8086&DEV_340A.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_340A
%PCI\VEN_8086&DEV_340B.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_340B
%PCI\VEN_8086&DEV_340C.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_340C
%PCI\VEN_8086&DEV_340D.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_340D
%PCI\VEN_8086&DEV_340E.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_340E
%PCI\VEN_8086&DEV_340F.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_340F
%PCI\VEN_8086&DEV_3410.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3410
%PCI\VEN_8086&DEV_3411.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3411
%PCI\VEN_8086&DEV_3418.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3418
%PCI\VEN_8086&DEV_3419.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3419
%PCI\VEN_8086&DEV_3420.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3420
%PCI\VEN_8086&DEV_3421.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3421
%PCI\VEN_8086&DEV_3422.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3422
%PCI\VEN_8086&DEV_3423.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3423
%PCI\VEN_8086&DEV_3424.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3424
%PCI\VEN_8086&DEV_3425.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3425
%PCI\VEN_8086&DEV_3426.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3426
%PCI\VEN_8086&DEV_3427.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3427
%PCI\VEN_8086&DEV_3428.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3428
%PCI\VEN_8086&DEV_3429.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_3429
%PCI\VEN_8086&DEV_342A.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_342A
%PCI\VEN_8086&DEV_342B.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_342B
%PCI\VEN_8086&DEV_342C.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_342C
%PCI\VEN_8086&DEV_342D.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_342D
%PCI\VEN_8086&DEV_342E.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_342E
%PCI\VEN_8086&DEV_342F.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_342F
%PCI\VEN_8086&DEV_3430.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_3430
%PCI\VEN_8086&DEV_3431.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_3431
%PCI\VEN_8086&DEV_3432.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_3432
%PCI\VEN_8086&DEV_3433.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_3433
%PCI\VEN_8086&DEV_3438.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3438
%PCI\VEN_8086&DEV_3500.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3500
%PCI\VEN_8086&DEV_3501.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3501
%PCI\VEN_8086&DEV_3504.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3504
%PCI\VEN_8086&DEV_3505.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3505
%PCI\VEN_8086&DEV_350C.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_350C
%PCI\VEN_8086&DEV_350D.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_350D
%PCI\VEN_8086&DEV_3510.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3510
%PCI\VEN_8086&DEV_3511.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3511
%PCI\VEN_8086&DEV_3514.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3514
%PCI\VEN_8086&DEV_3515.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3515
%PCI\VEN_8086&DEV_3518.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3518
%PCI\VEN_8086&DEV_3519.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3519
%PCI\VEN_8086&DEV_3575.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_3575      ;Intel 82830
%PCI\VEN_8086&DEV_3576.DeviceDesc%         = AGP440_Install,PCI\VEN_8086&DEV_3576      ; 82830-3576
%PCI\VEN_8086&DEV_3578.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_3578      ;Intel 82830
%PCI\VEN_8086&DEV_3580.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3580
%PCI\VEN_8086&DEV_3581.DeviceDesc%   = AGP440_Install, PCI\VEN_8086&DEV_3581       ; 82852/82855 GM/GME/PM Processor to AGP Controller
%PCI\VEN_8086&DEV_3584.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3584
%PCI\VEN_8086&DEV_3585.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3585
%PCI\VEN_8086&DEV_3590.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3590               ;PHX
%PCI\VEN_8086&DEV_3591.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3591
%PCI\VEN_8086&DEV_3592.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3592
%PCI\VEN_8086&DEV_3593.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3593
%PCI\VEN_8086&DEV_3594.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3594
%PCI\VEN_8086&DEV_3595.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3595
%PCI\VEN_8086&DEV_3596.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3596
%PCI\VEN_8086&DEV_3597.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3597
%PCI\VEN_8086&DEV_3598.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3598
%PCI\VEN_8086&DEV_3599.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3599
%PCI\VEN_8086&DEV_359A.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_359A
%PCI\VEN_8086&DEV_359B.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_359B
%PCI\VEN_8086&DEV_359E.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_359E               ;PHX
%PCI\VEN_8086&DEV_35B0.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_35B0
%PCI\VEN_8086&DEV_35B1.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_35B1
%PCI\VEN_8086&DEV_35B5.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_35B5
%PCI\VEN_8086&DEV_35B6.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_35B6
%PCI\VEN_8086&DEV_35B7.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_35B7
%PCI\VEN_8086&DEV_35C8.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_35C8

%PCI\VEN_8086&DEV_3600.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3600
%PCI\VEN_8086&DEV_3604.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3604
%PCI\VEN_8086&DEV_3605.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3605
%PCI\VEN_8086&DEV_3606.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3606
%PCI\VEN_8086&DEV_3607.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3607
%PCI\VEN_8086&DEV_3608.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3608
%PCI\VEN_8086&DEV_3609.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_3609
%PCI\VEN_8086&DEV_360A.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_360A
%PCI\VEN_8086&DEV_360B.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_360B
%PCI\VEN_8086&DEV_360C.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_360C
%PCI\VEN_8086&DEV_360D.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_360D
%PCI\VEN_8086&DEV_360E.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_360E
%PCI\VEN_8086&DEV_360F.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_360F
%PCI\VEN_8086&DEV_3610.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_3610
%PCI\VEN_8086&DEV_3A10.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3A10
%PCI\VEN_8086&DEV_3A14.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3A14
%PCI\VEN_8086&DEV_3A16.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3A16
%PCI\VEN_8086&DEV_3A18.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3A18
%PCI\VEN_8086&DEV_3A1A.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3A1A
%PCI\VEN_8086&DEV_3A1E.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3A1E
%PCI\VEN_8086&DEV_3A30.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_3A30
%PCI\VEN_8086&DEV_3A32.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_3A32
%PCI\VEN_8086&DEV_3A40.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_3A40
%PCI\VEN_8086&DEV_3A42.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_3A42
%PCI\VEN_8086&DEV_3A44.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_3A44
%PCI\VEN_8086&DEV_3A46.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_3A46
%PCI\VEN_8086&DEV_3A48.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_3A48
%PCI\VEN_8086&DEV_3A4A.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_3A4A
%PCI\VEN_8086&DEV_3A51.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_3A51
%PCI\VEN_8086&DEV_3A60.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_3A60
%PCI\VEN_8086&DEV_3A62.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_3A62
%PCI\VEN_8086&DEV_3A70.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_3A70
%PCI\VEN_8086&DEV_3A72.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_3A72
%PCI\VEN_8086&DEV_3A74.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_3A74
%PCI\VEN_8086&DEV_3A76.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_3A76
%PCI\VEN_8086&DEV_3A78.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_3A78
%PCI\VEN_8086&DEV_3A7A.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_3A7A
%PCI\VEN_8086&DEV_3B00.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B00     
%PCI\VEN_8086&DEV_3B01.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B01 
%PCI\VEN_8086&DEV_3B02.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B02     
%PCI\VEN_8086&DEV_3B03.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B03 
%PCI\VEN_8086&DEV_3B04.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B04     
%PCI\VEN_8086&DEV_3B05.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B05 
%PCI\VEN_8086&DEV_3B06.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B06     
%PCI\VEN_8086&DEV_3B07.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B07 
%PCI\VEN_8086&DEV_3B08.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B08     
%PCI\VEN_8086&DEV_3B09.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B09 
%PCI\VEN_8086&DEV_3B0A.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B0A     
%PCI\VEN_8086&DEV_3B0B.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B0B 
%PCI\VEN_8086&DEV_3B0C.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B0C     
%PCI\VEN_8086&DEV_3B0D.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B0D 
%PCI\VEN_8086&DEV_3B0E.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B0E     
%PCI\VEN_8086&DEV_3B0F.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B0F 
%PCI\VEN_8086&DEV_3B10.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B10     
%PCI\VEN_8086&DEV_3B11.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B11 
%PCI\VEN_8086&DEV_3B12.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B12     
%PCI\VEN_8086&DEV_3B13.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B13 
%PCI\VEN_8086&DEV_3B14.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B14     
%PCI\VEN_8086&DEV_3B15.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B15 
%PCI\VEN_8086&DEV_3B16.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B16     
%PCI\VEN_8086&DEV_3B17.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B17 
%PCI\VEN_8086&DEV_3B18.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B18     
%PCI\VEN_8086&DEV_3B19.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B19 
%PCI\VEN_8086&DEV_3B1A.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B1A     
%PCI\VEN_8086&DEV_3B1B.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B1B 
%PCI\VEN_8086&DEV_3B1C.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B1C     
%PCI\VEN_8086&DEV_3B1D.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B1D 
%PCI\VEN_8086&DEV_3B1E.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B1E     
%PCI\VEN_8086&DEV_3B1F.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_3B1F
%PCI\VEN_8086&DEV_3B30.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_3B30
%PCI\VEN_8086&DEV_3B32.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_3B32
%PCI\VEN_8086&DEV_3B53.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_3B53
%PCI\VEN_8086&DEV_3B42.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_3B42
%PCI\VEN_8086&DEV_3B44.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_3B44
%PCI\VEN_8086&DEV_3B46.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_3B46
%PCI\VEN_8086&DEV_3B48.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_3B48
%PCI\VEN_8086&DEV_3B4A.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_3B4A
%PCI\VEN_8086&DEV_3B4C.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_3B4C
%PCI\VEN_8086&DEV_3B4E.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_3B4E
%PCI\VEN_8086&DEV_3B50.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_3B50
%PCI\VEN_8086&DEV_4000.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_4000
%PCI\VEN_8086&DEV_4001.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_4001
%PCI\VEN_8086&DEV_4003.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_4003
%PCI\VEN_8086&DEV_4021.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_4021
%PCI\VEN_8086&DEV_4022.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_4022
%PCI\VEN_8086&DEV_4023.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_4023
%PCI\VEN_8086&DEV_4024.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_4024
%PCI\VEN_8086&DEV_4025.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_4025
%PCI\VEN_8086&DEV_4026.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_4026
%PCI\VEN_8086&DEV_4027.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_4027
%PCI\VEN_8086&DEV_4028.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_4028
%PCI\VEN_8086&DEV_4029.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_4029
%PCI\VEN_8086&DEV_402D.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_402D
%PCI\VEN_8086&DEV_402E.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_402E
%PCI\VEN_8086&DEV_4030.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_4030
%PCI\VEN_8086&DEV_4031.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_4031
%PCI\VEN_8086&DEV_4032.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_4032
%PCI\VEN_8086&DEV_4035.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_4035
%PCI\VEN_8086&DEV_4036.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_4036
%PCI\VEN_8086&DEV_537C.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_537C
%PCI\VEN_8086&DEV_65C0.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_65C0
%PCI\VEN_8086&DEV_65E2.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_65E2
%PCI\VEN_8086&DEV_65E3.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_65E3
%PCI\VEN_8086&DEV_65E4.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_65E4
%PCI\VEN_8086&DEV_65E5.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_65E5
%PCI\VEN_8086&DEV_65E6.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_65E6
%PCI\VEN_8086&DEV_65E7.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_65E7
%PCI\VEN_8086&DEV_65F0.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_65F0
%PCI\VEN_8086&DEV_65F1.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_65F1
%PCI\VEN_8086&DEV_65F2.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_65F3
%PCI\VEN_8086&DEV_65F5.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_65F5
%PCI\VEN_8086&DEV_65F6.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_65F6
%PCI\VEN_8086&DEV_65F7.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_65F7
%PCI\VEN_8086&DEV_65F8.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_65F8
%PCI\VEN_8086&DEV_65F9.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_65F9
%PCI\VEN_8086&DEV_65FA.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_65FA
%PCI\VEN_8086&DEV_65FF.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_65FF
%PCI\VEN_8086&DEV_7000.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_7000            ; INTEL PCI-ISA bridge
%PCI\VEN_8086&DEV_7030.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_7030
%PCI\VEN_8086&DEV_7100.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_7100
%PCI\VEN_8086&DEV_7110_EIO.DeviceDesc%     = MSISADRV, PCI\VEN_8086&DEV_7110&CC_0680 ; INTEL PIIX4 PCI-ISA bridge (EIO mode)
%PCI\VEN_8086&DEV_7110_ISA.DeviceDesc%     = MSISADRV, PCI\VEN_8086&DEV_7110&CC_0601 ; INTEL PIIX4 PCI-ISA bridge (ISA mode)
%PCI\VEN_8086&DEV_7110_OLD_EIO.DeviceDesc% = MSISADRV, PCI\VEN_8086&DEV_7110&REV_01&CC_0680
%PCI\VEN_8086&DEV_7110_OLD_ISA.DeviceDesc% = MSISADRV, PCI\VEN_8086&DEV_7110&REV_01&CC_0601
%PCI\VEN_8086&DEV_7113_OLD.DeviceDesc%     = NO_DRV, PCI\VEN_8086&DEV_7113&REV_00
%PCI\VEN_8086&DEV_7113_OLD.DeviceDesc%     = NO_DRV, PCI\VEN_8086&DEV_7113&REV_01
%PCI\VEN_8086&DEV_7113.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_7113
%PCI\VEN_8086&DEV_7120.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_7120
%PCI\VEN_8086&DEV_7122.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_7122
%PCI\VEN_8086&DEV_7124.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_7124             ; 82810E-7124
%PCI\VEN_8086&DEV_7180.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_7180
%PCI\VEN_8086&DEV_7181.DeviceDesc%         = AGP440_Install,PCI\VEN_8086&DEV_7181        ; 440LX
%PCI\VEN_8086&DEV_7190.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_7190
%PCI\VEN_8086&DEV_7191.DeviceDesc%         = AGP440_Install,PCI\VEN_8086&DEV_7191        ; 440BX
%PCI\VEN_8086&DEV_7192.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_7192
%PCI\VEN_8086&DEV_7194.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_7194
%PCI\VEN_8086&DEV_7198.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_7198
%PCI\VEN_8086&DEV_719B.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_719B
%PCI\VEN_8086&DEV_71A1.DeviceDesc%         = AGP440_Install,PCI\VEN_8086&DEV_71A1        ; 440GX
%PCI\VEN_8086&DEV_7600.DeviceDesc%         = MSISADRV, PCI\VEN_8086&DEV_7600            ; INTEL PCI-ISA bridge
%PCI\VEN_8086&DEV_7603.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_7603
%PCI\VEN_8086&DEV_8002.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_8002
%PCI\VEN_8086&DEV_84C4.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_84C4
%PCI\VEN_8086&DEV_84C5.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_84C5
%PCI\VEN_8086&DEV_A000.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_A000
%PCI\VEN_8086&DEV_A010.DeviceDesc%         = NO_DRV, PCI\VEN_8086&DEV_A010
%PCI\VEN_8086&DEV_B152.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_B152     ;Intel 21152 PCI to PCI bridge
%PCI\VEN_8086&DEV_B154.DeviceDesc%         = PCI_DRV, PCI\VEN_8086&DEV_B154     ;Intel 21154 PCI to PCI bridge
%PCI\VEN_8086&DEV_B555&SUBSYS_B555119F.DeviceDesc% = NO_DRV,PCI\VEN_8086&DEV_B555&SUBSYS_B555119F
%PCI\VEN_8086&DEV_D130.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_D130
%PCI\VEN_8086&DEV_D131.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_D131
%PCI\VEN_8086&DEV_D132.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_D132
%PCI\VEN_8086&DEV_D133.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_D133
%PCI\VEN_8086&DEV_D134.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_D134
%PCI\VEN_8086&DEV_D135.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_D135
%PCI\VEN_8086&DEV_D136.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_D136
%PCI\VEN_8086&DEV_D137.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_D137
%PCI\VEN_8086&DEV_D138.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_D138
%PCI\VEN_8086&DEV_D139.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_D139
%PCI\VEN_8086&DEV_D13A.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_D13A
%PCI\VEN_8086&DEV_D13B.DeviceDesc%         = PCI_DRV,PCI\VEN_8086&DEV_D13B
%PCI\VEN_8086&DEV_D150.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_D150
%PCI\VEN_8086&DEV_D151.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_D151
%PCI\VEN_8086&DEV_D155.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_D155
%PCI\VEN_8086&DEV_D156.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_D156
%PCI\VEN_8086&DEV_D157.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_D157
%PCI\VEN_8086&DEV_D158.DeviceDesc%         = NO_DRV,PCI\VEN_8086&DEV_D158

[MICRON_SYS.NTx86]
%PCI\VEN_1042&DEV_3000.DeviceDesc% = NO_DRV, PCI\VEN_1042&DEV_3000
%PCI\VEN_1042&DEV_3010.DeviceDesc% = NO_DRV, PCI\VEN_1042&DEV_3010

[NATSEMI_SYS.NTx86]
%PCI\VEN_1066&DEV_0001.DeviceDesc% = NO_DRV, PCI\VEN_1066&DEV_0001
%PCI\VEN_1066&DEV_8002.DeviceDesc% = MSISADRV, PCI\VEN_1066&DEV_8002
%PCI\VEN_1066&DEV_0002.DeviceDesc% = MSISADRV, PCI\VEN_1066&DEV_0002
%PCI\VEN_100B&DEV_0011.DeviceDesc% = MSISADRV, PCI\VEN_100B&DEV_0011

[NEC_SYS.NTx86]
%PCI\VEN_1033&DEV_00A8&CC_0600.DeviceDesc% = NO_DRV, PCI\VEN_1033&DEV_00A8&CC_0600
%PCI\VEN_1033&DEV_00A8&CC_0000.DeviceDesc% = NO_DRV, PCI\VEN_1033&DEV_00A8&CC_0000
%PCI\VEN_1033&DEV_00A9&CC_0600.DeviceDesc% = NO_DRV, PCI\VEN_1033&DEV_00A9&CC_0600
%PCI\VEN_1033&DEV_00AA&CC_0500.DeviceDesc% = NO_DRV, PCI\VEN_1033&DEV_00AA&CC_0500
%PCI\VEN_1033&DEV_00AB.DeviceDesc% = NO_DRV, PCI\VEN_1033&DEV_00AB&SUBSYS_00AB1033
%PCI\VEN_1033&DEV_00AC&CC_0600.DeviceDesc% = NO_DRV, PCI\VEN_1033&DEV_00AC&CC_0600
%PCI\VEN_1033&DEV_00AD&CC_0600.DeviceDesc% = NO_DRV, PCI\VEN_1033&DEV_00AD&CC_0600
%PCI\VEN_1033&DEV_00AE&CC_0600.DeviceDesc% = NO_DRV, PCI\VEN_1033&DEV_00AE&CC_0600
%PCI\VEN_1033&DEV_00AF.DeviceDesc% = NO_DRV, PCI\VEN_1033&DEV_00AF
%PCI\VEN_1033&DEV_00B0.DeviceDesc% = NO_DRV, PCI\VEN_1033&DEV_00B0
%PCI\VEN_1033&DEV_00B1&CC_0600.DeviceDesc% = NO_DRV, PCI\VEN_1033&DEV_00B1&CC_0600

[NVIDIA_SYS.NTx86]
%PCI\VEN_10DE&DEV_005E.DeviceDesc% = NO_DRV, PCI\VEN_10DE&DEV_005E
%PCI\VEN_10DE&DEV_00D2.DeviceDesc% = NVIDIAAGP_Install,PCI\VEN_10DE&DEV_00D2
%PCI\VEN_10DE&DEV_00D3.DeviceDesc% = NO_DRV, PCI\VEN_10DE&DEV_00D3
%PCI\VEN_10DE&DEV_00E4.DeviceDesc% = NO_DRV, PCI\VEN_10DE&DEV_00E4
%PCI\VEN_10DE&DEV_0052.DeviceDesc% = NO_DRV, PCI\VEN_10DE&DEV_0052
%PCI\VEN_10DE&DEV_0084.DeviceDesc% = NO_DRV, PCI\VEN_10DE&DEV_0084
%PCI\VEN_10DE&DEV_00D4.DeviceDesc% = NO_DRV, PCI\VEN_10DE&DEV_00D4
%PCI\VEN_10DE&DEV_0264.DeviceDesc% = NO_DRV, PCI\VEN_10DE&DEV_0264
%PCI\VEN_10DE&DEV_0368.DeviceDesc% = NO_DRV, PCI\VEN_10DE&DEV_0368
%PCI\VEN_10DE&DEV_03EB.DeviceDesc% = NO_DRV, PCI\VEN_10DE&DEV_03EB
%PCI\VEN_10DE&DEV_00E2.DeviceDesc% = NVIDIAAGP_Install,PCI\VEN_10DE&DEV_00E2
%PCI\VEN_10DE&DEV_01B7.DeviceDesc%   = NVIDIAAGP_Install,PCI\VEN_10DE&DEV_01B7
%PCI\VEN_10DE&DEV_01E8.DeviceDesc%   = NVIDIAAGP_Install,PCI\VEN_10DE&DEV_01E8
%PCI\VEN_10DE&DEV_0446.DeviceDesc% = NO_DRV, PCI\VEN_10DE&DEV_0446
%PCI\VEN_10DE&DEV_0542.DeviceDesc% = NO_DRV, PCI\VEN_10DE&DEV_0542
%PCI\VEN_10DE&DEV_07D8.DeviceDesc% = NO_DRV, PCI\VEN_10DE&DEV_07D8
%PCI\VEN_10DE&DEV_0752.DeviceDesc% = NO_DRV, PCI\VEN_10DE&DEV_0752
%PCI\VEN_10DE&DEV_0AA2.DeviceDesc% = NO_DRV, PCI\VEN_10DE&DEV_0AA2


[OPTI_SYS.NTx86]
%PCI\VEN_1045&DEV_C822.DeviceDesc% = MSISADRV, PCI\VEN_1045&DEV_C822
%PCI\VEN_1045&DEV_C832.DeviceDesc% = MSISADRV, PCI\VEN_1045&DEV_C832
%PCI\VEN_1045&DEV_C557.DeviceDesc% = NO_DRV, PCI\VEN_1045&DEV_C557
%PCI\VEN_1045&DEV_C558.DeviceDesc% = MSISADRV, PCI\VEN_1045&DEV_C558
%PCI\VEN_1045&DEV_C567.DeviceDesc% = NO_DRV, PCI\VEN_1045&DEV_C567
%PCI\VEN_1045&DEV_C568.DeviceDesc% = MSISADRV, PCI\VEN_1045&DEV_C568
%PCI\VEN_1045&DEV_C700.DeviceDesc% = MSISADRV, PCI\VEN_1045&DEV_C700
%PCI\VEN_1045&DEV_C701.DeviceDesc% = NO_DRV, PCI\VEN_1045&DEV_C701

[SERVERWORKS_SYS.NTx86]
%PCI\VEN_1166&DEV_0005&CC_0604.DeviceDesc% = NO_DRV, PCI\VEN_1166&DEV_0005&CC_0604
%PCI\VEN_1166&DEV_0005&CC_0600.DeviceDesc%       = NO_DRV, PCI\VEN_1166&DEV_0005&CC_0600
%PCI\VEN_1166&DEV_0007.DeviceDesc%               = NO_DRV, PCI\VEN_1166&DEV_0007
%PCI\VEN_1166&DEV_0008.DeviceDesc%               = NO_DRV, PCI\VEN_1166&DEV_0008
%PCI\VEN_1166&DEV_0009&CC_0604.DeviceDesc% = NO_DRV, PCI\VEN_1166&DEV_0009&CC_0604
%PCI\VEN_1166&DEV_0009&CC_0600.DeviceDesc%       = NO_DRV, PCI\VEN_1166&DEV_0009&CC_0600
%PCI\VEN_1166&DEV_0010&CC_0600.DeviceDesc%       = NO_DRV, PCI\VEN_1166&DEV_0010&CC_0600
%PCI\VEN_1166&DEV_0011&CC_0600.DeviceDesc%       = NO_DRV, PCI\VEN_1166&DEV_0011&CC_0600
%PCI\VEN_1166&DEV_0012&CC_0600.DeviceDesc%       = NO_DRV, PCI\VEN_1166&DEV_0012&CC_0600
%PCI\VEN_1166&DEV_0013.DeviceDesc%               = NO_DRV, PCI\VEN_1166&DEV_0013
%PCI\VEN_1166&DEV_0014&CC_0604.DeviceDesc% = NO_DRV, PCI\VEN_1166&DEV_0014&CC_0604
%PCI\VEN_1166&DEV_0014&CC_0600.DeviceDesc%       = NO_DRV, PCI\VEN_1166&DEV_0014&CC_0600
%PCI\VEN_1166&DEV_0015.DeviceDesc%               = NO_DRV, PCI\VEN_1166&DEV_0015
%PCI\VEN_1166&DEV_0016&CC_0604.DeviceDesc% = NO_DRV, PCI\VEN_1166&DEV_0016&CC_0604
%PCI\VEN_1166&DEV_0016&CC_0600.DeviceDesc%       = NO_DRV, PCI\VEN_1166&DEV_0016&CC_0600
%PCI\VEN_1166&DEV_0017&CC_0600.DeviceDesc%       = NO_DRV, PCI\VEN_1166&DEV_0017&CC_0600
%PCI\VEN_1166&DEV_0036&CC_0604.DeviceDesc%       = PCI_DRV, PCI\VEN_1166&DEV_0036&CC_0604
%PCI\VEN_1166&DEV_0101&CC_0600.DeviceDesc%       = NO_DRV, PCI\VEN_1166&DEV_0101&CC_0600
%PCI\VEN_1166&DEV_0104&CC_0604.DeviceDesc%       = PCI_DRV, PCI\VEN_1166&DEV_0104&CC_0604
%PCI\VEN_1166&DEV_0110&CC_0600.DeviceDesc%       = NO_DRV, PCI\VEN_1166&DEV_0110&CC_0600
%PCI\VEN_1166&DEV_0130&CC_0604.DeviceDesc%       = PCI_DRV, PCI\VEN_1166&DEV_0130&CC_0604
%PCI\VEN_1166&DEV_0132&CC_0604.DeviceDesc%       = PCI_DRV, PCI\VEN_1166&DEV_0132&CC_0604
%PCI\VEN_1166&DEV_0140&CC_0604.DeviceDesc%       = PCI_DRV, PCI\VEN_1166&DEV_0140&CC_0604
%PCI\VEN_1166&DEV_0142&CC_0604.DeviceDesc%       = PCI_DRV, PCI\VEN_1166&DEV_0142&CC_0604
%PCI\VEN_1166&DEV_0144&CC_0604.DeviceDesc%       = PCI_DRV, PCI\VEN_1166&DEV_0144&CC_0604
%PCI\VEN_1166&DEV_0200.DeviceDesc%               = MSISADRV, PCI\VEN_1166&DEV_0200
%PCI\VEN_1166&DEV_0201&CC_0600.DeviceDesc%       = NO_DRV, PCI\VEN_1166&DEV_0201&CC_0600
%PCI\VEN_1166&DEV_0203&CC_0600.DeviceDesc%       = NO_DRV, PCI\VEN_1166&DEV_0203&CC_0600
%PCI\VEN_1166&DEV_0205&CC_0600.DeviceDesc%       = NO_DRV, PCI\VEN_1166&DEV_0205&CC_0600
%PCI\VEN_1166&DEV_0214&CC_0108.DeviceDesc%       = NO_DRV, PCI\VEN_1166&DEV_0214&CC_1018
%PCI\VEN_1166&DEV_0225.DeviceDesc%               = MSISADRV, PCI\VEN_1166&DEV_0225
%PCI\VEN_1166&DEV_0227.DeviceDesc%               = MSISADRV, PCI\VEN_1166&DEV_0227
%PCI\VEN_1166&DEV_0230.DeviceDesc%               = NO_DRV, PCI\VEN_1166&DEV_0230
%PCI\VEN_1166&DEV_0234&CC_0601.DeviceDesc%       = MSISADRV, PCI\VEN_1166&DEV_0234&CC_0601


[SIS_SYS.NTx86]
%PCI\VEN_1039&DEV_0001.DeviceDesc% = SISAGP_Install, PCI\VEN_1039&DEV_0001
%PCI\VEN_1039&DEV_0008.DeviceDesc% = MSISADRV, PCI\VEN_1039&DEV_0008
%PCI\VEN_1039&DEV_0009.DeviceDesc% = NO_DRV, PCI\VEN_1039&DEV_0009
%PCI\VEN_1039&DEV_0406.DeviceDesc% = NO_DRV, PCI\VEN_1039&DEV_0406
%PCI\VEN_1039&DEV_0496.DeviceDesc% = MSISADRV, PCI\VEN_1039&DEV_0496
%PCI\VEN_1039&DEV_0540.DeviceDesc% = NO_DRV, PCI\VEN1039&DEV_0540
%PCI\VEN_1039&DEV_0630.DeviceDesc% = NO_DRV, PCI\VEN_1039&DEV_0630
%PCI\VEN_1039&DEV_0635.DeviceDesc% = NO_DRV, PCI\VEN_1039&DEV_0635
%PCI\VEN_1039&DEV_0730.DeviceDesc% = NO_DRV, PCI\VEN_1039&DEV_0730
%PCI\VEN_1039&DEV_0735.DeviceDesc% = NO_DRV, PCI\VEN_1039&DEV_0735
%PCI\VEN_1039&DEV_6001.DeviceDesc% = PCI_DRV, PCI\VEN_1039&DEV_6001
%PCI\VEN_1039&DEV_0755.DeviceDesc% = NO_DRV, PCI\VEN_1039&DEV_0755
%PCI\VEN_1039&DEV_0760.DeviceDesc% = NO_DRV, PCI\VEN_1039&DEV_0760
%PCI\VEN_1039&DEV_0756.DeviceDesc% = NO_DRV, PCI\VEN_1039&DEV_0756
%PCI\VEN_1039&DEV_0761.DeviceDesc% = NO_DRV, PCI\VEN_1039&DEV_0761
%PCI\VEN_1039&DEV_0648.DeviceDesc% = NO_DRV, PCI\VEN_1039&DEV_0648
%PCI\VEN_1039&DEV_0649.DeviceDesc% = NO_DRV, PCI\VEN_1039&DEV_0649
%PCI\VEN_1039&DEV_0655.DeviceDesc% = NO_DRV, PCI\VEN_1039&DEV_0655
%PCI\VEN_1039&DEV_0656.DeviceDesc% = NO_DRV, PCI\VEN_1039&DEV_0656
%PCI\VEN_1039&DEV_0661.DeviceDesc% = NO_DRV, PCI\VEN_1039&DEV_0661
%PCI\VEN_1039&DEV_0963.DeviceDesc% = MSISADRV, PCI\VEN_1039&DEV_0963
%PCI\VEN_1039&DEV_0964.DeviceDesc% = MSISADRV, PCI\VEN_1039&DEV_0964
%PCI\VEN_1039&DEV_0965.DeviceDesc% = MSISADRV, PCI\VEN_1039&DEV_0965
%PCI\VEN_1039&DEV_0966.DeviceDesc% = MSISADRV, PCI\VEN_1039&DEV_0966
%PCI\VEN_1039&DEV_0004.DeviceDesc% = PCI_DRV, PCI\VEN_1039&DEV_0004
%PCI\VEN_1039&DEV_000A.DeviceDesc% = PCI_DRV, PCI\VEN_1039&DEV_000A
%PCI\VEN_1039&DEV_0662.DeviceDesc% = NO_DRV, PCI\VEN_1039&DEV_0662
%PCI\VEN_1039&DEV_0741.DeviceDesc% = NO_DRV, PCI\VEN_1039&DEV_0741

[SMSC_SYS.NTx86]
%PCI\VEN_1055&DEV_9460.DeviceDesc% = MSISADRV,PCI\VEN_1055&DEV_9460
%PCI\VEN_1055&DEV_9463.DeviceDesc% = NO_DRV,PCI\VEN_1055&DEV_9463


[TEXAS_SYS.NTx86]
%PCI\VEN_104C&DEV_AC20.DeviceDesc% = PCI_DRV, PCI\VEN_104C&DEV_AC20

[TOSHIBA_SYS.NTx86]
%PCI\VEN_1179&DEV_0601.DeviceDesc% = MSISADRV, PCI\VEN_1179&DEV_0601    ; Installing msisadrv for host bridge
%PCI\VEN_1179&DEV_0618.DeviceDesc% = MSISADRV, PCI\VEN_1179&DEV_0618    ; Installing msisadrv for host bridge
%PCI\VEN_1179&DEV_0602.DeviceDesc% = MSISADRV, PCI\VEN_1179&DEV_0602
%PCI\VEN_1179&DEV_0603.DeviceDesc% = NO_DRV,PCI\VEN_1179&DEV_0603
%PCI\VEN_1179&DEV_0604.DeviceDesc% = PCI_DRV, PCI\VEN_1179&DEV_0604
%PCI\VEN_1179&DEV_0605.DeviceDesc% = PCI_DRV, PCI\VEN_1179&DEV_0605
%PCI\VEN_1179&DEV_0609.DeviceDesc% = PCI_DRV, PCI\VEN_1179&DEV_0609
%PCI\VEN_1179&DEV_0611.DeviceDesc% = MSISADRV, PCI\VEN_1179&DEV_0611    ; Dock only

[ULI_SYS.NTx86]
%PCI\VEN_10B9&DEV_5246.DeviceDesc% = ULIAGPKX_Install,PCI\VEN_10B9&DEV_5246

[UMC_SYS.NTx86]
%PCI\VEN_1060&DEV_8886.DeviceDesc% = MSISADRV, PCI\VEN_1060&DEV_8886
%PCI\VEN_1060&DEV_886A.DeviceDesc% = MSISADRV, PCI\VEN_1060&DEV_886A
%PCI\VEN_1060&DEV_E886.DeviceDesc% = MSISADRV, PCI\VEN_1060&DEV_E886
%PCI\VEN_1060&DEV_8881.DeviceDesc% = NO_DRV, PCI\VEN_1060&DEV_8881
%PCI\VEN_1060&DEV_0891.DeviceDesc% = NO_DRV, PCI\VEN_1060&DEV_0891
%PCI\VEN_1060&DEV_E881.DeviceDesc% = NO_DRV, PCI\VEN_1060&DEV_E881
%PCI\VEN_1060&DEV_E891.DeviceDesc% = NO_DRV, PCI\VEN_1060&DEV_E891

[VIA_SYS.NTx86]
%PCI\VEN_1106&DEV_0204.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0204
%PCI\VEN_1106&DEV_0208.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0208
%PCI\VEN_1106&DEV_0238.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0238
%PCI\VEN_1106&DEV_0258.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0258
%PCI\VEN_1106&DEV_0259.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0259
%PCI\VEN_1106&DEV_0269.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0269
%PCI\VEN_1106&DEV_0282.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0282
%PCI\VEN_1106&DEV_0296.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0296
%PCI\VEN_1106&DEV_0305.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0305
%PCI\VEN_1106&DEV_0308.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0308
%PCI\VEN_1106&DEV_0314.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0314
%PCI\VEN_1106&DEV_0324.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0324
%PCI\VEN_1106&DEV_0327.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0327
%PCI\VEN_1106&DEV_0336.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0336
%PCI\VEN_1106&DEV_0340.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0340
%PCI\VEN_1106&DEV_0351.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0351
%PCI\VEN_1106&DEV_0353.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0353
%PCI\VEN_1106&DEV_0364.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0364
%PCI\VEN_1106&DEV_0391.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0391
%PCI\VEN_1106&DEV_0409.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0409
%PCI\VEN_1106&DEV_0501.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0501
%PCI\VEN_1106&DEV_0505.DeviceDesc% = MSISADRV, PCI\VEN_1106&DEV_0505
%PCI\VEN_1106&DEV_0576.DeviceDesc% = MSISADRV, PCI\VEN_1106&DEV_0576
%PCI\VEN_1107&DEV_0576.DeviceDesc% = MSISADRV, PCI\VEN_1107&DEV_0576
%PCI\VEN_1106&DEV_0586.DeviceDesc% = MSISADRV, PCI\VEN_1106&DEV_0586
%PCI\VEN_1106&DEV_0596.DeviceDesc% = MSISADRV, PCI\VEN_1106&DEV_0596
%PCI\VEN_1106&DEV_0597.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0597
%PCI\VEN_1106&DEV_0598.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0598
%PCI\VEN_1106&DEV_0601.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0601
%PCI\VEN_1106&DEV_0605.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0605
%PCI\VEN_1106&DEV_0691.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_0691
%PCI\VEN_1106&DEV_0686.DeviceDesc% = MSISADRV, PCI\VEN_1106&DEV_0686
%PCI\VEN_1106&DEV_1204.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_1204
%PCI\VEN_1106&DEV_1208.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_1208
%PCI\VEN_1106&DEV_1238.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_1238
%PCI\VEN_1106&DEV_1258.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_1258
%PCI\VEN_1106&DEV_1259.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_1259
%PCI\VEN_1106&DEV_1269.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_1269
%PCI\VEN_1106&DEV_1282.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_1282
%PCI\VEN_1106&DEV_1296.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_1296
%PCI\VEN_1106&DEV_1308.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_1308
%PCI\VEN_1106&DEV_1314.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_1314
%PCI\VEN_1106&DEV_1324.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_1324
%PCI\VEN_1106&DEV_1327.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_1327
%PCI\VEN_1106&DEV_1336.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_1336
%PCI\VEN_1106&DEV_1340.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_1340
%PCI\VEN_1106&DEV_1351.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_1351
%PCI\VEN_1106&DEV_1353.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_1353
%PCI\VEN_1106&DEV_1364.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_1364
%PCI\VEN_1106&DEV_1409.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_1409
%PCI\VEN_1106&DEV_2204.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_2204
%PCI\VEN_1106&DEV_2208.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_2208
%PCI\VEN_1106&DEV_2238.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_2238
%PCI\VEN_1106&DEV_2258.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_2258
%PCI\VEN_1106&DEV_2259.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_2259
%PCI\VEN_1106&DEV_2269.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_2269
%PCI\VEN_1106&DEV_2282.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_2282
%PCI\VEN_1106&DEV_2296.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_2296
%PCI\VEN_1106&DEV_2308.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_2308
%PCI\VEN_1106&DEV_2314.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_2314
%PCI\VEN_1106&DEV_2324.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_2324
%PCI\VEN_1106&DEV_2327.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_2327
%PCI\VEN_1106&DEV_2336.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_2336
%PCI\VEN_1106&DEV_2340.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_2340
%PCI\VEN_1106&DEV_2351.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_2351
%PCI\VEN_1106&DEV_2353.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_2353
%PCI\VEN_1106&DEV_2364.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_2364
%PCI\VEN_1106&DEV_2409.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_2409
%PCI\VEN_1106&DEV_287A.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_287A
%PCI\VEN_1106&DEV_287B&CC_0604.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_287B&CC_0604
%PCI\VEN_1106&DEV_287B&CC_0600.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_287B&CC_0600
%PCI\VEN_1106&DEV_287C.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_287C
%PCI\VEN_1106&DEV_287D.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_287D
%PCI\VEN_1106&DEV_287E.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_287E
%PCI\VEN_1106&DEV_3040.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3040
%PCI\VEN_1106&DEV_3050.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3050
%PCI\VEN_1106&DEV_3051.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3051
%PCI\VEN_1106&DEV_3057.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3057
%PCI\VEN_1106&DEV_3074.DeviceDesc% = MSISADRV, PCI\VEN_1106&DEV_3074
%PCI\VEN_1106&DEV_3091.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3091
%PCI\VEN_1106&DEV_3099.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3099
%PCI\VEN_1106&DEV_3101.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3101
%PCI\VEN_1106&DEV_3109.DeviceDesc% = MSISADRV, PCI\VEN_1106&DEV_3109
%PCI\VEN_1106&DEV_3112.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3112
%PCI\VEN_1106&DEV_3113.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_3113
%PCI\VEN_1106&DEV_3116.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3116
%PCI\VEN_1106&DEV_3123.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3123
%PCI\VEN_1106&DEV_3128.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3128
%PCI\VEN_1106&DEV_3147.DeviceDesc% = MSISADRV,PCI\VEN_1106&DEV_3147
%PCI\VEN_1106&DEV_3148.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3148
%PCI\VEN_1106&DEV_3156.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3156
%PCI\VEN_1106&DEV_3168.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3168
%PCI\VEN_1106&DEV_3177.DeviceDesc% = MSISADRV,PCI\VEN_1106&DEV_3177
%PCI\VEN_1106&DEV_3188.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3188
%PCI\VEN_1106&DEV_3189.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3189
%PCI\VEN_1106&DEV_3204.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3204
%PCI\VEN_1106&DEV_3205.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3205
%PCI\VEN_1106&DEV_3208.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3208
%PCI\VEN_1106&DEV_3227.DeviceDesc% = MSISADRV,PCI\VEN_1106&DEV_3227
%PCI\VEN_1106&DEV_3238.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3238
%PCI\VEN_1106&DEV_324A.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_324A
%PCI\VEN_1106&DEV_324B&CC_0600.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_324B&CC_0600
%PCI\VEN_1106&DEV_324E.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_324E
%PCI\VEN_1106&DEV_3258.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3258
%PCI\VEN_1106&DEV_3259.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3259
%PCI\VEN_1106&DEV_3269.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3269
%PCI\VEN_1106&DEV_3282.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3282
%PCI\VEN_1106&DEV_3287.DeviceDesc% = MSISADRV, PCI\VEN_1106&DEV_3287
%PCI\VEN_1106&DEV_3296.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3296
%PCI\VEN_1106&DEV_3314.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3314
%PCI\VEN_1106&DEV_3324.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3324
%PCI\VEN_1106&DEV_3327.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3327
%PCI\VEN_1106&DEV_3336.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3336
%PCI\VEN_1106&DEV_3337.DeviceDesc% = MSISADRV, PCI\VEN_1106&DEV_3337
%PCI\VEN_1106&DEV_3340.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3340
%PCI\VEN_1106&DEV_3351.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3351
%PCI\VEN_1106&DEV_3353.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3353
%PCI\VEN_1106&DEV_3364.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3364
%PCI\VEN_1106&DEV_337A.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_337A
%PCI\VEN_1106&DEV_337B&CC_0600.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_337B&CC_0600
%PCI\VEN_1106&DEV_3409.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_3409
%PCI\VEN_1106&DEV_4204.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_4204
%PCI\VEN_1106&DEV_4208.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_4208
%PCI\VEN_1106&DEV_4238.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_4238
%PCI\VEN_1106&DEV_4258.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_4258
%PCI\VEN_1106&DEV_4259.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_4259
%PCI\VEN_1106&DEV_4269.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_4269
%PCI\VEN_1106&DEV_4282.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_4282
%PCI\VEN_1106&DEV_4296.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_4296
%PCI\VEN_1106&DEV_4308.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_4308
%PCI\VEN_1106&DEV_4314.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_4314
%PCI\VEN_1106&DEV_4324.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_4324
%PCI\VEN_1106&DEV_4327.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_4327
%PCI\VEN_1106&DEV_4336.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_4336
%PCI\VEN_1106&DEV_4340.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_4340
%PCI\VEN_1106&DEV_4351.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_4351
%PCI\VEN_1106&DEV_4353.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_4353
%PCI\VEN_1106&DEV_4364.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_4364
%PCI\VEN_1106&DEV_4409.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_4409
%PCI\VEN_1106&DEV_5208.DeviceDesc% = NO_DRV_MEM, PCI\VEN_1106&DEV_5208
%PCI\VEN_1106&DEV_5238.DeviceDesc% = NO_DRV_MEM, PCI\VEN_1106&DEV_5238
%PCI\VEN_1106&DEV_5308.DeviceDesc% = NO_DRV_MEM, PCI\VEN_1106&DEV_5308
%PCI\VEN_1106&DEV_5327.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_5327
%PCI\VEN_1106&DEV_5336.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_5336
%PCI\VEN_1106&DEV_5340.DeviceDesc% = NO_DRV_MEM, PCI\VEN_1106&DEV_5340
%PCI\VEN_1106&DEV_5351.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_5351
%PCI\VEN_1106&DEV_5353.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_5353
%PCI\VEN_1106&DEV_5364.DeviceDesc% = NO_DRV_MEM, PCI\VEN_1106&DEV_5364
%PCI\VEN_1106&DEV_5409.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_5409
%PCI\VEN_1106&DEV_6327.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_6327
%PCI\VEN_1106&DEV_6340.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_6340
%PCI\VEN_1106&DEV_6353.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_6353
%PCI\VEN_1106&DEV_6364.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_6364
%PCI\VEN_1106&DEV_6409.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_6409
%PCI\VEN_1106&DEV_7204.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_7204
%PCI\VEN_1106&DEV_7208.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_7208
%PCI\VEN_1106&DEV_7238.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_7238
%PCI\VEN_1106&DEV_7258.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_7258
%PCI\VEN_1106&DEV_7259.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_7259
%PCI\VEN_1106&DEV_7269.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_7269
%PCI\VEN_1106&DEV_7282.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_7282
%PCI\VEN_1106&DEV_7296.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_7296
%PCI\VEN_1106&DEV_7308.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_7308
%PCI\VEN_1106&DEV_7314.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_7314
%PCI\VEN_1106&DEV_7324.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_7324
%PCI\VEN_1106&DEV_7327.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_7327
%PCI\VEN_1106&DEV_7336.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_7336
%PCI\VEN_1106&DEV_7340.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_7340
%PCI\VEN_1106&DEV_7351.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_7351
%PCI\VEN_1106&DEV_7353.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_7353
%PCI\VEN_1106&DEV_7364.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_7364
%PCI\VEN_1106&DEV_7409.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_7409
%PCI\VEN_1106&DEV_8231.DeviceDesc% = MSISADRV, PCI\VEN_1106&DEV_8231
%PCI\VEN_1106&DEV_8235.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_8235
%PCI\VEN_1106&DEV_8324.DeviceDesc% = MSISADRV, PCI\VEN_1106&DEV_8324
%PCI\VEN_1106&DEV_8409.DeviceDesc% = MSISADRV, PCI\VEN_1106&DEV_8409
%PCI\VEN_1106&DEV_A208.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_A208
%PCI\VEN_1106&DEV_A238.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_A238
%PCI\VEN_1106&DEV_A327.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_A327
%PCI\VEN_1106&DEV_A364.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_A364
%PCI\VEN_1106&DEV_B113.DeviceDesc% = NO_DRV_MEM,PCI\VEN_1106&DEV_B113
%PCI\VEN_1106&DEV_C208.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_C208
%PCI\VEN_1106&DEV_C238.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_C238
%PCI\VEN_1106&DEV_C327.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_C327
%PCI\VEN_1106&DEV_C340.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_C340
%PCI\VEN_1106&DEV_C364.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_C364
%PCI\VEN_1106&DEV_D208.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_D208
%PCI\VEN_1106&DEV_D238.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_D238
%PCI\VEN_1106&DEV_D340.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_D340
%PCI\VEN_1106&DEV_E208.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_E208
%PCI\VEN_1106&DEV_E238.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_E238
%PCI\VEN_1106&DEV_E340.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_E340
%PCI\VEN_1106&DEV_F208.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_F208
%PCI\VEN_1106&DEV_F238.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_F238
%PCI\VEN_1106&DEV_F340.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_F340
%PCI\VEN_1106&DEV_8305.DeviceDesc% = VIAAGP_Install,PCI\VEN_1106&DEV_8305
%PCI\VEN_1106&DEV_8353.DeviceDesc% = MSISADRV, PCI\VEN_1106&DEV_8353
%PCI\VEN_1106&DEV_8391.DeviceDesc% = VIAAGP_Install,PCI\VEN_1106&DEV_8391
%PCI\VEN_1106&DEV_8598.DeviceDesc% = VIAAGP_Install,PCI\VEN_1106&DEV_8598
%PCI\VEN_1106&DEV_8501.DeviceDesc% = VIAAGP_Install,PCI\VEN_1106&DEV_8501
%PCI\VEN_1106&DEV_8601.DeviceDesc% = VIAAGP_Install,PCI\VEN_1106&DEV_8601
%PCI\VEN_1106&DEV_8605.DeviceDesc% = VIAAGP_Install,PCI\VEN_1106&DEV_8605
%PCI\VEN_1106&DEV_A353.DeviceDesc% = NO_DRV, PCI\VEN_1106&DEV_A353
%PCI\VEN_1106&DEV_B091.DeviceDesc% = VIAAGP_Install,PCI\VEN_1106&DEV_B091
%PCI\VEN_1106&DEV_B099.DeviceDesc% = VIAAGP_Install,PCI\VEN_1106&DEV_B099
%PCI\VEN_1106&DEV_B112.DeviceDesc% = VIAAGP_Install,PCI\VEN_1106&DEV_B112
%PCI\VEN_1106&DEV_B168.DeviceDesc% = VIAAGP_Install,PCI\VEN_1106&DEV_B168
%PCI\VEN_1106&DEV_B353.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_B353
%PCI\VEN_1106&DEV_C353.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_C353
%PCI\VEN_1106&DEV_E353.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_E353
%PCI\VEN_1106&DEV_F353.DeviceDesc% = PCI_DRV, PCI\VEN_1106&DEV_F353

[VLSI_SYS.NTx86]
%PCI\VEN_1004&DEV_0005.DeviceDesc% = NO_DRV, PCI\VEN_1004&DEV_0005
%PCI\VEN_1004&DEV_0006.DeviceDesc% = MSISADRV, PCI\VEN_1004&DEV_0006
%PCI\VEN_1004&DEV_0101.DeviceDesc% = MSISADRV, PCI\VEN_1004&DEV_0101
%PCI\VEN_1004&DEV_0102.DeviceDesc% = PCI_DRV, PCI\VEN_1004&DEV_0102
%PCI\VEN_1004&DEV_0103.DeviceDesc% = MSISADRV, PCI\VEN_1004&DEV_0103
%PCI\VEN_1004&DEV_0104.DeviceDesc% = NO_DRV, PCI\VEN_1004&DEV_0104

;****************************************************
; Generic PCI Root Bus/PCI-PCI Bridge
[PCI_DRV_ROOT]
CopyFiles=PCI_COPYFILES
SyssetupPnPFlags = 1
AddReg = PCI_DRV_ROOT_REG

[PCI_COPYFILES]
pci.sys,,,0x100 ;COPYFLG_PROTECTED_WINDOWS_DRIVER_FILE

[PCI_DRV_ROOT.Services]
AddService = pci, %SPSVCINST_ASSOCSERVICE%, pci_ServiceInstallSection

[PCI_DRV_ROOT.HW]
AddReg         = PCI_DRV_HW.AddReg

[PCI_DRV_ROOT_REG]
HKR,,ResourcePickerExceptions,0,"IO:HAL,MBRES;MEM:HAL,MBRES"
HKR,,ResourcePickerTags,0,"MBRES"

[PCI_DRV]
CopyFiles=PCI_COPYFILES
SyssetupPnPFlags = 1

[PCI_DRV.Services]
AddService = pci, %SPSVCINST_ASSOCSERVICE%, pci_ServiceInstallSection

[pci_ServiceInstallSection]
DisplayName    = %pci_svcdesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_CRITICAL%
ServiceBinary  = %12%\pci.sys
LoadOrderGroup = "Boot Bus Extender"
AddReg = pci_ServiceInstallSection_AddReg

[PCI_DRV.HW]
AddReg         = PCI_DRV_HW.AddReg

[PCI_DRV_HW.AddReg]
HKR,,UINumberDescFormat,,%PCISlot%

;****************************************************
; Generic ISA Bus / PCI-ISA Bridge / PCI-EISA Bridge
[MSISADRV]
CopyFiles=MsIsaDrv_CopyFiles

[MsIsaDrv_CopyFiles]
msisadrv.sys,,,0x100 ;COPYFLG_PROTECTED_WINDOWS_DRIVER_FILE

[MSISADRV.Services]
AddService = msisadrv, %SPSVCINST_ASSOCSERVICE%, msisadrv_ServiceInstallSection

[msisadrv_ServiceInstallSection]
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_CRITICAL%
ServiceBinary  = %12%\msisadrv.sys
LoadOrderGroup = "Boot Bus Extender"
AddReg = msisadrv_ServiceInstallSection_AddReg

;****************************************************
; External INFs may include ISAPNP_DRV section.  This section is provided for
; backwards compatibility with those infs.  New infs should use include
; msisadrv section instead.
;
[ISAPNP_DRV]
CopyFiles=MsIsaDrv_CopyFiles

[ISAPNP_DRV.Services]
AddService = msisadrv, %SPSVCINST_ASSOCSERVICE%, msisadrv_ServiceInstallSection

;****************************************************
; ISA PnP Bus
; The LEGACY_ISAPNP_DRV should only be used for systems which require
; the ability to enumerate devices via ISAPNP protocol.  Most systems should use
; msisadrv.
;

[LEGACY_ISAPNP_DRV]
CopyFiles=IsaPnp_CopyFiles

[IsaPnp_CopyFiles]
isapnp.sys,,,0x100 ;COPYFLG_PROTECTED_WINDOWS_DRIVER_FILE

[LEGACY_ISAPNP_DRV.Services]
AddService = isapnp, %SPSVCINST_ASSOCSERVICE%, isapnp_ServiceInstallSection, isapnp_EventLogInstallSection

[isapnp_ServiceInstallSection]
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_CRITICAL%
ServiceBinary  = %12%\isapnp.sys
LoadOrderGroup = "Boot Bus Extender"
AddReg         = ISAPNP_DRV.AddReg

[ISAPNP_DRV.AddReg]
HKR,,HasBootConfig,0x00010001,00000000

[isapnp_EventLogInstallSection]
AddReg = isapnp_EventLog_AddReg

[isapnp_EventLog_AddReg]
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\isapnp.sys"
HKR,,TypesSupported,%REG_DWORD%,7

;****************************************************
; Dock only PCI-(E)ISA Bridge
; Only neccessary if bridge is located prior to ISA bridge in laptop device
; number-wise
[ISAPNP_DOCKONLY_DRV]
CopyFiles=@isapnp.sys

[ISAPNP_DOCKONLY_DRV.HW]
AddReg = ISAPNP_DOCKONLY_DRV_AddReg

[ISAPNP_DOCKONLY_DRV.Services]
AddService = isapnp, %SPSVCINST_ASSOCSERVICE%, isapnp_ServiceInstallSection, isapnp_EventLogInstallSection

[ISAPNP_DOCKONLY_DRV_AddReg]
HKR,,DeferBridge,0x00010001,00000001


;**************************************************************************
; AGP filters that sit on top of PCI
;

;
; Microsoft AGPv3.5
;
[UAGP35_Install]
CopyFiles=@UAGP35.SYS

[UAGP35_Filter_Reg]
HKR,,"UpperFilters", 0x00010000,"UAGP35"
HKLM,"SYSTEM\CurrentControlSet\Services\uagp35\Parameters","1106316800",0x00030003,00,00,30,00,00,00,00,00
HKLM,"SYSTEM\CurrentControlSet\Services\uagp35\Parameters","1106316802",0x00030003,00,00,30,00,00,00,00,00
HKLM,"SYSTEM\CurrentControlSet\Services\uagp35\Parameters","1106316803",0x00030003,00,00,30,00,00,00,00,00
HKLM,"SYSTEM\CurrentControlSet\Services\uagp35\Parameters","1106318900",0x00030003,00,00,70,00,00,00,00,00
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\drivers\uagp35.sys"
HKR,,TypesSupported,%REG_DWORD%,7


[UAGP35_Install.HW]
AddReg = UAGP35_Filter_Reg

[UAGP35_Install.Services]
AddService = uagp35,0,uagp35_ServiceInstallSection
AddService = pci, %SPSVCINST_ASSOCSERVICE%, pci_ServiceInstallSection
DelService = agp440
DelService = viaagp1
DelService = sisagp

[uagp35_ServiceInstallSection]
DisplayName    = %uagp35_svcdesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_DEMAND_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\uagp35.sys
LoadOrderGroup = PnP Filter

;
; Intel 440LX/BX/EX
;
[AGP440_Install]
CopyFiles=AGP440_COPYFILES

[AGP440_COPYFILES]
AGP440.sys,,,0x100 ;COPYFLG_PROTECTED_WINDOWS_DRIVER_FILE
[AGP440_Filter_Reg]
HKR,,"UpperFilters", 0x00010000,"AGP440"
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\drivers\agp440.sys"
HKR,,TypesSupported,%REG_DWORD%,7

[AGP440_Install.HW]
AddReg = AGP440_Filter_Reg

[AGP440_Install.Services]
AddService = agp440,0,agp440_ServiceInstallSection
AddService = pci, %SPSVCINST_ASSOCSERVICE%, pci_ServiceInstallSection

[agp440_ServiceInstallSection]
DisplayName    = %agp440_svcdesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_DEMAND_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\agp440.sys
LoadOrderGroup = PnP Filter

;
; Intel 840
;
[AGP840_Install]
CopyFiles=AGP440_COPYFILES

[AGP840_Filter_Reg]
HKR,,"UpperFilters", 0x00010000,"AGP440"
HKLM,"SYSTEM\CurrentControlSet\Services\agp440\Parameters","3D3D07A1",0x00030003,04,00,00,00,00,00,00,00
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\drivers\agp440.sys"
HKR,,TypesSupported,%REG_DWORD%,7

[AGP840_Install.HW]
AddReg = AGP840_Filter_Reg

[AGP840_Install.Services]
AddService = agp440,0,agp440_ServiceInstallSection
AddService = pci, %SPSVCINST_ASSOCSERVICE%, pci_ServiceInstallSection


;
; VIA AGP chipset
;
[VIAAGP_Install]
CopyFiles=@VIAAGP.SYS

[AGPVIA_Filter_Reg]
HKR,,"UpperFilters", 0x00010000,"VIAAGP"
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\drivers\viaagp.sys"
HKR,,TypesSupported,%REG_DWORD%,7

[VIAAGP_Install.HW]
AddReg = AGPVIA_Filter_Reg

[VIAAGP_Install.Services]
AddService = viaagp,0,viaagp_ServiceInstallSection
AddService = pci, %SPSVCINST_ASSOCSERVICE%, pci_ServiceInstallSection

[viaagp_ServiceInstallSection]
DisplayName    = %agpvia_svcdesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_DEMAND_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\viaagp.sys
LoadOrderGroup = PnP Filter

;
; AMD AGP chipset
;
[AMDAGP_Install]
CopyFiles=@AMDAGP.SYS

[AMDAGP_Filter_Reg]
HKR,,"UpperFilters", 0x00010000,"AMDAGP"
HKLM,"SYSTEM\CurrentControlSet\Services\amdagp\Parameters","10DE002D",0x00030003,00,00,10,00,8F,FA,84,D5
HKLM,"SYSTEM\CurrentControlSet\Services\amdagp\Parameters","102B0525",0x00030003,00,00,10,00,8E,F8,83,A5
HKLM,"SYSTEM\CurrentControlSet\Services\amdagp\Parameters","53338A22",0x00030003,00,00,10,00,8E,F8,83,A5
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\drivers\amdagp.sys"
HKR,,TypesSupported,%REG_DWORD%,7

[AMDAGP_Install.HW]
AddReg = AMDAGP_Filter_Reg

[AMDAGP_Install.Services]
AddService = amdagp,0,amdagp_ServiceInstallSection
AddService = pci, %SPSVCINST_ASSOCSERVICE%, pci_ServiceInstallSection

[amdagp_ServiceInstallSection]
DisplayName    = %amdagp_svcdesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_DEMAND_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\amdagp.sys
LoadOrderGroup = PnP Filter

;
; Generic AGPv3.0 driver for AMD K8/9 platforms
;
[GAGP30KX_Install]
CopyFiles=@GAGP30KX.SYS

[GAGP30KX_Filter_Reg]
HKR,,"UpperFilters", 0x00010000,"GAGP30KX"
HKLM,"SYSTEM\CurrentControlSet\Services\gagp30kx\Parameters","10227454",0x00000001,00,00,d0,00,00,00,00,00
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\drivers\gagp30kx.sys"
HKR,,TypesSupported,%REG_DWORD%,7

[GAGP30KX_Install.HW]
AddReg = GAGP30KX_Filter_Reg

[GAGP30KX_Install.Services]
AddService = gagp30kx,0,gagp30kx_ServiceInstallSection
AddService = pci, %SPSVCINST_ASSOCSERVICE%, pci_ServiceInstallSection
DelService = amdagp8p
DelService = viaagp1
DelService = sisagp

[gagp30kx_ServiceInstallSection]
DisplayName    = %gagp30kx_svcdesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_DEMAND_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\gagp30kx.sys
LoadOrderGroup = PnP Filter

;
; SIS
;
[SISAGP_Install]
CopyFiles=@SISAGP.SYS

[SISAGP_Filter_Reg]
HKR,,"UpperFilters", 0x00010000,"SISAGP"
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\drivers\sisagp.sys"
HKR,,TypesSupported,%REG_DWORD%,7

[SISAGP_Install.HW]
AddReg = SISAGP_Filter_Reg

[SISAGP_Install.Services]
AddService = sisagp,0,sisagp_ServiceInstallSection
AddService = pci, %SPSVCINST_ASSOCSERVICE%, pci_ServiceInstallSection

[sisagp_ServiceInstallSection]
DisplayName    = %sisagp_svcdesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_DEMAND_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\sisagp.sys
LoadOrderGroup = PnP Filter

;
; Nvidia
;
[NVIDIAAGP_Install]
CopyFiles=@NV_AGP.SYS

[NVIDIAAGP_Filter_Reg]
HKR,,"UpperFilters", 0x00010000,"nv_agp"
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\drivers\nv_agp.sys"
HKR,,TypesSupported,%REG_DWORD%,7

[NVIDIAAGP_Install.HW]
AddReg = NVIDIAAGP_Filter_Reg

[NVIDIAAGP_Install.Services]
AddService = nv_agp,0,NVIDIAAGP_ServiceInstallSection
AddService = pci, %SPSVCINST_ASSOCSERVICE%, pci_ServiceInstallSection

[NVIDIAAGP_ServiceInstallSection]
DisplayName    = %agpnvidia_svcdesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_DEMAND_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\nv_agp.sys
LoadOrderGroup = PnP Filter

;
; ULI
;
[ULIAGPKX_Install]
CopyFiles=@ULIAGPKX.SYS

[ULIAGPKX_Filter_Reg]
HKR,,"UpperFilters", 0x00010000,"ULIAGPKX"
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\drivers\uliagpkx.sys"
HKR,,TypesSupported,%REG_DWORD%,7

[ULIAGPKX_Install.HW]
AddReg = ULIAGPKX_Filter_Reg

[ULIAGPKX_Install.Services]
AddService = uliagpkx,0,ULIAGPKX_ServiceInstallSection
AddService = pci, %SPSVCINST_ASSOCSERVICE%, pci_ServiceInstallSection

[ULIAGPKX_ServiceInstallSection]
DisplayName    = %uliagpkx_svcdesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_DEMAND_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\uliagpkx.sys
LoadOrderGroup = PnP Filter

;**************************************************************************
; Virtual Drive Enumerator
[VDRVROOT]
CopyFiles=VDRVROOT_CopyFiles

[VDRVROOT_CopyFiles]
vdrvroot.sys,,,0x100 ; COPYFLG_PROTECTED_WINDOWS_DRIVER_FILE

[VDRVROOT.Services]
AddService=vdrvroot, %SPSVCINST_ASSOCSERVICE%, VDRVROOT_Service

[VDRVROOT.HW]
AddReg=VDRVROOT_HW.AddReg

[VDRVROOT_Service]
DisplayName    = %vdrvroot_svcdesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_CRITICAL%
ServiceBinary  = %12%\vdrvroot.sys
LoadOrderGroup = "Boot Bus Extender"

[VDRVROOT_HW.AddReg]
HKR,VirtualDriveSupport,VHD,0x10001,1

;**************************************************************************
; Volume Manager
[Volmgr]
CopyFiles      = Volmgr_CopyFiles
Reboot

[Volmgr_CopyFiles]
volmgr.sys,,,0x100 ; COPYFLG_PROTECTED_WINDOWS_DRIVER_FILE

[Volmgr.Services]
AddService     = volmgr, %SPSVCINST_ASSOCSERVICE%, Volmgr_Service, Volmgr_Eventlog

[Volmgr_Service]
DisplayName    = %volmgr_svcdesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_CRITICAL%
ServiceBinary  = %12%\volmgr.sys
LoadOrderGroup = "System Bus Extender"
AddReg         = volmgr_Service_AddReg

[volmgr_Service_AddReg]
HKR,,Tag,0x00010001,9

[Volmgr_Eventlog]
AddReg         = Volmgr_Eventlog_AddReg

[Volmgr_Eventlog_AddReg]
HKR,, EventMessageFile, %REG_EXPAND_SZ%, "%%SystemRoot%%\System32\IoLogMsg.dll"
HKR,, TypesSupported, %REG_DWORD%, 7

;**************************************************************************
; Software Bus
[SWENUM]
CopyFiles=@swenum.sys

[SWENUM.CoInstallers]
AddReg          = SWENUM.CoInstallers.AddReg
CopyFiles       = SWENUM.CoInstallers.CopyFiles

[SWENUM.CoInstallers.AddReg]
HKR,,CoInstallers32,0x10000,"streamci.dll,SwEnumCoInstaller"

[SWENUM.CoInstallers.CopyFiles]
streamci.dll

[SWENUM.Services]
AddService = swenum, %SPSVCINST_ASSOCSERVICE%, SWENUM.ServiceInstall

[SWENUM.ServiceInstall]
DisplayName    = %swenum_svcdesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_DEMAND_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\swenum.sys

;**************************************************************************
; RDP Remote Keyboard & Mouse

; RDP Remote Keyboard
[RDP_KBD]
Include = keyboard.inf
Needs   = STANDARD_Inst

[RdpKbd_CopyFiles]

[RDP_KBD.HW]
AddReg=RDP_KBD.HW.AddReg

[RDP_KBD.HW.AddReg]
HKR,,"UpperFilters",0x00010000,"kbdclass"

[RDP_KBD.Services]
Include = keyboard.inf
AddService = TermDD, %SPSVCINST_ASSOCSERVICE%, TermDD.ServiceInstall
AddService = kbdclass,, kbdclass_Service_Inst, kbdclass_EventLog_Inst            ; Class Driver
DelService = rdp_console

; RDP Remote Mouse
[RDP_MOU]
CopyFiles=RdpMou_CopyFiles
Include = msmouse.inf
Needs   = Ser_Inst

[RdpMou_CopyFiles]
termdd.sys,,,0x100 ;COPYFLG_PROTECTED_WINDOWS_DRIVER_FILE

[RDP_MOU.HW]
AddReg=RDP_MOU.HW.AddReg

[RDP_MOU.HW.AddReg]
HKR,,"UpperFilters",0x00010000,"mouclass"

[RDP_MOU.Services]
Include = msmouse.inf
AddService = TermDD, %SPSVCINST_ASSOCSERVICE%, TermDD.ServiceInstall
AddService = mouclass,, mouclass_Service_Inst, mouclass_EventLog_Inst      ; Class Driver

[TermDD.ServiceInstall]
DisplayName    = %TermDD_svcdesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_SYSTEM_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\termdd.sys

[MSSMBIOS_DRV]
CopyFiles=Mssmbios_CopyFiles

[Mssmbios_CopyFiles]
mssmbios.sys,,,0x100 ;COPYFLG_PROTECTED_WINDOWS_DRIVER_FILE

[MSSMBIOS_DRV.Services]
AddService = mssmbios, %SPSVCINST_ASSOCSERVICE%, MSSMBIOS_DRV.ServiceInstall

[MSSMBIOS_DRV.ServiceInstall]
DisplayName    = %mssmbios_svcdesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_SYSTEM_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\mssmbios.sys

;**************************************************************************
; Do-nothing section used to avoid "Unknown hardware" installation prompts.
[NO_DRV]

[NO_DRV.Services]
AddService = , %SPSVCINST_ASSOCSERVICE%   ; null service install

; NO_DRV Variation with MUTEing
[NO_DRV_X]
AddReg = NO_DRV_X_REG

[NO_DRV_X.Services]
AddService = , %SPSVCINST_ASSOCSERVICE%   ; null service install

[NO_DRV_X_REG]
HKR,,ResourcePickerExceptions,0,"IO@0-0xFF:*;IO:HAL,MBRES;IRQ:HAL,*"
HKR,,ResourcePickerTags,0,"MBRES"

; NO_DRV Variation with MUTEing and SysSetupPnpFlags flags
[NO_DRV_X_PNP]
SyssetupPnPFlags = 1
AddReg = NO_DRV_X_PNP_REG

[NO_DRV_X_PNP.Services]
AddService = , %SPSVCINST_ASSOCSERVICE%   ; null service install

[NO_DRV_X_PNP_REG]
HKR,,ResourcePickerExceptions,0,"IO@0-0xFF:*;IO:HAL,MBRES;IRQ:HAL,*"
HKR,,ResourcePickerTags,0,"MBRES"

; NO_DRV Variation - MUTEing for PIC/APIC
[NO_DRV_PIC]
AddReg = NO_DRV_PIC_REG

[NO_DRV_PIC.Services]
AddService = , %SPSVCINST_ASSOCSERVICE%   ; null service install

[NO_DRV_PIC_REG]
HKR,,ResourcePickerExceptions,0,"IO@0-0xFF:*;IO:HAL,MBRES;MEM:HAL,MBRES,*;IRQ:HAL,MBRES,*"
HKR,,ResourcePickerTags,0,"MBRES"

; NO_DRV Variation - MUTEing for HPET
[NO_DRV_HPET]
AddReg = NO_DRV_HPET_REG

[NO_DRV_HPET.Services]
AddService = , %SPSVCINST_ASSOCSERVICE%   ; null service install

[NO_DRV_HPET_REG]
HKR,,ResourcePickerExceptions,0,"MEM:HAL,MBRES,*;IRQ:HAL,MBRES,*"
HKR,,ResourcePickerTags,0,"MBRES"

; NO_DRV Variation - MUTEing/TAGing for motherboard resource
[NO_DRV_MBRES]
AddReg = NO_DRV_MBRES_REG

[NO_DRV_MBRES.Services]
AddService = , %SPSVCINST_ASSOCSERVICE%   ; null service install

[NO_DRV_MBRES_REG]
HKR,,ResourcePickerExceptions,0,"IO:HAL,MBRES,*;MEM:HAL,MBRES,*"
HKR,,ResourcePickerTags,0,"MBRES"

; NO_DRV Variation - MUTEing for MEM only conflicts
[NO_DRV_MEM]
AddReg = NO_DRV_MEM_REG

[NO_DRV_MEM.Services]
AddService = , %SPSVCINST_ASSOCSERVICE%   ; null service install

[NO_DRV_MEM_REG]
HKR,,ResourcePickerExceptions,0,"MEM:HAL,MBRES,*"
HKR,,ResourcePickerTags,0,"MBRES"

; Overrides for dock eject priority (3rd party INFs should use the ID of the
; _DCK device, ie the one with a OEM hardware ID and a compat ID of PNP0C15)
[MS_TPDOCK]

[MS_TPDOCK.Services]
AddService = , %SPSVCINST_ASSOCSERVICE%   ; null service install

[MS_TPDOCK.HW]
AddReg = MS_TPDOCK_HW.AddReg

[MS_TPDOCK_HW.AddReg]
HKR,,EjectPriority,0x00010001,00000100

[MS_TPSLICE]

[MS_TPSLICE.Services]
AddService = , %SPSVCINST_ASSOCSERVICE%   ; null service install

[MS_TPSLICE.HW]
AddReg = MS_TPSLICE_HW.AddReg

[MS_TPSLICE_HW.AddReg]
HKR,,EjectPriority,0x00010001,00000080

;**************************************************************************
; Section for device INFs to include in their DDInstall section, for features
; that are not detectable by just looking at the device hardware.
[PciIoSpaceNotRequired]
AddReg=PciIoSpaceNotRequired.RegHW
[PciIoSpaceNotRequired.RegHW]
HKR,e5b3b5ac-9725-4f78-963f-03dfb1d828c7,IoNotRequired,0x10001,1

[PciASPMOptIn]
AddReg=PciASPMOptIn.RegHW
[PciASPMOptIn.RegHW]
HKR,e5b3b5ac-9725-4f78-963f-03dfb1d828c7,ASPMOptIn,0x10001,1

[PciASPMOptOut]
AddReg=PciASPMOptOut.RegHW
[PciASPMOptOut.RegHW]
HKR,e5b3b5ac-9725-4f78-963f-03dfb1d828c7,ASPMOptOut,0x10001,1

[pci_ServiceInstallSection_AddReg]
HKR,,Tag,0x00010001,3

[msisadrv_ServiceInstallSection_AddReg]
HKR,,Tag,0x00010001,2

[Strings]
; localizable

MSFT            = "Microsoft"

;*******************************************
;device descriptions

GENDEV_MFG = "(Standard system devices)"
*pnp0a00.DeviceDesc           = "ISA Plug and Play bus"
*pnp0a01.DeviceDesc           = "EISA bus"
*pnp0a04.DeviceDesc           = "ISA Plug and Play bus with VL slots"
*pnp0a03.DeviceDesc           = "PCI bus"
PCI\CC_0604.DeviceDesc        = "PCI standard PCI-to-PCI bridge"
PCI\CC_0604&DT_4.DeviceDesc   = "PCI Express standard Root Port"
PCI\CC_0604&DT_5.DeviceDesc   = "PCI Express standard Upstream Switch Port"
PCI\CC_0604&DT_6.DeviceDesc   = "PCI Express standard Downstream Switch Port"
PCI\CC_0604&DT_7.DeviceDesc   = "PCI standard PCI Express to PCI/PCI-X Bridge"
PCI\CC_0604&DT_8.DeviceDesc   = "PCI standard PCI/PCI-X to PCI Express Bridge"
PCI\CC_0601.DeviceDesc        = "PCI standard ISA bridge"
PCI\CC_0602.DeviceDesc        = "PCI standard EISA bridge"
PCI\CC_0500.DeviceDesc        = "PCI standard RAM Controller"
PCI\CC_0600.DeviceDesc        = "PCI standard host CPU bridge"
Volmgr.DeviceDesc             = "Volume Manager"
SWENUM.DeviceDesc             = "Plug and Play Software Device Enumerator"
VDRVROOT.DeviceDesc           = "Microsoft Virtual Drive Enumerator Driver"

Root\MSSMBios.DeviceDesc      = "Microsoft System Management BIOS Driver"
RDP_MOU.DeviceDesc            = "Terminal Server Mouse Driver"
RDP_KBD.DeviceDesc            = "Terminal Server Keyboard Driver"
TermDD_svcdesc                = "Terminal Device Driver"

acpi0004.DeviceDesc="ACPI Module Device"
*pnp0000.DeviceDesc="Programmable interrupt controller"
*pnp0001.DeviceDesc="EISA programmable interrupt controller"
*pnp0003.DeviceDesc="Advanced programmable interrupt controller"
*pnp0004.DeviceDesc="Cyrix SLiC MP interrupt controller"
*pnp0100.DeviceDesc="System timer"
*pnp0101.DeviceDesc="EISA system timer"
*pnp0103.DeviceDesc="High precision event timer"
*pnp0200.DeviceDesc="Direct memory access controller"
*pnp0201.DeviceDesc="EISA direct memory access controller"
*pnp0800.DeviceDesc="System speaker"
*pnp0a05.DeviceDesc="Generic Bus"
*pnp0a06.DeviceDesc="Extended IO Bus"
*pnp0b00.DeviceDesc="System CMOS/real time clock"
*pnp0c00.DeviceDesc="Plug and Play BIOS"
*pnp0c01.DeviceDesc="System board"
*pnp0c02.DeviceDesc="Motherboard resources"
*pnp0c04.DeviceDesc="Numeric data processor"
;*pnp0c05.DeviceDesc="Advanced Power Management support"
*pnp0c09.DeviceDesc="Microsoft ACPI-Compliant Embedded Controller"
;*pnp0c0a.DeviceDesc="ACPI Battery"
*pnp0c0b.DeviceDesc="ACPI Fan"
*pnp0c0c.DeviceDesc="ACPI Power Button"
*pnp0c0d.DeviceDesc="ACPI Lid"
*pnp0c0e.DeviceDesc="ACPI Sleep Button"
;*pnp0c0f.DeviceDesc="ACPI IRQ Holder for PCI IRQ Steering"
;*pnp0c13.DeviceDesc="Plug and Play BIOS (fail safe)"
*PNP0C15.DeviceDesc="Docking Station"
*PNP0C32.DeviceDesc="Direct Application Launch Button"
ACPI\FixedButton.DeviceDesc="ACPI Fixed Feature Button"
ACPI\ThermalZone.DeviceDesc="ACPI Thermal Zone"
ACPI\DockDevice.DeviceDesc="Docking Station"
*LEGACYISAPNP.DeviceDesc="Legacy ISAPNP device"
ISAPNP\ReadDataPort.DeviceDesc="ISAPNP Read Data Port"
LPTENUM\MicrosoftRawPort958A.DeviceDesc = "Printer Port Logical Interface"

ACC_MFG = "ACC"
PCI\VEN_10AA&DEV_0000.DeviceDesc = "ACC Microelectronics Pentium(r) CPU to PCI & PCI to ISA bridge"

ACER_MFG="ACER"
PCI\VEN_1025&DEV_1435.DeviceDesc = "ACER 486 CPU to PCI & PCI to ISA bridge"

ALI_MFG="ALi"
PCI\VEN_10B9&DEV_1445.DeviceDesc = "ALi 486 CPU to PCI & PCI to ISA bridge"
PCI\VEN_10B9&DEV_1449.DeviceDesc = "ALi PCI to ISA bridge"
PCI\VEN_10B9&DEV_1451.DeviceDesc = "ALi Pentium(r) CPU to PCI bridge"
PCI\VEN_10B9&DEV_1489.DeviceDesc = "ALi 486 CPU to PCI & PCI to ISA bridge"
PCI\VEN_10B9&DEV_1521.DeviceDesc = "ALi CPU to PCI bridge"
PCI\VEN_10B9&DEV_1523.DeviceDesc = "ALi M1523 PCI to ISA bridge"
PCI\VEN_10B9&DEV_1531.DeviceDesc = "ALi M1531 CPU to PCI bridge"
PCI\VEN_10B9&DEV_1533.DeviceDesc = "ALi PCI to ISA bridge"
PCI\VEN_10B9&DEV_1541.DeviceDesc = "ALi M1541 CPU to PCI bridge"
PCI\VEN_10B9&DEV_1621.DeviceDesc = "ALi CPU to PCI bridge"
PCI\VEN_10B9&DEV_1647.DeviceDesc = "ALi CPU to PCI bridge"
PCI\VEN_10B9&DEV_1651.DeviceDesc = "ALi CPU to PCI bridge"
PCI\VEN_10B9&DEV_5243.DeviceDesc = "ALi M1541 PCI to AGP Controller"
PCI\VEN_10B9&DEV_5247.DeviceDesc = "ALi PCI to AGP Controller"
PCI\VEN_10B9&DEV_7101.DeviceDesc = "ALi 7101 Power Management Controller"

AMD_MFG = "AMD"
PCI\VEN_1002&DEV_5A23.DeviceDesc = "AMD IOMMU Device"
PCI\VEN_1022&DEV_1100.DeviceDesc = "AMD HyperTransport(tm) Configuration"
PCI\VEN_1022&DEV_1101.DeviceDesc = "AMD Address Map Configuration"
PCI\VEN_1022&DEV_1102.DeviceDesc = "AMD DRAM and HyperTransport(tm) Trace Mode Configuration"
PCI\VEN_1022&DEV_1103.DeviceDesc = "AMD Miscellaneous Configuration"
PCI\VEN_1022&DEV_7007.DeviceDesc = "AMD-751 Processor to AGP Controller"
PCI\VEN_1022&DEV_700D.DeviceDesc = "AMD-762 Processor to AGP Controller"
PCI\VEN_1022&DEV_700F.DeviceDesc = "AMD-761 Processor to AGP Controller"
PCI\VEN_1022&DEV_740B.DeviceDesc = "AMD-756 Power Management Controller"
PCI\VEN_1022&DEV_7413.DeviceDesc = "AMD-766 Power Management Controller"
PCI\VEN_1022&DEV_7443.DeviceDesc = "AMD-768 Power Management Controller"
PCI\VEN_1022&DEV_7451.DeviceDesc = "AMD-8131 HyperTransport(tm) IOAPIC Controller"
PCI\VEN_1022&DEV_7459.DeviceDesc = "AMD-8132 HyperTransport(tm) IOAPIC Controller"
PCI\VEN_1022&DEV_746A.DeviceDesc = "AMD-8111 SMBus 2.0 Controller"
PCI\VEN_1022&DEV_746B.DeviceDesc = "AMD-8111 System Management Controller"

ATI_MFG = "ATI"
PCI\VEN_1002&DEV_4371.DeviceDesc = "ATI I/O Communications Processor PCI Bus Controller"
PCI\VEN_1002&DEV_4372.DeviceDesc = "ATI I/O Communications Processor SMBus Controller"
PCI\VEN_1002&DEV_4377.DeviceDesc = "ATI I/O Communications Processor LPC Controller"
PCI\VEN_1002&DEV_4384.DeviceDesc = "ATI I/O Communications Processor PCI Bus Controller"
PCI\VEN_1002&DEV_4385.DeviceDesc = "ATI I/O Communications Processor SMBus Controller"
PCI\VEN_1002&DEV_438D.DeviceDesc = "ATI I/O Communications Processor LPC Controller"

COMPAQ_MFG="Compaq"
PCI\VEN_0E11&DEV_0001.DeviceDesc         = "Compaq PCI to EISA bridge"
PCI\VEN_0E11&DEV_0002.DeviceDesc         = "Compaq PCI to ISA bridge"
PCI\VEN_0E11&DEV_1000.DeviceDesc         = "Compaq CPU to PCI bridge [original model 1000]"
PCI\VEN_0E11&DEV_2000.DeviceDesc         = "Compaq CPU to PCI bridge [original model 2000]"
PCI\VEN_0E11&DEV_AE29.DeviceDesc         = "Compaq MIS-L PCI to Internal ISA bridge"
PCI\VEN_0E11&DEV_AE2B.DeviceDesc         = "Compaq MIS-E PCI to ISA Plug and Play bridge"
PCI\VEN_0E11&DEV_A0F0.DeviceDesc         = "Compaq Advanced System Management Controller"
PCI\VEN_0E11&DEV_A0F3.DeviceDesc         = "Compaq OSB PCI to ISA Plug and Play bridge"
PCI\VEN_0E11&DEV_A0F7.DeviceDesc         = "Compaq PCI Hotplug Controller"
PCI\VEN_0E11&DEV_AE2A.DeviceDesc         = "Compaq MPC CPU to PCI bridge"
PCI\VEN_0E11&DEV_AE31.DeviceDesc         = "Compaq System Management Controller"
PCI\VEN_0E11&DEV_AE69.DeviceDesc         = "Compaq CETUS-L PCI to Internal ISA bridge"
PCI\VEN_0E11&DEV_AE6C&CC_0600.DeviceDesc = "Compaq DRACO CPU to PCI bridge"
PCI\VEN_0E11&DEV_AE6C&CC_0604.DeviceDesc = "Compaq DRACO PCI to PCI bridge"
PCI\VEN_0E11&DEV_AE6D.DeviceDesc         = "Compaq NorthStar CPU to PCI bridge"
PCI\VEN_8086&DEV_123F&SUBSYS_A2F90E11.DeviceDesc = "Compaq PCI Hotplug Controller"
*CPQA0EF.DeviceDesc                      = "Compaq Deskpro Thermal Sensor"
*CPQAE08.DeviceDesc                      = "Compaq Deskpro Thermal Sensor"
*CPQAE30.DeviceDesc                      = "Compaq Armada 4100 Family Mobile CD Expansion Unit"
*CPQAE3B.DeviceDesc                      = "Compaq Armada 4100 Family Convenience Base"
*CPQAE3C.DeviceDesc                      = "Compaq Armada 4100 Family Convenience Base W/Ethernet"
*CPQAE4A.DeviceDesc                      = "Compaq ArmadaStation"
*CPQAE4B.DeviceDesc                      = "Compaq Armada MiniStation T"
*CPQAE4C.DeviceDesc                      = "Compaq Armada MiniStation EX"
*CPQAE4D.DeviceDesc                      = "Compaq Armada MiniStation E"
*CPQAE53.DeviceDesc                      = "Compaq Armada 1500 Convenience Base"
*CPQAE54.DeviceDesc                      = "Compaq Armada 1500 10BaseT Ethernet Convenience Base"
*CPQAE55.DeviceDesc                      = "Compaq Armada 1500 100BaseT Ethernet Convenience Base"
*CPQB05F.DeviceDesc                      = "Compaq 10/100 BaseTX Ethernet Convenience Base II"
*CPQB118.DeviceDesc                      = "Compaq ArmadaStation EM"
*CPQB119.DeviceDesc                      = "Compaq Armada Convenience Base EM"
*CPQB11A.DeviceDesc                      = "Compaq Port Replicator EM"
*CPQFA1B.DeviceDesc                      = "Compaq Deskpro 486/50 system memory board"

CONTAQ_MFG = "CONTAQ"
PCI\VEN_1080&DEV_0600.DeviceDesc = "CONTAQ 82C596 CPU to PCI & PCI to ISA bridge [original model]"

CYRIX_MFG = "CYRIX"
PCI\VEN_1078&DEV_0000.DeviceDesc = "Cyrix Cx5520 Rev 0 PCI to ISA bridge"
PCI\VEN_1078&DEV_0002.DeviceDesc = "Cyrix Cx5520 Rev 1 PCI to ISA bridge"

DEC_MFG = "DEC"
PCI\VEN_1011&DEV_0001.DeviceDesc = "DEC 21050 PCI to PCI bridge"
PCI\VEN_1011&DEV_0021.DeviceDesc = "DEC 21052 PCI to PCI bridge"
PCI\VEN_1011&DEV_0022.DeviceDesc = "DEC 21150 PCI to PCI bridge"
PCI\VEN_1011&DEV_0024.DeviceDesc = "DEC 21152 PCI to PCI bridge"
PCI\VEN_1011&DEV_0025.DeviceDesc = "DEC 21153 PCI to PCI bridge"
PCI\VEN_1011&DEV_0026.DeviceDesc = "DEC 21154 PCI to PCI bridge"

HITACHI_MFG = "Hitachi"
PCI\VEN_1054&DEV_3005.DeviceDesc         = "Hitachi HA8000-ex/880 CPU to PCI bridge - NCA"
PCI\VEN_1054&DEV_3006.DeviceDesc         = "Hitachi HA8000-ex/880 CPU to PCI bridge - NCD"

HP_MFG = "Hewlett-Packard"
PCI\VEN_103C&DEV_10C1.DeviceDesc = "HP NetServer Smart IRQ Router"
PCI\VEN_103C&DEV_10ED.DeviceDesc = "HP TopTools Remote Control"
PCI\VEN_103C&DEV_1219.DeviceDesc = "HP NetServer PCI Hot-Plug Controller"
PCI\VEN_103C&DEV_121A.DeviceDesc = "HP NetServer SMIC Controller"
PCI\VEN_103C&DEV_121B.DeviceDesc = "HP NetServer Legacy COM Port Decoder"
PCI\VEN_103C&DEV_121C.DeviceDesc = "HP NetServer PCI COM Port Decoder"
HWPC209.DeviceDesc               = "HP Configuration Interface"

IBM_MFG = "IBM"
PCI\VEN_1014&DEV_000A.DeviceDesc        = "IBM PCI to ISA Plug and Play bridge"
PCI\VEN_1014&DEV_0017.DeviceDesc        = "IBM CPU to PCI bridge"
PCI\VEN_1014&DEV_0022&REV_00.DeviceDesc = "IBM 82351 PCI to PCI bridge"
PCI\VEN_1014&DEV_0022.DeviceDesc        = "IBM PCI to PCI bridge"
PCI\VEN_1014&DEV_0095.DeviceDesc        = "IBM 20H2999 PCI to PCI Docking bridge"
*IBM006A.DeviceDesc                     = "IBM ThinkPad Ultrabay Plus Carriage"

INTEL_MFG = "Intel"
*INT0800.DeviceDesc                      = "Intel(R) 82802 Firmware Hub Device"
*INT3350.DeviceDesc                      = "Intel(R) 460GX AGP"
PCI\VEN_8086&DEV_0008.DeviceDesc         = "Intel Extended Express System Support Controller"
PCI\VEN_8086&DEV_0040.DeviceDesc         = "Intel(R) processor DRAM Controller - 0040"
PCI\VEN_8086&DEV_0041.DeviceDesc         = "Intel(R) processor PCI Express Root Port - 0041"
PCI\VEN_8086&DEV_0050.DeviceDesc         = "Intel(R) processor Thermal Management Controller - 0050"
PCI\VEN_8086&DEV_0051.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family Performance Counters - 0051"
PCI\VEN_8086&DEV_0326.DeviceDesc         = "Intel(R) 6700/6702PXH I/OxAPIC Interrupt Controller A - 0326"
PCI\VEN_8086&DEV_0327.DeviceDesc         = "Intel(R) 6700PXH I/OxAPIC Interrupt Controller B - 0327"
PCI\VEN_8086&DEV_0329.DeviceDesc         = "Intel(R) 6700PXH PCI Express-to-PCI Bridge A - 0329"
PCI\VEN_8086&DEV_032A.DeviceDesc         = "Intel(R) 6700PXH PCI Express-to-PCI Bridge B - 032A"
PCI\VEN_8086&DEV_032C.DeviceDesc         = "Intel(R) 6702PXH PCI Express-to-PCI Bridge A - 032C"
PCI\VEN_8086&DEV_0330.DeviceDesc         = "Intel(R) 80332 PCI Express-to-PCI Bridge A - 0330"
PCI\VEN_8086&DEV_0331.DeviceDesc         = "Intel(R) 80332 I/OxAPIC Interrupt Controller A - 0331"
PCI\VEN_8086&DEV_0332.DeviceDesc         = "Intel(R) 80332 PCI Express-to-PCI Bridge B - 0332"
PCI\VEN_8086&DEV_0333.DeviceDesc         = "Intel(R) 80332 I/OxAPIC Interrupt Controller B - 0333"
PCI\VEN_8086&DEV_0334.DeviceDesc         = "Intel(R) 80332 Memory Controller - 0334"
PCI\VEN_8086&DEV_0370.DeviceDesc         = "Intel(R) 80333 PCI Express-to-PCI Bridge A - 0370"
PCI\VEN_8086&DEV_0371.DeviceDesc         = "Intel(R) 80333 I/OxAPIC Interrupt Controller A - 0371"
PCI\VEN_8086&DEV_0372.DeviceDesc         = "Intel(R) 80333 PCI Express-to-PCI Bridge B - 0372"
PCI\VEN_8086&DEV_0373.DeviceDesc         = "Intel(R) 80333 I/OxAPIC Interrupt Controller B - 0373"
PCI\VEN_8086&DEV_0374.DeviceDesc         = "Intel(R) 80333 Memory Controller - 0374"
PCI\VEN_8086&DEV_0482.DeviceDesc         = "Intel 82375EB/SB PCI to EISA bridge"
PCI\VEN_8086&DEV_0483.DeviceDesc         = "Intel 82420EX i486 CPU to PCI bridge"
PCI\VEN_8086&DEV_0484.DeviceDesc         = "Intel 82378 SIO PCI to ISA bridge"
PCI\VEN_8086&DEV_0486.DeviceDesc         = "Intel 82420EX i486 PCIset with ISA bridge"
PCI\VEN_8086&DEV_04A3_OLD.DeviceDesc     = "Intel 82434LX Pentium(R) Processor to PCI bridge"
PCI\VEN_8086&DEV_04A3.DeviceDesc         = "Intel 82434NX Pentium(R) Processor to PCI bridge"
PCI\VEN_8086&DEV_1130.DeviceDesc         = "Intel(R) 82815 Processor to I/O Controller - 1130"
PCI\VEN_8086&DEV_1131.DeviceDesc         = "Intel(R) 82815 Processor to AGP Controller - 1131"
PCI\VEN_8086&DEV_1161.DeviceDesc         = "Intel(R) 82806AA Advanced Programmable Interrupt Controller"
PCI\VEN_8086&DEV_1225.DeviceDesc         = "Intel Pentium(R) Extended Express Processor to PCI bridge"
PCI\VEN_8086&DEV_122D.DeviceDesc         = "Intel 82437FX Pentium(R) Processor to PCI bridge"
PCI\VEN_8086&DEV_122E.DeviceDesc         = "Intel 82371FB PCI to ISA bridge"
PCI\VEN_8086&DEV_1234.DeviceDesc         = "Intel 82371MX PCI to ISA bridge"
PCI\VEN_8086&DEV_1235.DeviceDesc         = "Intel 82437MX Pentium(R) Processor to PCI bridge"
PCI\VEN_8086&DEV_1237.DeviceDesc         = "Intel 82441FX Pentium(R) Pro Processor to PCI bridge"
PCI\VEN_8086&DEV_123B.DeviceDesc         = "Intel 82380PB PCI to PCI Docking bridge"
PCI\VEN_8086&DEV_123C.DeviceDesc         = "Intel 82380AB PCI to ISA docking bridge"
PCI\VEN_8086&DEV_123D.DeviceDesc         = "Intel (683053) Programmable Interrupt Device"
PCI\VEN_8086&DEV_123F.DeviceDesc         = "Intel WXB PCI Hotplug Controller"
PCI\VEN_8086&DEV_124B.DeviceDesc         = "Intel 82380FB PCI to PCI Docking Bridge"
PCI\VEN_8086&DEV_1250.DeviceDesc         = "Intel 82439HX Pentium(R) Processor to PCI bridge"
PCI\VEN_8086&DEV_1360.DeviceDesc         = "Intel(R) 82806AA PCI Bridge"
PCI\VEN_8086&DEV_1361.DeviceDesc         = "Intel(R) 82806AA Controller (reserved)"
PCI\VEN_8086&DEV_1460.DeviceDesc         = "Intel(R) P64H2 PCI to PCI Bridge - 1460"
PCI\VEN_8086&DEV_1461.DeviceDesc         = "Intel(R) P64H2 I/O Advanced Programmable Interrupt Controller - 1461"
PCI\VEN_8086&DEV_1462.DeviceDesc         = "Intel(R) P64H2 PCI Hot Plug Controller - 1462"
PCI\VEN_8086&DEV_1A21.DeviceDesc         = "Intel(R) 82840 Processor to I/O Controller"
PCI\VEN_8086&DEV_1A23.DeviceDesc         = "Intel(R) 82840 Processor to AGP Controller"
PCI\VEN_8086&DEV_1A24.DeviceDesc         = "Intel(R) 82840 PCI Bridge"
PCI\VEN_8086&DEV_1A30.DeviceDesc         = "Intel(R) 82845 Processor to I/O Controller - 1A30"
PCI\VEN_8086&DEV_1A31.DeviceDesc         = "Intel(R) 82845 Processor to AGP Controller - 1A31"
PCI\VEN_8086&DEV_1A38.DeviceDesc         = "Intel(R) 5000 Series Chipsets Integrated Device - 1A38"
PCI\VEN_8086&DEV_2410.DeviceDesc         = "Intel(R) 82801AA LPC Interface Controller"
PCI\VEN_8086&DEV_2413.DeviceDesc         = "Intel(R) 82801AA SMBus Controller"
PCI\VEN_8086&DEV_2418.DeviceDesc         = "Intel(R) 82801AA PCI Bridge"
PCI\VEN_8086&DEV_2420.DeviceDesc         = "Intel(R) 82801AB LPC Interface Controller"
PCI\VEN_8086&DEV_2423.DeviceDesc         = "Intel(R) 82801AB SMBus Controller"
PCI\VEN_8086&DEV_2428.DeviceDesc         = "Intel(R) 82801AB PCI Bridge"
PCI\VEN_8086&DEV_2440.DeviceDesc         = "Intel(R) 82801BA LPC Interface Controller - 2440"
PCI\VEN_8086&DEV_2443.DeviceDesc         = "Intel(R) 82801BA/BAM SMBus Controller - 2443"
PCI\VEN_8086&DEV_2448.DeviceDesc         = "Intel(R) 82801 PCI Bridge - 2448"
PCI\VEN_8086&DEV_244C.DeviceDesc         = "Intel(R) 82801BAM LPC Interface Controller - 244C"
PCI\VEN_8086&DEV_244E.DeviceDesc         = "Intel(R) 82801 PCI Bridge - 244E"
PCI\VEN_8086&DEV_2480.DeviceDesc         = "Intel(R) 82801CA LPC Interface Controller - 2480"
PCI\VEN_8086&DEV_2483.DeviceDesc         = "Intel(R) 82801CA/CAM SMBus Controller - 2483"
PCI\VEN_8086&DEV_248C.DeviceDesc         = "Intel(R) 82801CAM LPC Interface Controller - 248C"
PCI\VEN_8086&DEV_24C0.DeviceDesc         = "Intel(R) 82801DB LPC Interface Controller - 24C0"
PCI\VEN_8086&DEV_24C3.DeviceDesc         = "Intel(R) 82801DB/DBM SMBus Controller - 24C3"
PCI\VEN_8086&DEV_24CC.DeviceDesc         = "Intel(R) 82801DBM LPC Interface Controller - 24CC"
PCI\VEN_8086&DEV_24D0.DeviceDesc         = "Intel(R) 82801EB LPC Interface Controller - 24D0"
PCI\VEN_8086&DEV_24D3.DeviceDesc         = "Intel(R) 82801EB SMBus Controller - 24D3"
PCI\VEN_8086&DEV_24DC.DeviceDesc         = "Intel(R) 82801EB LPC Interface Controller - 24DC"
PCI\VEN_8086&DEV_2500.DeviceDesc         = "Intel(R) 82820 Processor to I/O Controller"
PCI\VEN_8086&DEV_2501.DeviceDesc         = "Intel(R) 82820 Processor to I/O Controller"
PCI\VEN_8086&DEV_250B.DeviceDesc         = "Intel(R) 82820 Processor to I/O Controller"
PCI\VEN_8086&DEV_250F.DeviceDesc         = "Intel(R) 82820 Processor to AGP Controller"
PCI\VEN_8086&DEV_2530.DeviceDesc         = "Intel(R) 82850 Processor to I/O Controller - 2530"
PCI\VEN_8086&DEV_2531.DeviceDesc         = "Intel(R) 82860 Processor to I/O Controller - 2531"
PCI\VEN_8086&DEV_2532.DeviceDesc         = "Intel(R) 82850/82860 Processor to AGP Controller - 2532"
PCI\VEN_8086&DEV_2533.DeviceDesc         = "Intel(R) 82860 PCI Bridge - 2533"
PCI\VEN_8086&DEV_2534.DeviceDesc         = "Intel(R) 82860 PCI Bridge - 2534"
PCI\VEN_8086&DEV_2540.DeviceDesc         = "Intel(R) E7500 Chipset Host Controller - 2540"
PCI\VEN_8086&DEV_2541.DeviceDesc         = "Intel(R) E7000 Series Host RASUM Controller - 2541"
PCI\VEN_8086&DEV_2543.DeviceDesc         = "Intel(R) E7000 Series Hub Interface B PCI-to-PCI Bridge - 2543"
PCI\VEN_8086&DEV_2544.DeviceDesc         = "Intel(R) E7000 Series Hub Interface B RASUM Controller - 2544"
PCI\VEN_8086&DEV_2545.DeviceDesc         = "Intel(R) E7000 Series Hub Interface C PCI-to-PCI Bridge - 2545"
PCI\VEN_8086&DEV_2546.DeviceDesc         = "Intel(R) E7000 Series Hub Interface C RASUM Controller - 2546"
PCI\VEN_8086&DEV_2547.DeviceDesc         = "Intel(R) E7000 Series Hub Interface D PCI-to-PCI Bridge - 2547"
PCI\VEN_8086&DEV_2548.DeviceDesc         = "Intel(R) E7000 Series Hub Interface D RASUM Controller - 2548"
PCI\VEN_8086&DEV_254C.DeviceDesc         = "Intel(R) E7501 Chipset Host Controller - 254C"
PCI\VEN_8086&DEV_2550.DeviceDesc         = "Intel(R) E7505 Chipset Host Controller - 2550"
PCI\VEN_8086&DEV_2551.DeviceDesc         = "Intel(R) E7000 Series RAS Controller - 2551"
PCI\VEN_8086&DEV_2552.DeviceDesc         = "Intel(R) E7000 Series Processor to AGP Controller - 2552"
PCI\VEN_8086&DEV_2553.DeviceDesc         = "Intel(R) E7000 Series Hub Interface B PCI-to-PCI Bridge - 2553"
PCI\VEN_8086&DEV_2554.DeviceDesc         = "Intel(R) E7000 Series Hub Interface B PCI-to-PCI Bridge RAS Controller - 2554"
PCI\VEN_8086&DEV_255D.DeviceDesc         = "Intel(R) E7205 Chipset Host Controller - 255D"
PCI\VEN_8086&DEV_2560.DeviceDesc         = "Intel(R) 82845G/GL/GE/PE/GV/E Processor to I/O Controller - 2560"
PCI\VEN_8086&DEV_2561.DeviceDesc         = "Intel(R) 82845G/GL/GE/PE/GV/E Processor to AGP Controller - 2561"
PCI\VEN_8086&DEV_2570.DeviceDesc         = "Intel(R) 82865G/PE/P/GV/82848P Processor to I/O Controller - 2570"
PCI\VEN_8086&DEV_2571.DeviceDesc         = "Intel(R) 82865G/PE/P/GV/82848P Processor to AGP Controller - 2571"
PCI\VEN_8086&DEV_2573.DeviceDesc         = "Intel(R) 82865G/PE/P/GV/82848P Processor to PCI to CSA bridge - 2573"
PCI\VEN_8086&DEV_2576.DeviceDesc         = "Intel(R) 82865G/PE/P/GV/82848P Processor to I/O Memory Interface - 2576"
PCI\VEN_8086&DEV_2578.DeviceDesc         = "Intel(R) 82875P/E7210 Memory Controller Hub - 2578"
PCI\VEN_8086&DEV_2579.DeviceDesc         = "Intel(R) 82875P Processor to AGP Controller - 2579"
PCI\VEN_8086&DEV_257B.DeviceDesc         = "Intel(R) 82875P/E7210 Processor to PCI to CSA bridge - 257B"
PCI\VEN_8086&DEV_257E.DeviceDesc         = "Intel(R) 82875P/E7210 Processor to I/O Memory Interface - 257E"
PCI\VEN_8086&DEV_2580.DeviceDesc         = "Intel(R) 915G/P/GV/GL/PL/910GE/GL Processor to I/O Controller - 2580"
PCI\VEN_8086&DEV_2581.DeviceDesc         = "Intel(R) 915G/P/GV/GL/PL/910GE/GL PCI Express Root Port - 2581"
PCI\VEN_8086&DEV_2584.DeviceDesc         = "Intel(R) 925X/XE Memory Controller Hub - 2584"
PCI\VEN_8086&DEV_2585.DeviceDesc         = "Intel(R) 925X/XE PCI Express Root Port - 2585"
PCI\VEN_8086&DEV_2588.DeviceDesc         = "Intel(R) E7220/E7221 Memory Controller Hub - 2588"
PCI\VEN_8086&DEV_2589.DeviceDesc         = "Intel(R) E7220/E7221 PCI Express Root Port - 2589"
PCI\VEN_8086&DEV_2590.DeviceDesc         = "Mobile Intel(R) 915GM/PM/GMS/910GML Express Processor to DRAM Controller - 2590"
PCI\VEN_8086&DEV_2591.DeviceDesc         = "Mobile Intel(R) 915GM/PM Express PCI Express Root Port - 2591"
PCI\VEN_8086&DEV_25A1.DeviceDesc         = "Intel(R) 6300ESB LPC Interface Controller - 25A1"
PCI\VEN_8086&DEV_25A4.DeviceDesc         = "Intel(R) 6300ESB SMBus Controller - 25A4"
PCI\VEN_8086&DEV_25AB.DeviceDesc         = "Intel(R) 6300ESB Watchdog Timer - 25AB"
PCI\VEN_8086&DEV_25AC.DeviceDesc         = "Intel(R) 6300ESB I/O Advanced Programmable Interrupt Controller - 25AC"
PCI\VEN_8086&DEV_25AE.DeviceDesc         = "Intel(R) 6300ESB 64-bit PCI-X Bridge - 25AE"
PCI\VEN_8086&DEV_25C0.DeviceDesc         = "Intel(R) 5000X Chipset Memory Controller Hub - 25C0"
PCI\VEN_8086&DEV_25D0.DeviceDesc         = "Intel(R) 5000Z Chipset Memory Controller Hub - 25D0"
PCI\VEN_8086&DEV_25D4.DeviceDesc         = "Intel(R) 5000V Chipset Memory Controller Hub - 25D4"
PCI\VEN_8086&DEV_25D8.DeviceDesc         = "Intel(R) 5000P Chipset Memory Controller Hub - 25D8"
PCI\VEN_8086&DEV_25E2.DeviceDesc         = "Intel(R) 5000 Series Chipset PCI Express x4 Port 2 - 25E2"
PCI\VEN_8086&DEV_25E3.DeviceDesc         = "Intel(R) 5000 Series Chipset PCI Express x4 Port 3 - 25E3"
PCI\VEN_8086&DEV_25E4.DeviceDesc         = "Intel(R) 5000 Series Chipset PCI Express x4 Port 4 - 25E4"
PCI\VEN_8086&DEV_25E5.DeviceDesc         = "Intel(R) 5000 Series Chipset PCI Express x4 Port 5 - 25E5"
PCI\VEN_8086&DEV_25E6.DeviceDesc         = "Intel(R) 5000 Series Chipset PCI Express x4 Port 6 - 25E6"
PCI\VEN_8086&DEV_25E7.DeviceDesc         = "Intel(R) 5000 Series Chipset PCI Express x4 Port 7 - 25E7"
PCI\VEN_8086&DEV_25F0.DeviceDesc         = "Intel(R) 5000 Series Chipset Error Reporting Registers - 25F0"
PCI\VEN_8086&DEV_25F1.DeviceDesc         = "Intel(R) 5000 Series Chipset Reserved Registers - 25F1"
PCI\VEN_8086&DEV_25F3.DeviceDesc         = "Intel(R) 5000 Series Chipset Reserved Registers - 25F3"
PCI\VEN_8086&DEV_25F5.DeviceDesc         = "Intel(R) 5000 Series Chipset FBD Registers - 25F5"
PCI\VEN_8086&DEV_25F6.DeviceDesc         = "Intel(R) 5000 Series Chipset FBD Registers - 25F6"
PCI\VEN_8086&DEV_25F7.DeviceDesc         = "Intel(R) 5000 Series Chipset PCI Express x8 Port 2-3 - 25F7"
PCI\VEN_8086&DEV_25F8.DeviceDesc         = "Intel(R) 5000 Series Chipset PCI Express x8 Port 4-5 - 25F8"
PCI\VEN_8086&DEV_25F9.DeviceDesc         = "Intel(R) 5000 Series Chipset PCI Express x8 Port 6-7 - 25F9"
PCI\VEN_8086&DEV_25FA.DeviceDesc         = "Intel(R) 5000X Chipset PCI Express x16 Port 4-7 - 25FA"
PCI\VEN_8086&DEV_2600.DeviceDesc         = "Intel(R) E8500/E8501 Hub Interface - 2600"
PCI\VEN_8086&DEV_2601.DeviceDesc         = "Intel(R) E8500/E8501 PCI Express x4 Port D - 2601"
PCI\VEN_8086&DEV_2602.DeviceDesc         = "Intel(R) E8500/E8501 PCI Express x4 Port C0 - 2602"
PCI\VEN_8086&DEV_2603.DeviceDesc         = "Intel(R) E8500/E8501 PCI Express x4 Port C1 - 2603"
PCI\VEN_8086&DEV_2604.DeviceDesc         = "Intel(R) E8500/E8501 PCI Express x4 Port B0 - 2604"
PCI\VEN_8086&DEV_2605.DeviceDesc         = "Intel(R) E8500/E8501 PCI Express x4 Port B1 - 2605"
PCI\VEN_8086&DEV_2606.DeviceDesc         = "Intel(R) E8500/E8501 PCI Express x4 Port A0 - 2606"
PCI\VEN_8086&DEV_2607.DeviceDesc         = "Intel(R) E8500/E8501 PCI Express x4 Port A1 - 2607"
PCI\VEN_8086&DEV_2608.DeviceDesc         = "Intel(R) E8500/E8501 PCI Express x8 Port C - 2608"
PCI\VEN_8086&DEV_2609.DeviceDesc         = "Intel(R) E8500/E8501 PCI Express x8 Port B - 2609"
PCI\VEN_8086&DEV_260A.DeviceDesc         = "Intel(R) E8500/E8501 PCI Express x8 Port A - 260A"
PCI\VEN_8086&DEV_260C.DeviceDesc         = "Intel(R) E8500/E8501 IMI Registers - 260C"
PCI\VEN_8086&DEV_2610.DeviceDesc         = "Intel(R) E8500/E8501 Interrupt Registers - 2610"
PCI\VEN_8086&DEV_2611.DeviceDesc         = "Intel(R) E8500/E8501 Address Mapping Registers - 2611"
PCI\VEN_8086&DEV_2612.DeviceDesc         = "Intel(R) E8500/E8501 RAS Registers - 2612"
PCI\VEN_8086&DEV_2613.DeviceDesc         = "Intel(R) E8500/E8501 Registers - 2613"
PCI\VEN_8086&DEV_2614.DeviceDesc         = "Intel(R) E8500/E8501 Registers - 2614"
PCI\VEN_8086&DEV_2615.DeviceDesc         = "Intel(R) E8500/E8501 Registers - 2615"
PCI\VEN_8086&DEV_2617.DeviceDesc         = "Intel(R) E8500/E8501 Registers - 2617"
PCI\VEN_8086&DEV_2618.DeviceDesc         = "Intel(R) E8500/E8501 Registers - 2618"
PCI\VEN_8086&DEV_2619.DeviceDesc         = "Intel(R) E8500/E8501 Registers - 2619"
PCI\VEN_8086&DEV_261A.DeviceDesc         = "Intel(R) E8500/E8501 Registers - 261A"
PCI\VEN_8086&DEV_261B.DeviceDesc         = "Intel(R) E8500/E8501 Registers - 261B"
PCI\VEN_8086&DEV_261C.DeviceDesc         = "Intel(R) E8500/E8501 Registers - 261C"
PCI\VEN_8086&DEV_261D.DeviceDesc         = "Intel(R) E8500/E8501 Registers - 261D"
PCI\VEN_8086&DEV_261E.DeviceDesc         = "Intel(R) E8500/E8501 Registers - 261E"
PCI\VEN_8086&DEV_2620.DeviceDesc         = "Intel(R) E8500/E8501 External Memory Bridge - 2620"
PCI\VEN_8086&DEV_2621.DeviceDesc         = "Intel(R) E8500/E8501 XMB Control Registers - 2621"
PCI\VEN_8086&DEV_2622.DeviceDesc         = "Intel(R) E8500/E8501 XMB Memory Interleaving Registers - 2622"
PCI\VEN_8086&DEV_2623.DeviceDesc         = "Intel(R) E8500/E8501 XMB DDR Initialization and Calibration - 2623"
PCI\VEN_8086&DEV_2624.DeviceDesc         = "Intel(R) E8500/E8501 XMB Registers - 2624"
PCI\VEN_8086&DEV_2625.DeviceDesc         = "Intel(R) E8500/E8501 XMB Registers - 2625"
PCI\VEN_8086&DEV_2626.DeviceDesc         = "Intel(R) E8500/E8501 XMB Registers - 2626"
PCI\VEN_8086&DEV_2627.DeviceDesc         = "Intel(R) E8500/E8501 XMB Registers - 2627"
PCI\VEN_8086&DEV_2640.DeviceDesc         = "Intel(R) 82801FB LPC Interface Controller - 2640"
PCI\VEN_8086&DEV_2641.DeviceDesc         = "Intel(R) 82801FBM LPC Interface Controller - 2641"
PCI\VEN_8086&DEV_2642.DeviceDesc         = "Intel(R) 82801FB LPC Interface Controller - 2642"
PCI\VEN_8086&DEV_2660.DeviceDesc         = "Intel(R) 82801FB/FBM PCI Express Root Port - 2660"
PCI\VEN_8086&DEV_2662.DeviceDesc         = "Intel(R) 82801FB/FBM PCI Express Root Port - 2662"
PCI\VEN_8086&DEV_2664.DeviceDesc         = "Intel(R) 82801FB/FBM PCI Express Root Port - 2664"
PCI\VEN_8086&DEV_2666.DeviceDesc         = "Intel(R) 82801FB/FBM PCI Express Root Port - 2666"
PCI\VEN_8086&DEV_266A.DeviceDesc         = "Intel(R) 82801FB/FBM SMBus Controller - 266A"
PCI\VEN_8086&DEV_2670.DeviceDesc         = "Intel(R) 631xESB/6321ESB/3100 Chipset LPC Interface Controller - 2670"
PCI\VEN_8086&DEV_2690.DeviceDesc         = "Intel(R) 631xESB/6321ESB/3100 Chipset PCI Express Root Port 1 - 2690"
PCI\VEN_8086&DEV_2692.DeviceDesc         = "Intel(R) 631xESB/6321ESB/3100 Chipset PCI Express Root Port 2 - 2692"
PCI\VEN_8086&DEV_2694.DeviceDesc         = "Intel(R) 631xESB/6321ESB/3100 Chipset PCI Express Root Port 3 - 2694"
PCI\VEN_8086&DEV_2696.DeviceDesc         = "Intel(R) 631xESB/6321ESB/3100 Chipset PCI Express Root Port 4 - 2696"
PCI\VEN_8086&DEV_269B.DeviceDesc         = "Intel(R) 631xESB/6321ESB/3100 Chipset SMBus Controller - 269B"
PCI\VEN_8086&DEV_2770.DeviceDesc         = "Intel(R) 945G/GZ/GC/P/PL Processor to I/O Controller - 2770"
PCI\VEN_8086&DEV_2771.DeviceDesc         = "Intel(R) 945G/GZ/GC/P/PL PCI Express Root Port - 2771"
PCI\VEN_8086&DEV_2774.DeviceDesc         = "Intel(R) 955X Memory Controller Hub - 2774"
PCI\VEN_8086&DEV_2775.DeviceDesc         = "Intel(R) 955X PCI Express Root Port - 2775"
PCI\VEN_8086&DEV_2778.DeviceDesc         = "Intel(R) E7230/3000/3010 Processor to I/O Controller - 2778"
PCI\VEN_8086&DEV_2779.DeviceDesc         = "Intel(R) E7230/3000/3010 PCI Express Root Port - 2779"
PCI\VEN_8086&DEV_277A.DeviceDesc         = "Intel(R) 975X/3010 PCI Express Root Port - 277A"
PCI\VEN_8086&DEV_277C.DeviceDesc         = "Intel(R) 975X Memory Controller Hub - 277C"
PCI\VEN_8086&DEV_277D.DeviceDesc         = "Intel(R) 975X PCI Express Root Port - 277D"
PCI\VEN_8086&DEV_27A0.DeviceDesc         = "Mobile Intel(R) 945GM/GU/PM/GMS/940GML/943GML and Intel(R) 945GT Express Processor to DRAM Controller - 27A0"
PCI\VEN_8086&DEV_27A1.DeviceDesc         = "Mobile Intel(R) 945GM/GU/PM/GMS/940GML/943GML and Intel(R) 945GT Express PCI Express Root Port - 27A1"
PCI\VEN_8086&DEV_27AC.DeviceDesc         = "Mobile Intel(R) 945GME Express Processor to DRAM Controller - 27AC"
PCI\VEN_8086&DEV_27AD.DeviceDesc         = "Mobile Intel(R) 945GME Express PCI Express Root Port - 27AD"
PCI\VEN_8086&DEV_27B0.DeviceDesc         = "Intel(R) 82801GH (ICH7DH) LPC Interface Controller - 27B0"
PCI\VEN_8086&DEV_27B8.DeviceDesc         = "Intel(R) 82801GB/GR (ICH7 Family) LPC Interface Controller - 27B8"
PCI\VEN_8086&DEV_27B9.DeviceDesc         = "Intel(R) 82801GBM (ICH7-M/U) LPC Interface Controller - 27B9"
PCI\VEN_8086&DEV_27BC.DeviceDesc         = "Intel(R) N10 Family LPC Interface Controller - 27BC"
PCI\VEN_8086&DEV_27BD.DeviceDesc         = "Intel(R) 82801GHM (ICH7-M/U DH) LPC Interface Controller - 27BD"
PCI\VEN_8086&DEV_27DA.DeviceDesc         = "Intel(R) 82801G (ICH7 Family) SMBus Controller - 27DA"
PCI\VEN_8086&DEV_27D0.DeviceDesc         = "Intel(R) 82801G (ICH7 Family) PCI Express Root Port - 27D0"
PCI\VEN_8086&DEV_27D2.DeviceDesc         = "Intel(R) 82801G (ICH7 Family) PCI Express Root Port - 27D2"
PCI\VEN_8086&DEV_27D4.DeviceDesc         = "Intel(R) 82801G (ICH7 Family) PCI Express Root Port - 27D4"
PCI\VEN_8086&DEV_27D6.DeviceDesc         = "Intel(R) 82801G (ICH7 Family) PCI Express Root Port - 27D6"
PCI\VEN_8086&DEV_27E0.DeviceDesc         = "Intel(R) 82801GR/GH/GHM (ICH7 Family) PCI Express Root Port - 27E0"
PCI\VEN_8086&DEV_27E2.DeviceDesc         = "Intel(R) 82801GR/GH/GHM (ICH7 Family) PCI Express Root Port - 27E2"
PCI\VEN_8086&DEV_2810.DeviceDesc         = "Intel(R) ICH8/ICH8R Family LPC Interface Controller - 2810"
PCI\VEN_8086&DEV_2811.DeviceDesc         = "Intel(R) ICH8M-E LPC Interface Controller - 2811"
PCI\VEN_8086&DEV_2812.DeviceDesc         = "Intel(R) ICH8DH LPC Interface Controller - 2812"
PCI\VEN_8086&DEV_2814.DeviceDesc         = "Intel(R) ICH8DO LPC Interface Controller - 2814"
PCI\VEN_8086&DEV_2815.DeviceDesc         = "Intel(R) ICH8M LPC Interface Controller - 2815"
PCI\VEN_8086&DEV_283E.DeviceDesc         = "Intel(R) ICH8 Family SMBus Controller - 283E"
PCI\VEN_8086&DEV_283F.DeviceDesc         = "Intel(R) ICH8 Family PCI Express Root Port 1 - 283F"
PCI\VEN_8086&DEV_2841.DeviceDesc         = "Intel(R) ICH8 Family PCI Express Root Port 2 - 2841"
PCI\VEN_8086&DEV_2843.DeviceDesc         = "Intel(R) ICH8 Family PCI Express Root Port 3 - 2843"
PCI\VEN_8086&DEV_2845.DeviceDesc         = "Intel(R) ICH8 Family PCI Express Root Port 4 - 2845"
PCI\VEN_8086&DEV_2847.DeviceDesc         = "Intel(R) ICH8 Family PCI Express Root Port 5 - 2847"
PCI\VEN_8086&DEV_2849.DeviceDesc         = "Intel(R) ICH8 Family PCI Express Root Port 6 - 2849"
PCI\VEN_8086&DEV_284F.DeviceDesc         = "Intel(R) ICH8 Family Thermal Reporting Device - 284F"
PCI\VEN_8086&DEV_2910.DeviceDesc         = "Intel(R) ICH9 LPC Interface Controller - 2910"
PCI\VEN_8086&DEV_2911.DeviceDesc         = "Intel(R) ICH9M LPC Interface Controller - 2911"
PCI\VEN_8086&DEV_2912.DeviceDesc         = "Intel(R) ICH9DH LPC Interface Controller - 2912"
PCI\VEN_8086&DEV_2914.DeviceDesc         = "Intel(R) ICH9DO LPC Interface Controller - 2914"
PCI\VEN_8086&DEV_2916.DeviceDesc         = "Intel(R) ICH9R LPC Interface Controller - 2916"
PCI\VEN_8086&DEV_2917.DeviceDesc         = "Intel(R) ICH9M-E LPC Interface Controller - 2917"
PCI\VEN_8086&DEV_2918.DeviceDesc         = "Intel(R) ICH9 LPC Interface Controller - 2918"
PCI\VEN_8086&DEV_2919.DeviceDesc         = "Intel(R) ICH9M LPC Interface Controller - 2919"
PCI\VEN_8086&DEV_2930.DeviceDesc         = "Intel(R) ICH9 Family SMBus Controller - 2930"
PCI\VEN_8086&DEV_2932.DeviceDesc         = "Intel(R) ICH9 Family Thermal Subsystem - 2932"
PCI\VEN_8086&DEV_2940.DeviceDesc         = "Intel(R) ICH9 Family PCI Express Root Port 1 - 2940"
PCI\VEN_8086&DEV_2942.DeviceDesc         = "Intel(R) ICH9 Family PCI Express Root Port 2 - 2942"
PCI\VEN_8086&DEV_2944.DeviceDesc         = "Intel(R) ICH9 Family PCI Express Root Port 3 - 2944"
PCI\VEN_8086&DEV_2946.DeviceDesc         = "Intel(R) ICH9 Family PCI Express Root Port 4 - 2946"
PCI\VEN_8086&DEV_2948.DeviceDesc         = "Intel(R) ICH9 Family PCI Express Root Port 5 - 2948"
PCI\VEN_8086&DEV_294A.DeviceDesc         = "Intel(R) ICH9 Family PCI Express Root Port 6 - 294A"
PCI\VEN_8086&DEV_2970.DeviceDesc         = "Intel(R) 946GZ/PL/GL Processor to I/O Controller - 2970"
PCI\VEN_8086&DEV_2971.DeviceDesc         = "Intel(R) 946GZ/PL/GL PCI Express Root Port - 2971"
PCI\VEN_8086&DEV_2980.DeviceDesc         = "Intel(R) G35 Express Chipset Processor to I/O Controller - 2980"
PCI\VEN_8086&DEV_2981.DeviceDesc         = "Intel(R) G35 Express Chipset PCI Express Root Port - 2981"
PCI\VEN_8086&DEV_2990.DeviceDesc         = "Intel(R) Q963/Q965 Processor to I/O Controller - 2990"
PCI\VEN_8086&DEV_2991.DeviceDesc         = "Intel(R) Q963/Q965 PCI Express Root Port - 2991"
PCI\VEN_8086&DEV_29A0.DeviceDesc         = "Intel(R) P965/G965 Processor to I/O Controller - 29A0"
PCI\VEN_8086&DEV_29A1.DeviceDesc         = "Intel(R) P965/G965 PCI Express Root Port - 29A1"
PCI\VEN_8086&DEV_29B0.DeviceDesc         = "Intel(R) Q35 Express Chipset Processor to I/O Controller - 29B0"
PCI\VEN_8086&DEV_29B1.DeviceDesc         = "Intel(R) Q35 Express Chipset PCI Express Root Port - 29B1"
PCI\VEN_8086&DEV_29C0.DeviceDesc         = "Intel(R) G33/G31/P35/P31 Express Chipset Processor to I/O Controller - 29C0"
PCI\VEN_8086&DEV_29C1.DeviceDesc         = "Intel(R) G33/G31/P35/P31 Express Chipset PCI Express Root Port - 29C1"
PCI\VEN_8086&DEV_29D0.DeviceDesc         = "Intel(R) Q33 Express Chipset Processor to I/O Controller - 29D0"
PCI\VEN_8086&DEV_29D1.DeviceDesc         = "Intel(R) Q33 Express Chipset PCI Express Root Port - 29D1"
PCI\VEN_8086&DEV_29E0.DeviceDesc         = "Intel(R) X38/X48 Express Chipset Processor to I/O Controller - 29E0"
PCI\VEN_8086&DEV_29E1.DeviceDesc         = "Intel(R) X38/X48 Express Chipset PCI Express Root Port - 29E1"
PCI\VEN_8086&DEV_29E9.DeviceDesc         = "Intel(R) X38/X48 Express Chipset PCI Express Root Port - 29E9"
PCI\VEN_8086&DEV_29F0.DeviceDesc         = "Intel(R) 3200/3210 Chipset DRAM Controller - 29F0"
PCI\VEN_8086&DEV_29F1.DeviceDesc         = "Intel(R) 3200/3210 Chipset Host-Primary PCI Express Bridge - 29F1"
PCI\VEN_8086&DEV_29F9.DeviceDesc         = "Intel(R) 3210 Chipset Host-Secondary PCI Express Bridge - 29F9"
PCI\VEN_8086&DEV_2A00.DeviceDesc         = "Mobile Intel(R) PM965/GM965/GL960/GS965 Express Processor to DRAM Controller - 2A00"
PCI\VEN_8086&DEV_2A01.DeviceDesc         = "Mobile Intel(R) PM965/GM965/GL960/GS965 Express PCI Express Root Port - 2A01"
PCI\VEN_8086&DEV_2A09.DeviceDesc         = "Intel(R) Performance Counters - 2A09"
PCI\VEN_8086&DEV_2A10.DeviceDesc         = "Mobile Intel(R) GME965/GLE960 Express Processor to DRAM Controller - 2A10"
PCI\VEN_8086&DEV_2A11.DeviceDesc         = "Mobile Intel(R) GME965/GLE960 Express PCI Express Root Port - 2A11"
PCI\VEN_8086&DEV_2A19.DeviceDesc         = "Intel(R) Performance Counters - 2A19"
PCI\VEN_8086&DEV_2A29.DeviceDesc         = "Intel(R) Performance Counters - 2A29"
PCI\VEN_8086&DEV_2A39.DeviceDesc         = "Intel(R) Performance Counters - 2A39"
PCI\VEN_8086&DEV_2A40.DeviceDesc         = "Mobile Intel(R) 4 Series Chipset Processor to DRAM Controller - 2A40"
PCI\VEN_8086&DEV_2A41.DeviceDesc         = "Mobile Intel(R) 4 Series Chipset PCI Express Root Port - 2A41"
PCI\VEN_8086&DEV_2A49.DeviceDesc         = "Intel(R) Performance Counters - 2A49"
PCI\VEN_8086&DEV_2A59.DeviceDesc         = "Intel(R) Performance Counters - 2A59"
PCI\VEN_8086&DEV_2A69.DeviceDesc         = "Intel(R) Performance Counters - 2A69"
PCI\VEN_8086&DEV_2A79.DeviceDesc         = "Intel(R) Performance Counters - 2A79"
PCI\VEN_8086&DEV_2A89.DeviceDesc         = "Intel(R) Performance Counters - 2A89"
PCI\VEN_8086&DEV_2A99.DeviceDesc         = "Intel(R) Performance Counters - 2A99"
PCI\VEN_8086&DEV_2AA9.DeviceDesc         = "Intel(R) Performance Counters - 2AA9"
PCI\VEN_8086&DEV_2AB9.DeviceDesc         = "Intel(R) Performance Counters - 2AB9"
PCI\VEN_8086&DEV_2AC9.DeviceDesc         = "Intel(R) Performance Counters - 2AC9"
PCI\VEN_8086&DEV_2AD9.DeviceDesc         = "Intel(R) Performance Counters - 2AD9"
PCI\VEN_8086&DEV_2AE9.DeviceDesc         = "Intel(R) Performance Counters - 2AE9"
PCI\VEN_8086&DEV_2AF9.DeviceDesc         = "Intel(R) Performance Counters - 2AF9"
PCI\VEN_8086&DEV_2B00.DeviceDesc         = "System Configuration Controller Interrupt - 2B00"
PCI\VEN_8086&DEV_2B02.DeviceDesc         = "System Configuration Controller Serial Interface - 2B02"
PCI\VEN_8086&DEV_2B68.DeviceDesc         = "System Configuration Controller Firmware - 2B68"
PCI\VEN_8086&DEV_2B6A.DeviceDesc         = "System Configuration Controller Error Control - 2B6A"
PCI\VEN_8086&DEV_2B04.DeviceDesc         = "Power Controller - 2B04"
PCI\VEN_8086&DEV_2B08.DeviceDesc         = "Caching Agent 0 - 2B08"
PCI\VEN_8086&DEV_2B0C.DeviceDesc         = "Caching Agent 1 - 2B0C"
PCI\VEN_8086&DEV_2B10.DeviceDesc         = "Intel(R) QPI Home Agent 0 - 2B10"
PCI\VEN_8086&DEV_2B14.DeviceDesc         = "Memory Controller 0 - 2B14"
PCI\VEN_8086&DEV_2B16.DeviceDesc         = "Memory Controller 0 - 2B16"
PCI\VEN_8086&DEV_2B13.DeviceDesc         = "Memory Controller 0 - 2B13"
PCI\VEN_8086&DEV_2B18.DeviceDesc         = "Intel(R) QPI Home Agent - 2B18"
PCI\VEN_8086&DEV_2B1C.DeviceDesc         = "Memory Controller 1 - 2B1C"
PCI\VEN_8086&DEV_2B1E.DeviceDesc         = "Memory Controller 1 - 2B1E"
PCI\VEN_8086&DEV_2B1B.DeviceDesc         = "Memory Controller 1 - 2B1B"
PCI\VEN_8086&DEV_2B20.DeviceDesc         = "Last Level Cache Coherence Engine 0 - 2B20"
PCI\VEN_8086&DEV_2B24.DeviceDesc         = "Last Level Cache Coherence Engine 1 - 2B24"
PCI\VEN_8086&DEV_2B28.DeviceDesc         = "Last Level Cache Coherence Engine 2 - 2B28"
PCI\VEN_8086&DEV_2B2C.DeviceDesc         = "Last Level Cache Coherence Engine 3 - 2B2C"
PCI\VEN_8086&DEV_2B30.DeviceDesc         = "Last Level Cache Coherence Engine 4 - 2B30"
PCI\VEN_8086&DEV_2B34.DeviceDesc         = "Last Level Cache Coherence Engine 5 - 2B34"
PCI\VEN_8086&DEV_2B38.DeviceDesc         = "Last Level Cache Coherence Engine 6 - 2B38"
PCI\VEN_8086&DEV_2B3C.DeviceDesc         = "Last Level Cache Coherence Engine 7 - 2B3C"
PCI\VEN_8086&DEV_2B40.DeviceDesc         = "Intel(R) QuickPath Interconnect Router Port 0-1 - 2B40"
PCI\VEN_8086&DEV_2B42.DeviceDesc         = "Intel(R) QuickPath Interconnect Router Port 2-3 - 2B42"
PCI\VEN_8086&DEV_2B44.DeviceDesc         = "Intel(R) QuickPath Interconnect Router Port 4-5 - 2B44"
PCI\VEN_8086&DEV_2B46.DeviceDesc         = "Intel(R) QuickPath Interconnect Router Port 6-7 - 2B46"
PCI\VEN_8086&DEV_2B48.DeviceDesc         = "Test and Debug 0 - 2B48"
PCI\VEN_8086&DEV_2B4C.DeviceDesc         = "Test and Debug 1 - 2B4C"
PCI\VEN_8086&DEV_2B50.DeviceDesc         = "Intel(R) QPI Physical port 0 - 2B50"
PCI\VEN_8086&DEV_2B52.DeviceDesc         = "Intel(R) QPI Physical port 0 - 2B52"
PCI\VEN_8086&DEV_2B54.DeviceDesc         = "Intel(R) QPI Physical port 1 - 2B54"
PCI\VEN_8086&DEV_2B56.DeviceDesc         = "Intel(R) QPI Physical port 1 - 2B56"
PCI\VEN_8086&DEV_2B58.DeviceDesc         = "Intel(R) QPI Physical port 2 - 2B58"
PCI\VEN_8086&DEV_2B5A.DeviceDesc         = "Intel(R) QPI Physical port 2 - 2B5A"
PCI\VEN_8086&DEV_2B5C.DeviceDesc         = "Intel(R) QPI Physical port 3 - 2B5C"
PCI\VEN_8086&DEV_2B5E.DeviceDesc         = "Intel(R) QPI Physical port 3 - 2B5E"
PCI\VEN_8086&DEV_2B60.DeviceDesc         = "Intel(R) SMI Physical port 0 - 2B60"
PCI\VEN_8086&DEV_2B62.DeviceDesc         = "Intel(R) SMI Physical port 0 - 2B62"
PCI\VEN_8086&DEV_2B64.DeviceDesc         = "Intel(R) SMI Physical port 1 - 2B64"
PCI\VEN_8086&DEV_2B66.DeviceDesc         = "Intel(R) SMI Physical port 1 - 2B66"
PCI\VEN_8086&DEV_2C01.DeviceDesc         = "Intel(R) QuickPath Architecture System Address Decoder - 2C01"
PCI\VEN_8086&DEV_2C10.DeviceDesc         = "Intel(R) QuickPath Interconnect Link 0 - 2C10"
PCI\VEN_8086&DEV_2C11.DeviceDesc         = "Intel(R) QuickPath Interconnect Physical 0 - 2C11"
PCI\VEN_8086&DEV_2C14.DeviceDesc         = "Intel(R) QuickPath Interconnect Link 1 - 2C14"
PCI\VEN_8086&DEV_2C15.DeviceDesc         = "Intel(R) QuickPath Interconnect Physical 1 - 2C15"
PCI\VEN_8086&DEV_2C18.DeviceDesc         = "Integrated Memory Controller - 2C18"
PCI\VEN_8086&DEV_2C19.DeviceDesc         = "Integrated Memory Controller Target Address Decoder - 2C19"
PCI\VEN_8086&DEV_2C1A.DeviceDesc         = "Integrated Memory Controller RAS Registers - 2C1A"
PCI\VEN_8086&DEV_2C1C.DeviceDesc         = "Integrated Memory Controller Test Registers - 2C1C"
PCI\VEN_8086&DEV_2C20.DeviceDesc         = "Integrated Memory Controller Channel 0 Control Registers - 2C20"
PCI\VEN_8086&DEV_2C21.DeviceDesc         = "Integrated Memory Controller Channel 0 Address Registers - 2C21"
PCI\VEN_8086&DEV_2C22.DeviceDesc         = "Integrated Memory Controller Channel 0 Rank Registers - 2C22"
PCI\VEN_8086&DEV_2C23.DeviceDesc         = "Integrated Memory Controller Channel 0 Thermal Control Registers - 2C23"
PCI\VEN_8086&DEV_2C28.DeviceDesc         = "Integrated Memory Controller Channel 1 Control Registers - 2C28"
PCI\VEN_8086&DEV_2C29.DeviceDesc         = "Integrated Memory Controller Channel 1 Address Registers - 2C29"
PCI\VEN_8086&DEV_2C2A.DeviceDesc         = "Integrated Memory Controller Channel 1 Rank Registers - 2C2A"
PCI\VEN_8086&DEV_2C2B.DeviceDesc         = "Integrated Memory Controller Channel 1 Thermal Control Registers - 2C2B"
PCI\VEN_8086&DEV_2C30.DeviceDesc         = "Integrated Memory Controller Channel 2 Control Registers - 2C30"
PCI\VEN_8086&DEV_2C31.DeviceDesc         = "Integrated Memory Controller Channel 2 Address Registers - 2C31"
PCI\VEN_8086&DEV_2C32.DeviceDesc         = "Integrated Memory Controller Channel 2 Rank Registers - 2C32"
PCI\VEN_8086&DEV_2C33.DeviceDesc         = "Integrated Memory Controller Channel 2 Thermal Control Registers - 2C33"
PCI\VEN_8086&DEV_2C40.DeviceDesc         = "Intel(R) QuickPath Architecture Generic Non-Core Registers - 2C40"
PCI\VEN_8086&DEV_2C41.DeviceDesc         = "Intel(R) QuickPath Architecture Generic Non-Core Registers - 2C41"
PCI\VEN_8086&DEV_2C50.DeviceDesc         = "Intel(R) QuickPath Architecture Generic Non-Core Registers - 2C50"
PCI\VEN_8086&DEV_2C51.DeviceDesc         = "Intel(R) QuickPath Architecture Generic Non-Core Registers - 2C51"
PCI\VEN_8086&DEV_2C52.DeviceDesc         = "Intel(R) QuickPath Architecture Generic Non-Core Registers - 2C52"
PCI\VEN_8086&DEV_2C53.DeviceDesc         = "Intel(R) QuickPath Architecture Generic Non-Core Registers - 2C53"
PCI\VEN_8086&DEV_2C54.DeviceDesc         = "Intel(R) QuickPath Architecture Generic Non-Core Registers - 2C54"
PCI\VEN_8086&DEV_2C55.DeviceDesc         = "Intel(R) QuickPath Architecture Generic Non-Core Registers - 2C55"
PCI\VEN_8086&DEV_2C56.DeviceDesc         = "Intel(R) QuickPath Architecture Generic Non-Core Registers - 2C56"
PCI\VEN_8086&DEV_2C57.DeviceDesc         = "Intel(R) QuickPath Architecture Generic Non-Core Registers - 2C57"
PCI\VEN_8086&DEV_2C81.DeviceDesc         = "Intel(R) QuickPath Architecture System Address Decoder - 2C81"
PCI\VEN_8086&DEV_2C90.DeviceDesc         = "Intel(R) QPI Link - 2C90"
PCI\VEN_8086&DEV_2C91.DeviceDesc         = "Intel(R) QPI Physical 0 - 2C91"
PCI\VEN_8086&DEV_2C98.DeviceDesc         = "Intel(R) processor Integrated Memory Controller - 2C98"
PCI\VEN_8086&DEV_2C99.DeviceDesc         = "Intel(R) processor Integrated Memory Controller Target Address Decoder - 2C99"
PCI\VEN_8086&DEV_2C9C.DeviceDesc         = "Intel(R) processor Integrated Memory Controller Test Registers - 2C9C"
PCI\VEN_8086&DEV_2CA0.DeviceDesc         = "Intel(R) processor Integrated Memory Controller Channel 0 Control Registers - 2CA0"
PCI\VEN_8086&DEV_2CA1.DeviceDesc         = "Intel(R) processor Integrated Memory Controller Channel 0 Address Registers - 2CA1"
PCI\VEN_8086&DEV_2CA2.DeviceDesc         = "Intel(R) processor Integrated Memory Controller Channel 0 Rank Registers - 2CA2"
PCI\VEN_8086&DEV_2CA3.DeviceDesc         = "Intel(R) processor Integrated Memory Controller Channel 0 Thermal Control Registers - 2CA3"
PCI\VEN_8086&DEV_2CA8.DeviceDesc         = "Intel(R) processor Integrated Memory Controller Channel 1 Control Registers - 2CA8"
PCI\VEN_8086&DEV_2CA9.DeviceDesc         = "Intel(R) processor Integrated Memory Controller Channel 1 Address Registers - 2CA9"
PCI\VEN_8086&DEV_2CAA.DeviceDesc         = "Intel(R) processor Integrated Memory Controller Channel 1 Rank Registers - 2CAA"
PCI\VEN_8086&DEV_2CAB.DeviceDesc         = "Intel(R) processor Integrated Memory Controller Channel 1 Thermal Control Registers - 2CAB"
PCI\VEN_8086&DEV_2E00.DeviceDesc         = "Intel(R) 4 Series Chipset Processor to I/O Controller - 2E00"
PCI\VEN_8086&DEV_2E01.DeviceDesc         = "Intel(R) 4 Series Chipset PCI Express Root Port - 2E01"
PCI\VEN_8086&DEV_2E08.DeviceDesc         = "Intel(R) Performance Counters - 2E08"
PCI\VEN_8086&DEV_2E09.DeviceDesc         = "Intel(R) 4 Series Chipset PCI Express Root Port - 2E09"
PCI\VEN_8086&DEV_2E10.DeviceDesc         = "Intel(R) 4 Series Chipset Processor to I/O Controller - 2E10"
PCI\VEN_8086&DEV_2E11.DeviceDesc         = "Intel(R) 4 Series Chipset PCI Express Root Port - 2E11"
PCI\VEN_8086&DEV_2E18.DeviceDesc         = "Intel(R) Performance Counters - 2E18"
PCI\VEN_8086&DEV_2E19.DeviceDesc         = "Intel(R) 4 Series Chipset PCI Express Root Port - 2E19"
PCI\VEN_8086&DEV_2E20.DeviceDesc         = "Intel(R) 4 Series Chipset Processor to I/O Controller - 2E20"
PCI\VEN_8086&DEV_2E21.DeviceDesc         = "Intel(R) 4 Series Chipset PCI Express Root Port - 2E21"
PCI\VEN_8086&DEV_2E28.DeviceDesc         = "Intel(R) Performance Counters - 2E28"
PCI\VEN_8086&DEV_2E29.DeviceDesc         = "Intel(R) 4 Series Chipset PCI Express Root Port - 2E29"
PCI\VEN_8086&DEV_2E30.DeviceDesc         = "Intel(R) 4 Series Chipset Processor to I/O Controller - 2E30"
PCI\VEN_8086&DEV_2E31.DeviceDesc         = "Intel(R) 4 Series Chipset PCI Express Root Port - 2E31"
PCI\VEN_8086&DEV_2E38.DeviceDesc         = "Intel(R) Performance Counters - 2E38"
PCI\VEN_8086&DEV_2E40.DeviceDesc         = "Intel(R) 4 Series Chipset Processor to I/O Controller - 2E40"
PCI\VEN_8086&DEV_2E41.DeviceDesc         = "Intel(R) 4 Series Chipset PCI Express Root Port - 2E41"
PCI\VEN_8086&DEV_2E48.DeviceDesc         = "Intel(R) Performance Counters - 2E48"
PCI\VEN_8086&DEV_2E58.DeviceDesc         = "Intel(R) Performance Counters - 2E58"
PCI\VEN_8086&DEV_2E68.DeviceDesc         = "Intel(R) Performance Counters - 2E68"
PCI\VEN_8086&DEV_2E78.DeviceDesc         = "Intel(R) Performance Counters - 2E78"
PCI\VEN_8086&DEV_2E88.DeviceDesc         = "Intel(R) Performance Counters - 2E88"
PCI\VEN_8086&DEV_2E90.DeviceDesc         = "Intel(R) 4 Series Chipset Processor to I/O Controller - 2E90"
PCI\VEN_8086&DEV_2E91.DeviceDesc         = "Intel(R) 4 Series Chipset PCI Express Root Port - 2E91"
PCI\VEN_8086&DEV_2E98.DeviceDesc         = "Intel(R) Performance Counters - 2E98"
PCI\VEN_8086&DEV_2EA8.DeviceDesc         = "Intel(R) Performance Counters - 2EA8"
PCI\VEN_8086&DEV_2EB8.DeviceDesc         = "Intel(R) Performance Counters - 2EB8"
PCI\VEN_8086&DEV_2EC8.DeviceDesc         = "Intel(R) Performance Counters - 2EC8"
PCI\VEN_8086&DEV_2ED8.DeviceDesc         = "Intel(R) Performance Counters - 2ED8"
PCI\VEN_8086&DEV_2EE8.DeviceDesc         = "Intel(R) Performance Counters - 2EE8"
PCI\VEN_8086&DEV_2EF8.DeviceDesc         = "Intel(R) Performance Counters - 2EF8"
PCI\VEN_8086&DEV_3340.DeviceDesc         = "Intel(R) 82855PM Processor to I/O Controller - 3340"
PCI\VEN_8086&DEV_3341.DeviceDesc         = "Intel(R) 82855PM Processor to AGP Controller - 3341"
PCI\VEN_8086&DEV_3400.DeviceDesc         = "Intel(R) 5520/5500/X58 I/O Hub to ESI Port - 3400"
PCI\VEN_8086&DEV_3401.DeviceDesc         = "Intel(R) 5520/5500/X58 I/O Hub to ESI Port - 3401"
PCI\VEN_8086&DEV_3402.DeviceDesc         = "Intel(R) 5520/5500/X58 I/O Hub to ESI Port - 3402"
PCI\VEN_8086&DEV_3403.DeviceDesc         = "Intel(R) 5520/5500/X58 I/O Hub to ESI Port - 3403"
PCI\VEN_8086&DEV_3404.DeviceDesc         = "Intel(R) 5520/5500/X58 I/O Hub to ESI Port - 3404"
PCI\VEN_8086&DEV_3405.DeviceDesc         = "Intel(R) 5520/5500/X58 I/O Hub to ESI Port - 3405"
PCI\VEN_8086&DEV_3406.DeviceDesc         = "Intel(R) 5520/5500/X58 I/O Hub to ESI Port - 3406"
PCI\VEN_8086&DEV_3407.DeviceDesc         = "Intel(R) 5520/5500/X58 I/O Hub to ESI Port - 3407"
PCI\VEN_8086&DEV_3408.DeviceDesc         = "Intel(R) 5520/5500/X58 I/O Hub PCI Express Root Port 1 - 3408"
PCI\VEN_8086&DEV_3409.DeviceDesc         = "Intel(R) 5520/5500/X58 I/O Hub PCI Express Root Port 2 - 3409"
PCI\VEN_8086&DEV_340A.DeviceDesc         = "Intel(R) 5520/5500/X58 I/O Hub PCI Express Root Port 3 - 340A"
PCI\VEN_8086&DEV_340B.DeviceDesc         = "Intel(R) 5520/X58 I/O Hub PCI Express Root Port 4 - 340B"
PCI\VEN_8086&DEV_340C.DeviceDesc         = "Intel(R) 5520/X58 I/O Hub PCI Express Root Port 5 - 340C"
PCI\VEN_8086&DEV_340D.DeviceDesc         = "Intel(R) 5520/X58 I/O Hub PCI Express Root Port 6 - 340D"
PCI\VEN_8086&DEV_340E.DeviceDesc         = "Intel(R) 5520/5500/X58 I/O Hub PCI Express Root Port 7 - 340E"
PCI\VEN_8086&DEV_340F.DeviceDesc         = "Intel(R) 5520/5500/X58 I/O Hub PCI Express Root Port 8 - 340F"
PCI\VEN_8086&DEV_3410.DeviceDesc         = "Intel(R) 5520/5500/X58 I/O Hub PCI Express Root Port 9 - 3410"
PCI\VEN_8086&DEV_3411.DeviceDesc         = "Intel(R) 5520/5500/X58 I/O Hub PCI Express Root Port 10 - 3411"
PCI\VEN_8086&DEV_3418.DeviceDesc         = "Intel(R) 5520/5500/X58 Physical Layer Port 0 - 3418"
PCI\VEN_8086&DEV_3419.DeviceDesc         = "Intel(R) 5520/5500 Physical Layer Port 1 - 3419"
PCI\VEN_8086&DEV_3420.DeviceDesc         = "Intel(R) 5520/5500/X58 I/O Hub PCI Express Root Port 0 - 3420"
PCI\VEN_8086&DEV_3421.DeviceDesc         = "Intel(R) 5520/5500/X58 I/O Hub PCI Express Root Port 0 - 3421"
PCI\VEN_8086&DEV_3422.DeviceDesc         = "Intel(R) 5520/5500/X58 I/O Hub GPIO and Scratch Pad Registers - 3422"
PCI\VEN_8086&DEV_3423.DeviceDesc         = "Intel(R) 5520/5500/X58 I/O Hub Control Status and RAS Registers - 3423"
PCI\VEN_8086&DEV_3424.DeviceDesc         = "Intel(R) 5520/5500/X58 Performance Monitor - 3424"
PCI\VEN_8086&DEV_3425.DeviceDesc         = "Intel(R) 5520/5500/X58 Physical and Link Layer Registers Port 0 - 3425"
PCI\VEN_8086&DEV_3426.DeviceDesc         = "Intel(R) 5520/5500/X58 Routing and Protocol Layer Registers Port 0 - 3426"
PCI\VEN_8086&DEV_3427.DeviceDesc         = "Intel(R) 5520/5500 Physical and Link Layer Registers Port 1 - 3427"
PCI\VEN_8086&DEV_3428.DeviceDesc         = "Intel(R) 5520/5500 Routing and Protocol Layer Register Port 1 - 3428"
PCI\VEN_8086&DEV_3429.DeviceDesc         = "Intel(R) Chipset QuickData Technology device - 3429"
PCI\VEN_8086&DEV_342A.DeviceDesc         = "Intel(R) Chipset QuickData Technology device - 342A"
PCI\VEN_8086&DEV_342B.DeviceDesc         = "Intel(R) Chipset QuickData Technology device - 342B"
PCI\VEN_8086&DEV_342C.DeviceDesc         = "Intel(R) Chipset QuickData Technology device - 342C"
PCI\VEN_8086&DEV_342D.DeviceDesc         = "Intel(R) 5520/5500/X58 I/O Hub I/OxAPIC Interrupt Controller - 342D"
PCI\VEN_8086&DEV_342E.DeviceDesc         = "Intel(R) 5520/5500/X58 I/O Hub System Management Registers - 342E"
PCI\VEN_8086&DEV_342F.DeviceDesc         = "Intel(R) 5520/5500/X58 Trusted Execution Technology Registers - 342F"
PCI\VEN_8086&DEV_3430.DeviceDesc         = "Intel(R) Chipset QuickData Technology device - 3430"
PCI\VEN_8086&DEV_3431.DeviceDesc         = "Intel(R) Chipset QuickData Technology device - 3431"
PCI\VEN_8086&DEV_3432.DeviceDesc         = "Intel(R) Chipset QuickData Technology device - 3432"
PCI\VEN_8086&DEV_3433.DeviceDesc         = "Intel(R) Chipset QuickData Technology device - 3433"
PCI\VEN_8086&DEV_3438.DeviceDesc         = "Intel(R) 5520/5500/X58 I/O Hub Throttle Registers - 3438"
PCI\VEN_8086&DEV_3500.DeviceDesc         = "Intel(R) 6311ESB/6321ESB PCI Express Upstream Port - 3500"
PCI\VEN_8086&DEV_3501.DeviceDesc         = "Intel(R) 6310ESB PCI Express Upstream Port - 3501"
PCI\VEN_8086&DEV_3504.DeviceDesc         = "Intel(R) 6311ESB/6321ESB I/OxAPIC Interrupt Controller - 3504"
PCI\VEN_8086&DEV_3505.DeviceDesc         = "Intel(R) 6310ESB I/OxAPIC Interrupt Controller - 3505"
PCI\VEN_8086&DEV_350C.DeviceDesc         = "Intel(R) 6311ESB/6321ESB PCI Express to PCI-X Bridge - 350C"
PCI\VEN_8086&DEV_350D.DeviceDesc         = "Intel(R) 6310ESB PCI Express to PCI-X Bridge - 350D"
PCI\VEN_8086&DEV_3510.DeviceDesc         = "Intel(R) 6311ESB/6321ESB PCI Express Downstream Port E1 - 3510"
PCI\VEN_8086&DEV_3511.DeviceDesc         = "Intel(R) 6310ESB PCI Express Downstream Port E1 - 3511"
PCI\VEN_8086&DEV_3514.DeviceDesc         = "Intel(R) 6311ESB/6321ESB PCI Express Downstream Port E2 - 3514"
PCI\VEN_8086&DEV_3515.DeviceDesc         = "Intel(R) 6310ESB PCI Express Downstream Port E2 - 3515"
PCI\VEN_8086&DEV_3518.DeviceDesc         = "Intel(R) 6311ESB/6321ESB PCI Express Downstream Port E3 - 3518"
PCI\VEN_8086&DEV_3519.DeviceDesc         = "Intel(R) 6310ESB PCI Express Downstream Port E3 - 3519"
PCI\VEN_8086&DEV_3575.DeviceDesc         = "Intel(R) 82830 Processor to I/O Controller - 3575"
PCI\VEN_8086&DEV_3576.DeviceDesc         = "Intel(R) 82830 Processor to AGP Controller - 3576"
PCI\VEN_8086&DEV_3578.DeviceDesc         = "Intel(R) 82830 Processor to I/O Controller - 3578"
PCI\VEN_8086&DEV_3580.DeviceDesc         = "Intel(R) 82852/82855 GM/GME/PM/GMV to Processor I/O Controller - 3580"
PCI\VEN_8086&DEV_3581.DeviceDesc         = "Intel(R) 82852/82855 GM/GME/PM/GMV Processor to AGP Controller - 3581"
PCI\VEN_8086&DEV_3584.DeviceDesc         = "Intel(R) 82852/82855 GM/GME/PM/GMV Processor to I/O Controller - 3584"
PCI\VEN_8086&DEV_3585.DeviceDesc         = "Intel(R) 82852/82855 GM/GME/PM/GMV Processor to I/O Controller - 3585"
PCI\VEN_8086&DEV_3590.DeviceDesc         = "Intel(R) E7520 Memory Controller Hub - 3590"
PCI\VEN_8086&DEV_3591.DeviceDesc         = "Intel(R) E7525/E7520 Error Reporting Registers - 3591"
PCI\VEN_8086&DEV_3592.DeviceDesc         = "Intel(R) E7320 Memory Controller Hub - 3592"
PCI\VEN_8086&DEV_3593.DeviceDesc         = "Intel(R) E7320 Error Reporting Registers - 3593"
PCI\VEN_8086&DEV_3594.DeviceDesc         = "Intel(R) E7520 DMA Controller - 3594"
PCI\VEN_8086&DEV_3595.DeviceDesc         = "Intel(R) E7525/E7520/E7320 PCI Express Root Port A0 - 3595"
PCI\VEN_8086&DEV_3596.DeviceDesc         = "Intel(R) E7525/E7520/E7320 PCI Express Root Port A1 - 3596"
PCI\VEN_8086&DEV_3597.DeviceDesc         = "Intel(R) E7525/E7520 PCI Express Root Port B0 - 3597"
PCI\VEN_8086&DEV_3598.DeviceDesc         = "Intel(R) E7520 PCI Express Root Port B1 - 3598"
PCI\VEN_8086&DEV_3599.DeviceDesc         = "Intel(R) E7520 PCI Express Root Port C0 - 3599"
PCI\VEN_8086&DEV_359A.DeviceDesc         = "Intel(R) E7520 PCI Express Root Port C1 - 359A"
PCI\VEN_8086&DEV_359B.DeviceDesc         = "Intel(R) E7525/E7520/E7320 Extended Configuration Registers - 359B"
PCI\VEN_8086&DEV_359E.DeviceDesc         = "Intel(R) E7525 Memory Controller Hub - 359E"
PCI\VEN_8086&DEV_35B0.DeviceDesc         = "Intel(R) 3100 Chipset Memory I/O Controller Hub - 35B0"
PCI\VEN_8086&DEV_35B1.DeviceDesc         = "Intel(R) 3100 Chipset DRAM Controller Error Reporting Registers - 35B1"
PCI\VEN_8086&DEV_35B5.DeviceDesc         = "Intel(R) 3100 Chipset Enhanced DMA Controller - 35B5"
PCI\VEN_8086&DEV_35B6.DeviceDesc         = "Intel(R) 3100 Chipset PCI Express Port A - 35B6"
PCI\VEN_8086&DEV_35B7.DeviceDesc         = "Intel(R) 3100 Chipset PCI Express Port A1 - 35B7"
PCI\VEN_8086&DEV_35C8.DeviceDesc         = "Intel(R) 3100 Chipset Extended Configuration Test Overflow Registers - 35C8"

PCI\VEN_8086&DEV_3600.DeviceDesc         = "Intel(R) 7300 Chipset Memory Controller Hub - 3600"
PCI\VEN_8086&DEV_3604.DeviceDesc         = "Intel(R) 7300 Chipset PCI Express Port 1 - 3604"
PCI\VEN_8086&DEV_3605.DeviceDesc         = "Intel(R) 7300 Chipset PCI Express Port 2 - 3605"
PCI\VEN_8086&DEV_3606.DeviceDesc         = "Intel(R) 7300 Chipset PCI Express Port 3 - 3606"
PCI\VEN_8086&DEV_3607.DeviceDesc         = "Intel(R) 7300 Chipset PCI Express Port 4 - 3607"
PCI\VEN_8086&DEV_3608.DeviceDesc         = "Intel(R) 7300 Chipset PCI Express Port 5 - 3608"
PCI\VEN_8086&DEV_3609.DeviceDesc         = "Intel(R) 7300 Chipset PCI Express Port 6 - 3609"
PCI\VEN_8086&DEV_360A.DeviceDesc         = "Intel(R) 7300 Chipset PCI Express Port 7 - 360A"
PCI\VEN_8086&DEV_360B.DeviceDesc         = "Intel(R) 7300 Chipset QuickData Technology Device - 360B"
PCI\VEN_8086&DEV_360C.DeviceDesc         = "Intel(R) 7300 Chipset FSB Registers - 360C"
PCI\VEN_8086&DEV_360D.DeviceDesc         = "Intel(R) 7300 Chipset Snoop Filter Registers - 360D"
PCI\VEN_8086&DEV_360E.DeviceDesc         = "Intel(R) 7300 Chipset Debug and Miscellaneous Registers - 360E"
PCI\VEN_8086&DEV_360F.DeviceDesc         = "Intel(R) 7300 Chipset FBD Branch 0 Registers - 360F"
PCI\VEN_8086&DEV_3610.DeviceDesc         = "Intel(R) 7300 Chipset FBD Branch 1 Registers - 3610"
PCI\VEN_8086&DEV_3A10.DeviceDesc         = "Intel(R) ICH10 LPC Interface Controller - 3A10"
PCI\VEN_8086&DEV_3A14.DeviceDesc         = "Intel(R) ICH10DO LPC Interface Controller - 3A14"
PCI\VEN_8086&DEV_3A16.DeviceDesc         = "Intel(R) ICH10R LPC Interface Controller - 3A16"
PCI\VEN_8086&DEV_3A18.DeviceDesc         = "Intel(R) ICH10 LPC Interface Controller - 3A18"
PCI\VEN_8086&DEV_3A1A.DeviceDesc         = "Intel(R) ICH10D LPC Interface Controller - 3A1A"
PCI\VEN_8086&DEV_3A1E.DeviceDesc         = "Intel(R) ICH10 LPC Interface Controller - 3A1E"
PCI\VEN_8086&DEV_3A30.DeviceDesc         = "Intel(R) ICH10 Family SMBus Controller - 3A30"
PCI\VEN_8086&DEV_3A32.DeviceDesc         = "Intel(R) ICH10 Family Thermal Subsystem - 3A32"
PCI\VEN_8086&DEV_3A40.DeviceDesc         = "Intel(R) ICH10 Family PCI Express Root Port 1 - 3A40"
PCI\VEN_8086&DEV_3A42.DeviceDesc         = "Intel(R) ICH10 Family PCI Express Root Port 2 - 3A42"
PCI\VEN_8086&DEV_3A44.DeviceDesc         = "Intel(R) ICH10 Family PCI Express Root Port 3 - 3A44"
PCI\VEN_8086&DEV_3A46.DeviceDesc         = "Intel(R) ICH10 Family PCI Express Root Port 4 - 3A46"
PCI\VEN_8086&DEV_3A48.DeviceDesc         = "Intel(R) ICH10 Family PCI Express Root Port 5 - 3A48"
PCI\VEN_8086&DEV_3A4A.DeviceDesc         = "Intel(R) ICH10 Family PCI Express Root Port 6 - 3A4A"
PCI\VEN_8086&DEV_3A51.DeviceDesc         = "Intel(R) ICH10 Family Virtualization Engine Controller - 3A51"
PCI\VEN_8086&DEV_3A60.DeviceDesc         = "Intel(R) ICH10 Family SMBus Controller - 3A60"
PCI\VEN_8086&DEV_3A62.DeviceDesc         = "Intel(R) ICH10 Family Thermal Subsystem - 3A62"
PCI\VEN_8086&DEV_3A70.DeviceDesc         = "Intel(R) ICH10 Family PCI Express Root Port 1 - 3A70"
PCI\VEN_8086&DEV_3A72.DeviceDesc         = "Intel(R) ICH10 Family PCI Express Root Port 2 - 3A72"
PCI\VEN_8086&DEV_3A74.DeviceDesc         = "Intel(R) ICH10 Family PCI Express Root Port 3 - 3A74"
PCI\VEN_8086&DEV_3A76.DeviceDesc         = "Intel(R) ICH10 Family PCI Express Root Port 4 - 3A76"
PCI\VEN_8086&DEV_3A78.DeviceDesc         = "Intel(R) ICH10 Family PCI Express Root Port 5 - 3A78"
PCI\VEN_8086&DEV_3A7A.DeviceDesc         = "Intel(R) ICH10 Family PCI Express Root Port 6 - 3A7A"
PCI\VEN_8086&DEV_3B00.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family LPC Interface Controller - 3B00"
PCI\VEN_8086&DEV_3B01.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family LPC Interface Controller - 3B01"
PCI\VEN_8086&DEV_3B02.DeviceDesc         = "Intel(R) P55 Express Chipset LPC Interface Controller - 3B02"
PCI\VEN_8086&DEV_3B03.DeviceDesc         = "Intel(R) PM55 Express Chipset LPC Interface Controller - 3B03"
PCI\VEN_8086&DEV_3B04.DeviceDesc         = "Intel(R) P57 Express Chipset LPC Interface Controller - 3B04"
PCI\VEN_8086&DEV_3B05.DeviceDesc         = "Intel(R) PM57 Express Chipset LPC Interface Controller - 3B05"
PCI\VEN_8086&DEV_3B06.DeviceDesc         = "Intel(R) H55 Express Chipset LPC Interface Controller - 3B06"
PCI\VEN_8086&DEV_3B07.DeviceDesc         = "Intel(R) QM57 Express Chipset LPC Interface Controller - 3B07"
PCI\VEN_8086&DEV_3B08.DeviceDesc         = "Intel(R) H57 Express Chipset LPC Interface Controller - 3B08"
PCI\VEN_8086&DEV_3B09.DeviceDesc         = "Intel(R) HM55 Express Chipset LPC Interface Controller - 3B09"
PCI\VEN_8086&DEV_3B0A.DeviceDesc         = "Intel(R) Q57 Express Chipset LPC Interface Controller - 3B0A"
PCI\VEN_8086&DEV_3B0B.DeviceDesc         = "Intel(R) HM57 Express Chipset LPC Interface Controller - 3B0B"
PCI\VEN_8086&DEV_3B0C.DeviceDesc         = "Intel(R) A57 Express Chipset LPC Interface Controller - 3B0C"
PCI\VEN_8086&DEV_3B0D.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family LPC Interface Controller - 3B0D"
PCI\VEN_8086&DEV_3B0E.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family LPC Interface Controller - 3B0E"
PCI\VEN_8086&DEV_3B0F.DeviceDesc         = "Intel(R) QS57 Express Chipset LPC Interface Controller - 3B0F"
PCI\VEN_8086&DEV_3B10.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family LPC Interface Controller - 3B10"
PCI\VEN_8086&DEV_3B11.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family LPC Interface Controller - 3B11"
PCI\VEN_8086&DEV_3B12.DeviceDesc         = "Intel(R) 3400 Chipset LPC Interface Controller - 3B12"
PCI\VEN_8086&DEV_3B13.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family LPC Interface Controller - 3B13"
PCI\VEN_8086&DEV_3B14.DeviceDesc         = "Intel(R) 3420 Chipset LPC Interface Controller - 3B14"
PCI\VEN_8086&DEV_3B15.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family LPC Interface Controller - 3B15"
PCI\VEN_8086&DEV_3B16.DeviceDesc         = "Intel(R) 3450 Chipset LPC Interface Controller - 3B16"
PCI\VEN_8086&DEV_3B17.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family LPC Interface Controller - 3B17"
PCI\VEN_8086&DEV_3B18.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family LPC Interface Controller - 3B18"
PCI\VEN_8086&DEV_3B19.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family LPC Interface Controller - 3B19"
PCI\VEN_8086&DEV_3B1A.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family LPC Interface Controller - 3B1A"
PCI\VEN_8086&DEV_3B1B.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family LPC Interface Controller - 3B1B"
PCI\VEN_8086&DEV_3B1C.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family LPC Interface Controller - 3B1C"
PCI\VEN_8086&DEV_3B1D.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family LPC Interface Controller - 3B1D"
PCI\VEN_8086&DEV_3B1E.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family LPC Interface Controller - 3B1E"
PCI\VEN_8086&DEV_3B1F.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family LPC Interface Controller - 3B1F"
PCI\VEN_8086&DEV_3B53.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family Virtualization Engine Controller - 3B53" 
PCI\VEN_8086&DEV_3B30.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family SMBus Controller - 3B30"
PCI\VEN_8086&DEV_3B32.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family Thermal Subsystem - 3B32"
PCI\VEN_8086&DEV_3B42.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family PCI Express Root Port 1 - 3B42"
PCI\VEN_8086&DEV_3B44.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family PCI Express Root Port 2 - 3B44"
PCI\VEN_8086&DEV_3B46.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family PCI Express Root Port 3 - 3B46"
PCI\VEN_8086&DEV_3B48.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family PCI Express Root Port 4 - 3B48"
PCI\VEN_8086&DEV_3B4A.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family PCI Express Root Port 5 - 3B4A"
PCI\VEN_8086&DEV_3B4C.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family PCI Express Root Port 6 - 3B4C"
PCI\VEN_8086&DEV_3B4E.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family PCI Express Root Port 7 - 3B4E"
PCI\VEN_8086&DEV_3B50.DeviceDesc         = "Intel(R) 5 Series/3400 Series Chipset Family PCI Express Root Port 8 - 3B50"
PCI\VEN_8086&DEV_4000.DeviceDesc         = "Intel(R) 5400 Chipset Memory Controller Hub - 4000"
PCI\VEN_8086&DEV_4001.DeviceDesc         = "Intel(R) 5400 Chipset Memory Controller Hub - 4001"
PCI\VEN_8086&DEV_4003.DeviceDesc         = "Intel(R) 5400 Chipset Memory Controller Hub - 4003"
PCI\VEN_8086&DEV_4021.DeviceDesc         = "Intel(R) 5400 Chipset PCI Express Port 1 - 4021"
PCI\VEN_8086&DEV_4022.DeviceDesc         = "Intel(R) 5400 Chipset PCI Express Port 2 - 4022"
PCI\VEN_8086&DEV_4023.DeviceDesc         = "Intel(R) 5400 Chipset PCI Express Port 3 - 4023"
PCI\VEN_8086&DEV_4024.DeviceDesc         = "Intel(R) 5400 Chipset PCI Express Port 4 - 4024"
PCI\VEN_8086&DEV_4025.DeviceDesc         = "Intel(R) 5400 Chipset PCI Express Port 5 - 4025"
PCI\VEN_8086&DEV_4026.DeviceDesc         = "Intel(R) 5400 Chipset PCI Express Port 6 - 4026"
PCI\VEN_8086&DEV_4027.DeviceDesc         = "Intel(R) 5400 Chipset PCI Express Port 7 - 4027"
PCI\VEN_8086&DEV_4028.DeviceDesc         = "Intel(R) 5400 Chipset PCI Express Port 8 - 4028"
PCI\VEN_8086&DEV_4029.DeviceDesc         = "Intel(R) 5400 Chipset PCI Express Port 9 - 4029"
PCI\VEN_8086&DEV_402D.DeviceDesc         = "Intel(R) 5400 Chipset IBIST Registers - 402D"
PCI\VEN_8086&DEV_402E.DeviceDesc         = "Intel(R) 5400 Chipset IBIST Registers - 402E"
PCI\VEN_8086&DEV_4030.DeviceDesc         = "Intel(R) 5400 Chipset FSB Registers - 4030"
PCI\VEN_8086&DEV_4031.DeviceDesc         = "Intel(R) 5400 Chipset CE/SF Registers - 4031"
PCI\VEN_8086&DEV_4032.DeviceDesc         = "Intel(R) 5400 Chipset IOxAPIC - 4032"
PCI\VEN_8086&DEV_4035.DeviceDesc         = "Intel(R) 5400 Chipset FBD Registers - 4035"
PCI\VEN_8086&DEV_4036.DeviceDesc         = "Intel(R) 5400 Chipset FBD Registers - 4036"
PCI\VEN_8086&DEV_537C.DeviceDesc         = "Intel(R) 31154 133MHz PCI TO PCI Bridge - 537C"
PCI\VEN_8086&DEV_65C0.DeviceDesc         = "Intel(R) 5100 Chipset Memory Controller Hub - 65C0"
PCI\VEN_8086&DEV_65E2.DeviceDesc         = "Intel(R) 5100 Chipset PCI Express x4 Port 2 - 65E2"
PCI\VEN_8086&DEV_65E3.DeviceDesc         = "Intel(R) 5100 Chipset PCI Express x4 Port 3 - 65E3"
PCI\VEN_8086&DEV_65E4.DeviceDesc         = "Intel(R) 5100 Chipset PCI Express x4 Port 4 - 65E4"
PCI\VEN_8086&DEV_65E5.DeviceDesc         = "Intel(R) 5100 Chipset PCI Express x4 Port 5 - 65E5"
PCI\VEN_8086&DEV_65E6.DeviceDesc         = "Intel(R) 5100 Chipset PCI Express x4 Port 6 - 65E6"
PCI\VEN_8086&DEV_65E7.DeviceDesc         = "Intel(R) 5100 Chipset PCI Express x4 Port 7 - 65E7"
PCI\VEN_8086&DEV_65F0.DeviceDesc         = "Intel(R) 5100 Chipset FSB Registers - 65F0"
PCI\VEN_8086&DEV_65F1.DeviceDesc         = "Intel(R) 5100 Chipset Reserved Registers - 65F1"
PCI\VEN_8086&DEV_65F2.DeviceDesc         = "Intel(R) 5100 Chipset Reserved Registers - 65F3"
PCI\VEN_8086&DEV_65F5.DeviceDesc         = "Intel(R) 5100 Chipset DDR Channel 0 Registers - 65F5"
PCI\VEN_8086&DEV_65F6.DeviceDesc         = "Intel(R) 5100 Chipset DDR Channel 1 Registers - 65F6"
PCI\VEN_8086&DEV_65F7.DeviceDesc         = "Intel(R) 5100 Chipset PCI Express x8 Port 2-3 - 65F7"
PCI\VEN_8086&DEV_65F8.DeviceDesc         = "Intel(R) 5100 Chipset PCI Express x8 Port 4-5 - 65F8"
PCI\VEN_8086&DEV_65F9.DeviceDesc         = "Intel(R) 5100 Chipset PCI Express x8 Port 6-7 - 65F9"
PCI\VEN_8086&DEV_65FA.DeviceDesc         = "Intel(R) 5100 Chipset PCI Express x16 Port 4-7 - 65FA"
PCI\VEN_8086&DEV_65FF.DeviceDesc         = "Intel(R) 5100 Chipset DMA Engine - 65FF"
PCI\VEN_8086&DEV_7000.DeviceDesc         = "Intel 82371SB PCI to ISA bridge"
PCI\VEN_8086&DEV_7030.DeviceDesc         = "Intel 82437VX Pentium(R) Processor to PCI bridge"
PCI\VEN_8086&DEV_7100.DeviceDesc         = "Intel 82439TX Pentium(R) Processor to PCI bridge"
PCI\VEN_8086&DEV_7110_EIO.DeviceDesc     = "Intel 82371AB/EB PCI to ISA bridge (EIO mode)"
PCI\VEN_8086&DEV_7110_ISA.DeviceDesc     = "Intel 82371AB/EB PCI to ISA bridge (ISA mode)"
PCI\VEN_8086&DEV_7110_OLD_EIO.DeviceDesc = "Intel 82371AB PCI to ISA bridge (EIO mode)"
PCI\VEN_8086&DEV_7110_OLD_ISA.DeviceDesc = "Intel 82371AB PCI to ISA bridge (ISA mode)"
PCI\VEN_8086&DEV_7113_OLD.DeviceDesc     = "Intel 82371AB Power Management Controller"
PCI\VEN_8086&DEV_7113.DeviceDesc         = "Intel 82371EB Power Management Controller"
PCI\VEN_8086&DEV_7120.DeviceDesc         = "Intel(R) 82810 System and Graphics Controller"
PCI\VEN_8086&DEV_7122.DeviceDesc         = "Intel(R) 82810 DC-100 System and Graphics Controller"
PCI\VEN_8086&DEV_7124.DeviceDesc         = "Intel(R) 82810e DC-133 System and Graphics Controller"
PCI\VEN_8086&DEV_7180.DeviceDesc         = "Intel 82443LX/EX Pentium(R) II Processor to PCI bridge"
PCI\VEN_8086&DEV_7181.DeviceDesc         = "Intel 82443LX/EX Pentium(R) II Processor to AGP Controller"
PCI\VEN_8086&DEV_7190.DeviceDesc         = "Intel 82443BX Pentium(R) II Processor to PCI Bridge"
PCI\VEN_8086&DEV_7191.DeviceDesc         = "Intel 82443BX Pentium(R) II Processor to AGP Controller"
PCI\VEN_8086&DEV_7192.DeviceDesc         = "Intel 82443BX Pentium(R) II Processor to PCI Bridge"
PCI\VEN_8086&DEV_7194.DeviceDesc         = "Intel(R) 82440MX Processor to I/O Controller"
PCI\VEN_8086&DEV_7198.DeviceDesc         = "Intel(R) 82440MX PCI to ISA Bridge"
PCI\VEN_8086&DEV_719B.DeviceDesc         = "Intel(R) 82440MX Power Management Controller"
PCI\VEN_8086&DEV_71A0.DeviceDesc         = "Intel 82443GX Pentium(R) II Xeon(tm) Processor to PCI Bridge"
PCI\VEN_8086&DEV_71A1.DeviceDesc         = "Intel 82443GX Pentium(R) II Xeon(tm) Processor to AGP Controller"
PCI\VEN_8086&DEV_7600.DeviceDesc         = "Intel 82372FB PCI to ISA Bridge"
PCI\VEN_8086&DEV_7603.DeviceDesc         = "Intel 82372FB System Management Bus Controller"
PCI\VEN_8086&DEV_8002.DeviceDesc         = "Intel(R) Trusted Execution Technology - 8002"
PCI\VEN_8086&DEV_84C4.DeviceDesc         = "Intel 82454KX/GX PCI bridge"
PCI\VEN_8086&DEV_84C5.DeviceDesc         = "Intel 82453KX/GX Memory Controller"
PCI\VEN_8086&DEV_A000.DeviceDesc         = "Intel(R) N10 Family DMI Bridge - A000"
PCI\VEN_8086&DEV_A010.DeviceDesc         = "Intel(R) N10 Family DMI Bridge - A010"
PCI\VEN_8086&DEV_B152.DeviceDesc         = "Intel 21152 PCI to PCI bridge"
PCI\VEN_8086&DEV_B154.DeviceDesc         = "Intel 21154 PCI to PCI bridge"
PCI\VEN_8086&DEV_B555&SUBSYS_B555119F.DeviceDesc = "Intel(R) 21555 PCI to PCI Bridge - B555"
PCI\VEN_8086&DEV_D130.DeviceDesc         = "Intel(R) processor DMI - D130"
PCI\VEN_8086&DEV_D131.DeviceDesc         = "Intel(R) processor DMI - D131"
PCI\VEN_8086&DEV_D132.DeviceDesc         = "Intel(R) processor DMI - D132"
PCI\VEN_8086&DEV_D133.DeviceDesc         = "Intel(R) processor DMI - D133"
PCI\VEN_8086&DEV_D134.DeviceDesc         = "Intel(R) processor DMI - D134"
PCI\VEN_8086&DEV_D135.DeviceDesc         = "Intel(R) processor DMI - D135"
PCI\VEN_8086&DEV_D136.DeviceDesc         = "Intel(R) processor DMI - D136"
PCI\VEN_8086&DEV_D137.DeviceDesc         = "Intel(R) processor DMI - D137"
PCI\VEN_8086&DEV_D138.DeviceDesc         = "Intel(R) processor PCI Express Root Port 1 - D138"
PCI\VEN_8086&DEV_D139.DeviceDesc         = "Intel(R) processor PCI Express Root Port 2 - D139"
PCI\VEN_8086&DEV_D13A.DeviceDesc         = "Intel(R) processor PCI Express Root Port 3 - D13A"
PCI\VEN_8086&DEV_D13B.DeviceDesc         = "Intel(R) processor PCI Express Root Port 4 - D13B"
PCI\VEN_8086&DEV_D150.DeviceDesc         = "Intel(R) QuickPath Interconnect - D150"
PCI\VEN_8086&DEV_D151.DeviceDesc         = "Intel(R) QuickPath Interconnect - D151"
PCI\VEN_8086&DEV_D155.DeviceDesc         = "Intel(R) processor System Management Registers - D155"
PCI\VEN_8086&DEV_D156.DeviceDesc         = "Intel(R) processor Semaphore and Scratchpad Registers - D156"
PCI\VEN_8086&DEV_D157.DeviceDesc         = "Intel(R) processor System Control and Status Registers - D157"
PCI\VEN_8086&DEV_D158.DeviceDesc         = "Intel(R) processor Miscellaneous Registers - D158"

MICRON_MFG = "Micron Electronics"
PCI\VEN_1042&DEV_3000.DeviceDesc = "Micron Samurai(tm) Pentium(r) II Processor to PCI bridge"
PCI\VEN_1042&DEV_3010.DeviceDesc = "Micron Samurai(tm) Pentium(r) II Processor to PCI bridge"

NATSEMI_MFG = "National Semiconductor"
PCI\VEN_1066&DEV_0001.DeviceDesc = "National PT86C521 Pentium(r) CPU to PCI bridge"
PCI\VEN_1066&DEV_8002.DeviceDesc = "National PT86C523 PCI to ISA bridge"
PCI\VEN_1066&DEV_0002.DeviceDesc = "National PT86C523 PCI to ISA bridge"
PCI\VEN_100B&DEV_0011.DeviceDesc = "National PCI System I/O"

NEC_MFG = "NEC"
PCI\VEN_1033&DEV_00A8&CC_0600.DeviceDesc = "NEC Enterprise Server Chipset - SAC"
PCI\VEN_1033&DEV_00A8&CC_0000.DeviceDesc = "NEC Enterprise Server Chipset - SAC"
PCI\VEN_1033&DEV_00A9&CC_0600.DeviceDesc = "NEC Enterprise Server Chipset - SDC"
PCI\VEN_1033&DEV_00AA&CC_0500.DeviceDesc = "NEC Enterprise Server Chipset - MAC"
PCI\VEN_1033&DEV_00AB.DeviceDesc         = "NEC Enterprise Server Chipset - MDC"
PCI\VEN_1033&DEV_00AC&CC_0600.DeviceDesc = "NEC Enterprise Server Chipset - IOC"
PCI\VEN_1033&DEV_00AD&CC_0600.DeviceDesc = "NEC Enterprise Server Chipset - DGU"
PCI\VEN_1033&DEV_00AE&CC_0600.DeviceDesc = "NEC Enterprise Server Chipset - GPB"
PCI\VEN_1033&DEV_00AF.DeviceDesc         = "NEC Enterprise Server Chipset - PPID"
PCI\VEN_1033&DEV_00B0.DeviceDesc         = "NEC Enterprise Server Chipset - SMBC"
PCI\VEN_1033&DEV_00B1&CC_0600.DeviceDesc = "NEC Enterprise Server Chipset - MPB"

NVIDIA_MFG = "NVIDIA"
PCI\VEN_10DE&DEV_005E.DeviceDesc = "NVIDIA nForce4 HyperTransport Bridge"
PCI\VEN_10DE&DEV_00D2.DeviceDesc = "NVIDIA nForce3 AGP Host to PCI Bridge"
PCI\VEN_10DE&DEV_00D3.DeviceDesc = "NVIDIA nForce4 Low Pin Count Controller"
PCI\VEN_10DE&DEV_00E4.DeviceDesc = "NVIDIA nForce PCI System Management"
PCI\VEN_10DE&DEV_0052.DeviceDesc = "NVIDIA nForce PCI System Management"
PCI\VEN_10DE&DEV_0084.DeviceDesc = "NVIDIA nForce PCI System Management"
PCI\VEN_10DE&DEV_00D4.DeviceDesc = "NVIDIA nForce PCI System Management"
PCI\VEN_10DE&DEV_0264.DeviceDesc = "NVIDIA nForce PCI System Management"
PCI\VEN_10DE&DEV_0368.DeviceDesc = "NVIDIA nForce PCI System Management"
PCI\VEN_10DE&DEV_03EB.DeviceDesc = "NVIDIA nForce PCI System Management"
PCI\VEN_10DE&DEV_00E2.DeviceDesc = "NVIDIA nForce3 250 AGP Host to PCI Bridge"
PCI\VEN_10DE&DEV_01B7.DeviceDesc = "NVIDIA nForce AGP Host to PCI Bridge"
PCI\VEN_10DE&DEV_01E8.DeviceDesc = "NVIDIA nForce2 AGP Host to PCI Bridge"
PCI\VEN_10DE&DEV_0446.DeviceDesc = "NVIDIA nForce PCI System Management"
PCI\VEN_10DE&DEV_0542.DeviceDesc = "NVIDIA nForce PCI System Management"
PCI\VEN_10DE&DEV_07D8.DeviceDesc = "NVIDIA nForce PCI System Management"
PCI\VEN_10DE&DEV_0752.DeviceDesc = "NVIDIA nForce PCI System Management"
PCI\VEN_10DE&DEV_0AA2.DeviceDesc = "NVIDIA nForce PCI System Management"


OPTI_MFG = "Opti"
PCI\VEN_1045&DEV_C822.DeviceDesc = "Opti 82C822 Pentium(r) CPU to PCI & PCI to ISA Plug and Play bridge"
PCI\VEN_1045&DEV_C832.DeviceDesc = "Opti 82C832 Pentium(r) CPU to PCI & PCI to ISA Plug and Play bridge"
PCI\VEN_1045&DEV_C557.DeviceDesc = "Opti 82C557 CPU to PCI bridge"
PCI\VEN_1045&DEV_C558.DeviceDesc = "Opti 82C558 PCI to ISA Plug and Play bridge"
PCI\VEN_1045&DEV_C567.DeviceDesc = "Opti Viper Max CPU to PCI bridge"
PCI\VEN_1045&DEV_C568.DeviceDesc = "Opti Viper Max PCI to ISA Plug and Play bridge"
PCI\VEN_1045&DEV_C700.DeviceDesc = "Opti FireStar PCI to ISA Plug and Play bridge"
PCI\VEN_1045&DEV_C701.DeviceDesc = "Opti FireStar CPU to PCI bridge"

SERVERWORKS_MFG = "ServerWorks (RCC)"
PCI\VEN_1166&DEV_0005&CC_0604.DeviceDesc = "ServerWorks (RCC) CNB20-LE Processor to AGP Controller"
PCI\VEN_1166&DEV_0005&CC_0600.DeviceDesc = "ServerWorks (RCC) CNB20-LE Processor to PCI Bridge(*)"
PCI\VEN_1166&DEV_0007.DeviceDesc         = "ServerWorks (RCC) CNB20-LE Processor to PCI Bridge"
PCI\VEN_1166&DEV_0008.DeviceDesc         = "ServerWorks (RCC) CNB20-HE Processor to PCI Bridge"
PCI\VEN_1166&DEV_0009&CC_0604.DeviceDesc = "ServerWorks (RCC) CNB20-HE Processor to AGP Controller"
PCI\VEN_1166&DEV_0009&CC_0600.DeviceDesc = "ServerWorks (RCC) CNB20-HE Processor to PCI Bridge(*)"
PCI\VEN_1166&DEV_0010&CC_0600.DeviceDesc = "ServerWorks Grand Champion CIOB_X - I/O Bridge 100 Mhz"
PCI\VEN_1166&DEV_0011&CC_0600.DeviceDesc = "ServerWorks Grand Champion CMIC_HE - NorthBridge High End"
PCI\VEN_1166&DEV_0012&CC_0600.DeviceDesc = "ServerWorks Grand Champion CNB3.0HE - NorthBridge Low End"
PCI\VEN_1166&DEV_0013.DeviceDesc         = "ServerWorks (RCC) CNB20-HE Processor to PCI Bridge"
PCI\VEN_1166&DEV_0014&CC_0604.DeviceDesc = "ServerWorks (RCC) CMIC_LE Processor to AGP 4X Controller"
PCI\VEN_1166&DEV_0014&CC_0600.DeviceDesc = "ServerWorks (RCC) CMIC_LE Processor to PCI Bridge(*)"
PCI\VEN_1166&DEV_0015.DeviceDesc         = "ServerWorks (RCC) CMIC-WS Processor to PCI Bridge"
PCI\VEN_1166&DEV_0016&CC_0604.DeviceDesc = "ServerWorks (RCC) CIOB-G Processor to AGP Controller"
PCI\VEN_1166&DEV_0016&CC_0600.DeviceDesc = "ServerWorks (RCC) CIOB-G Processor to PCI Bridge(*)"
PCI\VEN_1166&DEV_0017&CC_0600.DeviceDesc = "ServerWorks Grand Champion CMIC_SL - NorthBridge Super Lite"
PCI\VEN_1166&DEV_0036&CC_0604.DeviceDesc = "ServerWorks (Broadcom) HT-1000 HT-PCI-X Bridge 0"
PCI\VEN_1166&DEV_0101&CC_0600.DeviceDesc = "ServerWorks Grand Champion CIOB_X2 - I/O Bridge 133 Mhz"
PCI\VEN_1166&DEV_0104&CC_0604.DeviceDesc = "ServerWorks (Broadcom) HT-1000 HT-PCI-X Bridge"
PCI\VEN_1166&DEV_0110&CC_0600.DeviceDesc = "ServerWorks Grand Champion CIOB_E - I/O Bridge with GB Ethernet"
PCI\VEN_1166&DEV_0130&CC_0604.DeviceDesc = "ServerWorks (Broadcom) HT-2000 HT-PCI-X Bridge"
PCI\VEN_1166&DEV_0132&CC_0604.DeviceDesc = "ServerWorks (Broadcom) HT-2000 HT-PCI-E Bridge"
PCI\VEN_1166&DEV_0140&CC_0604.DeviceDesc = "ServerWorks (Broadcom) HT-2100 HT-PCI-E Bridge 0"
PCI\VEN_1166&DEV_0142&CC_0604.DeviceDesc = "ServerWorks (Broadcom) HT-2100 HT-PCI-E Bridge 1&3"
PCI\VEN_1166&DEV_0144&CC_0604.DeviceDesc = "ServerWorks (Broadcom) HT-2100 HT-PCI-E Bridge 2&4"
PCI\VEN_1166&DEV_0200.DeviceDesc         = "ServerWorks Champion OSB4 - SouthBridge 4"
PCI\VEN_1166&DEV_0201&CC_0600.DeviceDesc = "ServerWorks Champion CSB5 - SouthBridge 5"
PCI\VEN_1166&DEV_0203&CC_0600.DeviceDesc = "ServerWorks Champion CSB6 - SouthBridge 6"
PCI\VEN_1166&DEV_0205&CC_0600.DeviceDesc = "ServerWorks (Broadcom) HT-1000 HT-PCI-X Bridge 1"
PCI\VEN_1166&DEV_0214&CC_0108.DeviceDesc = "ServerWorks (Broadcom) HT-1000 HT-IDE"
PCI\VEN_1166&DEV_0225.DeviceDesc         = "Serverworks Champion CSB5 - SouthBridge 5 LPC"
PCI\VEN_1166&DEV_0227.DeviceDesc         = "Serverworks Champion CSB6 - SouthBridge 6 LPC"
PCI\VEN_1166&DEV_0230.DeviceDesc         = "Serverworks Champion CSB5 - SouthBridge 5 XIOAPIC"
PCI\VEN_1166&DEV_0234&CC_0601.DeviceDesc = "ServerWorks (Broadcom) HT-1000 HT-PCI-X to ISA Bridge"

SIS_MFG = "Silicon Integrated Systems"
PCI\VEN_1039&DEV_0001.DeviceDesc = "SIS Processor to AGP Controller"
PCI\VEN_1039&DEV_0008.DeviceDesc = "SIS PCI to ISA bridge"
PCI\VEN_1039&DEV_0009.DeviceDesc = "SIS PMU device"
PCI\VEN_1039&DEV_0406.DeviceDesc = "SIS Pentium(r) to PCI bridge [original model]"
PCI\VEN_1039&DEV_0496.DeviceDesc = "SIS CPU to PCI & PCI to ISA bridge [original model]"
PCI\VEN_1039&DEV_0540.DeviceDesc = "SiS540 Host CPU Bridge"
PCI\VEN_1039&DEV_0630.DeviceDesc = "SiS630 Host CPU Bridge"
PCI\VEN_1039&DEV_0635.DeviceDesc = "SiS635/633  Host CPU Bridge"
PCI\VEN_1039&DEV_0730.DeviceDesc = "SiS730 Host CPU Bridge"
PCI\VEN_1039&DEV_0735.DeviceDesc = "SiS735/733  Host CPU Bridge"
PCI\VEN_1039&DEV_6001.DeviceDesc = "SiS PCI-To-PCI Bridge"
PCI\VEN_1039&DEV_0755.DeviceDesc = "SiS755  Host CPU Bridge"
PCI\VEN_1039&DEV_0760.DeviceDesc = "SiS760  Host CPU Bridge"
PCI\VEN_1039&DEV_0756.DeviceDesc = "SiS756  Host CPU Bridge"
PCI\VEN_1039&DEV_0761.DeviceDesc = "SiS761  Host CPU Bridge"
PCI\VEN_1039&DEV_0648.DeviceDesc = "SiS648  Host CPU Bridge"
PCI\VEN_1039&DEV_0649.DeviceDesc = "SiS649  Host CPU Bridge"
PCI\VEN_1039&DEV_0655.DeviceDesc = "SiS655  Host CPU Bridge"
PCI\VEN_1039&DEV_0656.DeviceDesc = "SiS656  Host CPU Bridge"
PCI\VEN_1039&DEV_0661.DeviceDesc = "SiS661  Host CPU Bridge"
PCI\VEN_1039&DEV_0963.DeviceDesc = "SiS963  PCI to LPC Bridge"
PCI\VEN_1039&DEV_0964.DeviceDesc = "SiS964  PCI to LPC Bridge"
PCI\VEN_1039&DEV_0965.DeviceDesc = "SiS965  PCI to LPC Bridge"
PCI\VEN_1039&DEV_0966.DeviceDesc = "SiS966  PCI to LPC Bridge"
PCI\VEN_1039&DEV_0004.DeviceDesc = "SiS PCI Express x16 Root Port"
PCI\VEN_1039&DEV_000A.DeviceDesc = "SiS PCI Express x1 Root Port"
PCI\VEN_1039&DEV_0662.DeviceDesc = "SiS662 Host CPU Bridge"
PCI\VEN_1039&DEV_0741.DeviceDesc = "SiS741 Host CPU Bridge"

SMSC_MFG = "Standard Microsystems Corp."
PCI\VEN_1055&DEV_9460.DeviceDesc = "SMSC SLC90E66 PCI to ISA Bridge"
PCI\VEN_1055&DEV_9463.DeviceDesc = "SMSC SLC90E66 Power Management Controller"

TEXAS_MFG = "Texas Instruments"
PCI\VEN_104C&DEV_AC20.DeviceDesc = "TI 2030 PCI to PCI bridge"

TOSHIBA_MFG = "Toshiba"
PCI\VEN_1179&DEV_0601.DeviceDesc = "Toshiba CPU to PCI & PCI to ISA bridge"
PCI\VEN_1179&DEV_0618.DeviceDesc = "Toshiba CPU to PCI & PCI to ISA bridge"
PCI\VEN_1179&DEV_0602.DeviceDesc = "Toshiba PCI to ISA bridge"
PCI\VEN_1179&DEV_0603.DeviceDesc = "Toshiba PC Card Standard compatible Controller"
PCI\VEN_1179&DEV_0604.DeviceDesc = "Toshiba PCI-Docking Host bridge"
PCI\VEN_1179&DEV_0605.DeviceDesc = "Toshiba PCI-Docking bridge"
PCI\VEN_1179&DEV_0609.DeviceDesc = "Toshiba PCI-Docking bridge"
PCI\VEN_1179&DEV_0611.DeviceDesc = "Toshiba PCI to ISA bridge"

ULI_MFG = "ULI"
PCI\VEN_10B9&DEV_5246.DeviceDesc = "ULi AGP v3.0 Controller"

UMC_MFG = "UMC"
PCI\VEN_1060&DEV_8886.DeviceDesc = "UMC PCI to ISA bridge for desktop [without IDE support]"
PCI\VEN_1060&DEV_886A.DeviceDesc = "UMC PCI to ISA bridge for desktop [with IDE support]"
PCI\VEN_1060&DEV_E886.DeviceDesc = "UMC PCI to ISA bridge for notebook [with IDE support]"
PCI\VEN_1060&DEV_8881.DeviceDesc = "UMC 486 CPU to PCI bridge for desktop"
PCI\VEN_1060&DEV_0891.DeviceDesc = "UMC Pentium(r) CPU to PCI bridge for desktop"
PCI\VEN_1060&DEV_E881.DeviceDesc = "UMC 486 CPU to PCI bridge for notebook"
PCI\VEN_1060&DEV_E891.DeviceDesc = "UMC Pentium(r) CPU to PCI bridge for notebook"

VIA_MFG = "VIA"
PCI\VEN_1106&DEV_0204.DeviceDesc = "VIA CPU to PCI Bridge"
PCI\VEN_1106&DEV_0208.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_0238.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_0258.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_0259.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_0269.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_0282.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_0296.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_0305.DeviceDesc = "VIA CPU to PCI bridge"
PCI\VEN_1106&DEV_0308.DeviceDesc = "VIA CPU to PCI bridge"
PCI\VEN_1106&DEV_0314.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_0324.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_0327.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_0336.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_0340.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_0351.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_0353.DeviceDesc = "VIA MSP Standard Host Bridge"
PCI\VEN_1106&DEV_0364.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_0391.DeviceDesc = "VIA CPU to PCI bridge"
PCI\VEN_1106&DEV_0409.DeviceDesc = "VIA MSP Standard Host Bridge"
PCI\VEN_1106&DEV_0501.DeviceDesc = "VIA CPU to PCI bridge"
PCI\VEN_1106&DEV_0505.DeviceDesc = "VIA 82C5x5 CPU to PCI & PCI to ISA bridge"
PCI\VEN_1106&DEV_0576.DeviceDesc = "VIA 82C576 CPU to PCI & PCI to ISA bridge"
PCI\VEN_1106&DEV_0586.DeviceDesc = "VIA 82C586B (PIPC) PCI to ISA bridge"
PCI\VEN_1106&DEV_0596.DeviceDesc = "VIA PCI to ISA bridge"
PCI\VEN_1106&DEV_0597.DeviceDesc = "VIA V82C597 CPU to PCI bridge"
PCI\VEN_1106&DEV_0598.DeviceDesc = "VIA V82C598 CPU to PCI bridge"
PCI\VEN_1106&DEV_0601.DeviceDesc = "VIA CPU to PCI bridge"
PCI\VEN_1106&DEV_0605.DeviceDesc = "VIA CPU to PCI bridge"
PCI\VEN_1106&DEV_0691.DeviceDesc = "VIA CPU to PCI bridge"
PCI\VEN_1106&DEV_0686.DeviceDesc = "VIA PCI to ISA bridge"
PCI\VEN_1106&DEV_1204.DeviceDesc = "VIA CPU to PCI Bridge"
PCI\VEN_1106&DEV_1208.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_1238.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_1258.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_1259.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_1269.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_1282.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_1296.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_1308.DeviceDesc = "VIA CPU to PCI bridge"
PCI\VEN_1106&DEV_1314.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_1324.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_1327.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_1336.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_1340.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_1351.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_1353.DeviceDesc = "VIA MSP Standard Host Bridge"
PCI\VEN_1106&DEV_1364.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_1409.DeviceDesc = "VIA MSP Standard Host Bridge"
PCI\VEN_1106&DEV_2204.DeviceDesc = "VIA CPU to PCI Bridge"
PCI\VEN_1106&DEV_2208.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_2238.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_2258.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_2259.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_2269.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_2282.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_2296.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_2308.DeviceDesc = "VIA CPU to PCI bridge"
PCI\VEN_1106&DEV_2314.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_2324.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_2327.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_2336.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_2340.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_2351.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_2353.DeviceDesc = "VIA MSP Standard Host Bridge"
PCI\VEN_1106&DEV_2364.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_2409.DeviceDesc = "VIA MSP Standard Host Bridge"
PCI\VEN_1106&DEV_287A.DeviceDesc = "VIA Standard PCI to PCI Bridge"
PCI\VEN_1106&DEV_287B&CC_0604.DeviceDesc = "VIA Standard PCI to PCIE Bridge"
PCI\VEN_1106&DEV_287B&CC_0600.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_287C.DeviceDesc = "VIA Standard PCIE Root Port"
PCI\VEN_1106&DEV_287D.DeviceDesc = "VIA Standard PCIE Root Port"
PCI\VEN_1106&DEV_287E.DeviceDesc = "VIA Ultra VLINK Controller"
PCI\VEN_1106&DEV_3040.DeviceDesc = "VIA 82C586B Power Management Controller"
PCI\VEN_1106&DEV_3050.DeviceDesc = "VIA Power Management Controller"
PCI\VEN_1106&DEV_3051.DeviceDesc = "VIA Power Management Controller"
PCI\VEN_1106&DEV_3057.DeviceDesc = "VIA Power Management controller"
PCI\VEN_1106&DEV_3074.DeviceDesc = "VIA PCI to ISA bridge"
PCI\VEN_1106&DEV_3091.DeviceDesc = "VIA CPU to PCI bridge"
PCI\VEN_1106&DEV_3099.DeviceDesc = "VIA CPU to PCI Bridge"
PCI\VEN_1106&DEV_3101.DeviceDesc = "VIA CPU to PCI Bridge"
PCI\VEN_1106&DEV_3109.DeviceDesc = "VIA PCI to ISA bridge"
PCI\VEN_1106&DEV_3112.DeviceDesc = "VIA CPU to PCI Bridge"
PCI\VEN_1106&DEV_3113.DeviceDesc = "VIA VPX PCI to PCI Bridge"
PCI\VEN_1106&DEV_3116.DeviceDesc = "VIA Standard CPU to PCI Bridge"
PCI\VEN_1106&DEV_3123.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_3128.DeviceDesc = "VIA P4X266  CPU to PCI bridge"
PCI\VEN_1106&DEV_3147.DeviceDesc = "VIA VT8233A PCI to ISA bridge"
PCI\VEN_1106&DEV_3148.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_3156.DeviceDesc = "VIA Standard CPU to PCI Bridge"
PCI\VEN_1106&DEV_3168.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_3177.DeviceDesc = "VIA Standard PCI to ISA bridge"
PCI\VEN_1106&DEV_3188.DeviceDesc = "VIA Standard CPU to PCI Bridge"
PCI\VEN_1106&DEV_3189.DeviceDesc = "VIA Standard CPU to PCI Bridge"
PCI\VEN_1106&DEV_3204.DeviceDesc = "VIA CPU to PCI Bridge"
PCI\VEN_1106&DEV_3205.DeviceDesc = "VIA Standard CPU to PCI Bridge"
PCI\VEN_1106&DEV_3208.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_3227.DeviceDesc = "VIA Standard PCI to ISA Bridge"
PCI\VEN_1106&DEV_3238.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_324A.DeviceDesc = "VIA PCI to PCI Bridge Controller"
PCI\VEN_1106&DEV_324B&CC_0600.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_324E.DeviceDesc = "VIA Internal Module Bus"
PCI\VEN_1106&DEV_3258.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_3259.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_3269.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_3282.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_3287.DeviceDesc = "VIA Standard PCI to ISA Bridge"
PCI\VEN_1106&DEV_3296.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_3314.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_3324.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_3327.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_3336.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_3337.DeviceDesc = "VIA Standard PCI to ISA Bridge"
PCI\VEN_1106&DEV_3340.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_3351.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_3353.DeviceDesc = "VIA MSP DRAM Controller"
PCI\VEN_1106&DEV_3364.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_337A.DeviceDesc = "VIA Standard PCI to PCI Bridge"
PCI\VEN_1106&DEV_337B&CC_0600.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_3409.DeviceDesc = "VIA MSP DRAM Controller"
PCI\VEN_1106&DEV_4204.DeviceDesc = "VIA CPU to PCI Bridge"
PCI\VEN_1106&DEV_4208.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_4238.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_4258.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_4259.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_4269.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_4282.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_4296.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_4308.DeviceDesc = "VIA CPU to PCI Bridge"
PCI\VEN_1106&DEV_4314.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_4324.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_4327.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_4336.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_4340.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_4351.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_4353.DeviceDesc = "VIA MSP Power Management Controller"
PCI\VEN_1106&DEV_4364.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_4409.DeviceDesc = "VIA MSP Power Management Controller"
PCI\VEN_1106&DEV_5208.DeviceDesc = "VIA I/O APIC Interrupt Controller"
PCI\VEN_1106&DEV_5238.DeviceDesc = "VIA I/O APIC Interrupt Controller"
PCI\VEN_1106&DEV_5308.DeviceDesc = "VIA I/O APIC Interrupt Controller"
PCI\VEN_1106&DEV_5327.DeviceDesc = "VIA I/O APIC Interrupt Controller"
PCI\VEN_1106&DEV_5336.DeviceDesc = "VIA I/O APIC Interrupt Controller"
PCI\VEN_1106&DEV_5340.DeviceDesc = "VIA I/O APIC Interrupt Controller"
PCI\VEN_1106&DEV_5351.DeviceDesc = "VIA I/O APIC Interrupt Controller"
PCI\VEN_1106&DEV_5353.DeviceDesc = "VIA MSP I/O APIC"
PCI\VEN_1106&DEV_5364.DeviceDesc = "VIA I/O APIC Interrupt Controller"
PCI\VEN_1106&DEV_5409.DeviceDesc = "VIA MSP I/O APIC"
PCI\VEN_1106&DEV_6327.DeviceDesc = "VIA Security Device"
PCI\VEN_1106&DEV_6340.DeviceDesc = "VIA Security Device"
PCI\VEN_1106&DEV_6353.DeviceDesc = "VIA MSP Scratch Device"
PCI\VEN_1106&DEV_6364.DeviceDesc = "VIA Security Device"
PCI\VEN_1106&DEV_6409.DeviceDesc = "VIA MSP Scratch Device"
PCI\VEN_1106&DEV_7204.DeviceDesc = "VIA CPU to PCI Bridge"
PCI\VEN_1106&DEV_7208.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_7238.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_7258.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_7259.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_7269.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_7296.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_7282.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_7308.DeviceDesc = "VIA CPU to PCI Bridge"
PCI\VEN_1106&DEV_7314.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_7324.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_7327.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_7336.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_7340.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_7351.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_7353.DeviceDesc = "VIA MSP Standard Host Bridge"
PCI\VEN_1106&DEV_7364.DeviceDesc = "VIA Standard Host Bridge"
PCI\VEN_1106&DEV_7409.DeviceDesc = "VIA MSP Standard Host Bridge"
PCI\VEN_1106&DEV_8231.DeviceDesc = "VIA PCI to ISA bridge"
PCI\VEN_1106&DEV_8235.DeviceDesc = "VIA Power Management Controller"
PCI\VEN_1106&DEV_8305.DeviceDesc = "VIA CPU to AGP Controller"
PCI\VEN_1106&DEV_8324.DeviceDesc = "VIA PCI to ISA bridge"
PCI\VEN_1106&DEV_8353.DeviceDesc = "VIA MSP Miscellaneous Bus"
PCI\VEN_1106&DEV_8391.DeviceDesc = "VIA CPU to AGP Controller"
PCI\VEN_1106&DEV_8409.DeviceDesc = "VIA MSP Miscellaneous Bus"
PCI\VEN_1106&DEV_8598.DeviceDesc = "VIA CPU to AGP Controller"
PCI\VEN_1106&DEV_8501.DeviceDesc = "VIA CPU to AGP Controller"
PCI\VEN_1106&DEV_8601.DeviceDesc = "VIA CPU to AGP Controller"
PCI\VEN_1106&DEV_8605.DeviceDesc = "VIA CPU to AGP Controller"
PCI\VEN_1106&DEV_A208.DeviceDesc = "VIA PCI to PCI Bridge Controller"
PCI\VEN_1106&DEV_A238.DeviceDesc = "VIA PCI to PCI Bridge Controller"
PCI\VEN_1106&DEV_A327.DeviceDesc = "VIA PCI to PCI Bridge Controller"
PCI\VEN_1106&DEV_A353.DeviceDesc = "VIA MSP Module Bus"
PCI\VEN_1106&DEV_A364.DeviceDesc = "VIA PCI to PCI Bridge Controller"
PCI\VEN_1106&DEV_B091.DeviceDesc = "VIA CPU to AGP Controller"
PCI\VEN_1107&DEV_0576.DeviceDesc = "VIA 82C576 CPU to PCI & PCI to ISA bridge"
PCI\VEN_1106&DEV_B099.DeviceDesc = "VIA CPU to AGP Controller"
PCI\VEN_1106&DEV_B112.DeviceDesc = "VIA CPU to AGP Controller"
PCI\VEN_1106&DEV_B113.DeviceDesc = "VIA VPX I/O APIC"
PCI\VEN_1106&DEV_B168.DeviceDesc = "VIA CPU to AGP Controller"
PCI\VEN_1106&DEV_B353.DeviceDesc = "VIA MSP PCI to PCI Bridge"
PCI\VEN_1106&DEV_C208.DeviceDesc = "VIA PCI to PCI Bridge Controller"
PCI\VEN_1106&DEV_C238.DeviceDesc = "VIA PCI to PCI Bridge Controller"
PCI\VEN_1106&DEV_C327.DeviceDesc = "VIA PCI to PCI Bridge Controller"
PCI\VEN_1106&DEV_C340.DeviceDesc = "VIA PCI to PCI Bridge Controller"
PCI\VEN_1106&DEV_C353.DeviceDesc = "VIA MSP PCI Express Root Port"
PCI\VEN_1106&DEV_C364.DeviceDesc = "VIA PCI to PCI Bridge Controller"
PCI\VEN_1106&DEV_D208.DeviceDesc = "VIA PCI to PCI Bridge Controller"
PCI\VEN_1106&DEV_D238.DeviceDesc = "VIA PCI to PCI Bridge Controller"
PCI\VEN_1106&DEV_D340.DeviceDesc = "VIA PCI to PCI Bridge Controller"
PCI\VEN_1106&DEV_E208.DeviceDesc = "VIA PCI to PCI Bridge Controller"
PCI\VEN_1106&DEV_E238.DeviceDesc = "VIA PCI to PCI Bridge Controller"
PCI\VEN_1106&DEV_E340.DeviceDesc = "VIA PCI to PCI Bridge Controller"
PCI\VEN_1106&DEV_E353.DeviceDesc = "VIA MSP PCI Express Root Port"
PCI\VEN_1106&DEV_F208.DeviceDesc = "VIA PCI to PCI Bridge Controller"
PCI\VEN_1106&DEV_F238.DeviceDesc = "VIA PCI to PCI Bridge Controller"
PCI\VEN_1106&DEV_F340.DeviceDesc = "VIA PCI to PCI Bridge Controller"
PCI\VEN_1106&DEV_F353.DeviceDesc = "VIA MSP PCI Express Root Port"

VLSI_MFG = "VLSI"
PCI\VEN_1004&DEV_0005.DeviceDesc = "VLSI Pentium(r) CPU to PCI bridge"
PCI\VEN_1004&DEV_0006.DeviceDesc = "VLSI PCI to ISA Plug and Play bridge"
PCI\VEN_1004&DEV_0101.DeviceDesc = "VLSI VL82C532 PCI Peripheral Controller (PCI to ISA bridge)"
PCI\VEN_1004&DEV_0102.DeviceDesc = "VLSI VL82C534 PCI to PCI bridge"
PCI\VEN_1004&DEV_0103.DeviceDesc = "VLSI VL82C538 PCI to ISA bridge"
PCI\VEN_1004&DEV_0104.DeviceDesc = "VLSI VL82C535 CPU to PCI bridge"

;*******************************************
PCISlot = "PCI Slot %1!u!"
;*******************************************
;service descriptions
pci_svcdesc = "PCI Bus Driver"
msisadrv_svcdesc = "ISA/EISA Class Driver"
isapnp_svcdesc = "PnP ISA/EISA Bus Driver"
volmgr_svcdesc = "Volume Manager Driver"
swenum_svcdesc = "Software Bus Driver"
vdrvroot_svcdesc = "Microsoft Virtual Drive Enumerator Driver"

mssmbios_svcdesc = "Microsoft System Management BIOS Driver"
uagp35_svcdesc = "Microsoft AGPv3.5 Filter"

agp440_svcdesc = "Intel AGP Bus Filter"
agp460_svcdesc = "Intel AGP Bus Filter"
agpali_svcdesc = "ALI AGP Bus Filter"
sisagp_svcdesc = "SIS AGP Bus Filter"
agpvia_svcdesc = "VIA AGP Bus Filter"
amdagp_svcdesc = "AMD AGP Bus Filter Driver"
gagp30kx_svcdesc = "Microsoft Generic AGPv3.0 Filter for K8 Processor Platforms"
agpnvidia_svcdesc = "NVIDIA nForce AGP Bus Filter"
uliagpkx_svcdesc = "Uli AGP Bus Filter"

;*******************************************
;Non-localizable
SPSVCINST_ASSOCSERVICE = 0x00000002
SERVICE_KERNEL_DRIVER  = 1
SERVICE_BOOT_START     = 0
SERVICE_SYSTEM_START   = 1
SERVICE_DEMAND_START   = 3
SERVICE_ERROR_NORMAL   = 1
SERVICE_ERROR_CRITICAL = 3
REG_EXPAND_SZ          = 0x00020000
REG_DWORD              = 0x00010001
