;
; LSI_SAS2.INF - version WIN7.1 - LSI Corporation
;
; This is the INF file for Windows (in-box) for the LSI_SAS2 based
; PCI MPT environment (SAS2 devices)
;
; Copyright (c) LSI Corporation


[version]
signature="$Windows NT$"
Class=SCSIAdapter
ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318}
Provider=%LSI%
DriverVer=02/20/2009,2.00.02.71

;
; Source file information
;

[SourceDisksNames]
3426=windows cd

[SourceDisksFiles]
lsi_sas2.sys = 3426

[DestinationDirs]
DefaultDestDir = 12 ; DIRID_DRIVERS

[Manufacturer]
%LSI%=LSI,NTx86,NTia64,NTamd64
%DELL%=DELL,NTx86,NTia64,NTamd64

[LSI]

[LSI.NTx86]
%DevDesc1% = LSI_SAS_Inst, PCI\VEN_1000&DEV_0064
%DevDesc2% = LSI_SAS_Inst, PCI\VEN_1000&DEV_0065
%DevDesc3% = LSI_SAS_Inst, PCI\VEN_1000&DEV_0070
%DevDesc4% = LSI_SAS_Inst, PCI\VEN_1000&DEV_0072
%DevDesc5% = LSI_SAS_Inst, PCI\VEN_1000&DEV_0074
%DevDesc6% = LSI_SAS_Inst, PCI\VEN_1000&DEV_0076
%DevDesc7% = LSI_SAS_Inst, PCI\VEN_1000&DEV_0077

[LSI.NTia64]
%DevDesc1% = LSI_SAS_Inst, PCI\VEN_1000&DEV_0064
%DevDesc2% = LSI_SAS_Inst, PCI\VEN_1000&DEV_0065
%DevDesc3% = LSI_SAS_Inst, PCI\VEN_1000&DEV_0070
%DevDesc4% = LSI_SAS_Inst, PCI\VEN_1000&DEV_0072
%DevDesc5% = LSI_SAS_Inst, PCI\VEN_1000&DEV_0074
%DevDesc6% = LSI_SAS_Inst, PCI\VEN_1000&DEV_0076
%DevDesc7% = LSI_SAS_Inst, PCI\VEN_1000&DEV_0077

[LSI.NTamd64]
%DevDesc1% = LSI_SAS_Inst, PCI\VEN_1000&DEV_0064
%DevDesc2% = LSI_SAS_Inst, PCI\VEN_1000&DEV_0065
%DevDesc3% = LSI_SAS_Inst, PCI\VEN_1000&DEV_0070
%DevDesc4% = LSI_SAS_Inst, PCI\VEN_1000&DEV_0072
%DevDesc5% = LSI_SAS_Inst, PCI\VEN_1000&DEV_0074
%DevDesc6% = LSI_SAS_Inst, PCI\VEN_1000&DEV_0076
%DevDesc7% = LSI_SAS_Inst, PCI\VEN_1000&DEV_0077

[DELL]

[DELL.NTx86]
%DevDescD1% = LSI_SAS_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F1C1028
%DevDescD2% = LSI_SAS_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F1D1028
%DevDescD3% = LSI_SAS_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F1E1028
%DevDescD4% = LSI_SAS_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F1F1028
%DevDescD5% = LSI_SAS_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F201028
%DevDescD6% = LSI_SAS_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F211028
%DevDescD7% = LSI_SAS_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F221028

[DELL.NTia64]
%DevDescD1% = LSI_SAS_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F1C1028
%DevDescD2% = LSI_SAS_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F1D1028
%DevDescD3% = LSI_SAS_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F1E1028
%DevDescD4% = LSI_SAS_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F1F1028
%DevDescD5% = LSI_SAS_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F201028
%DevDescD6% = LSI_SAS_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F211028
%DevDescD7% = LSI_SAS_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F221028

[DELL.NTamd64]
%DevDescD1% = LSI_SAS_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F1C1028
%DevDescD2% = LSI_SAS_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F1D1028
%DevDescD3% = LSI_SAS_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F1E1028
%DevDescD4% = LSI_SAS_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F1F1028
%DevDescD5% = LSI_SAS_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F201028
%DevDescD6% = LSI_SAS_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F211028
%DevDescD7% = LSI_SAS_Dell_Inst, PCI\VEN_1000&DEV_0072&SUBSYS_1F221028

[ControlFlags]
ExcludeFromSelect = *

[LSI_SAS_Inst]
CopyFiles = LSI_SAS_CopyFiles

[LSI_SAS_Inst.HW]
DelReg = LegacyScsiportValues
AddReg = InterruptMgmtValues
Include = machine.inf
Needs = PciIoSpaceNotRequired

[LSI_SAS_Inst.Services]
AddService = LSI_SAS2, %SPSVCINST_ASSOCSERVICE%, LSI_SAS_Service_Inst, Miniport_EventLog_Inst

[LSI_SAS_Dell_Inst]
CopyFiles = LSI_SAS_CopyFiles
AddReg = LSI_SAS_Dell_AddReg

[LSI_SAS_Dell_Inst.HW]
DelReg = LegacyScsiportValues
AddReg = InterruptMgmtValues
Include = machine.inf
Needs = PciIoSpaceNotRequired

[LSI_SAS_Dell_Inst.Services]
AddService = LSI_SAS2, %SPSVCINST_ASSOCSERVICE%, LSI_SAS_Service_Inst, Miniport_EventLog_Inst

[LSI_SAS_Dell_AddReg]
HKLM,SYSTEM\CurrentControlSet\Services\Disk,TimeOutValue,0x00010001,0x0000003C

[LSI_SAS_Service_Inst]
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\lsi_sas2.sys
LoadOrderGroup = SCSI Miniport
AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type_sas

[LSI_SAS_CopyFiles]
lsi_sas2.sys,,,1

[LegacyScsiportValues]
HKR,Scsiport,BusNumber
HKR,Scsiport,LegacyInterfaceType
HKR,Scsiport,SlotNumber

[InterruptMgmtValues]
HKR,"Interrupt Management",0x00000010
HKR,"Interrupt Management\MessageSignaledInterruptProperties",0x00000010
HKR,"Interrupt Management\MessageSignaledInterruptProperties",MSISupported,0x00010001,1

[pnpsafe_pci_addreg]
HKR, "Parameters\PnpInterface", "5", 0x00010001, 0x00000001

[bus_type_sas]
HKR, "Parameters", "BusType", 0x00010001, 0x0000000A

[Miniport_EventLog_Inst]
AddReg = Miniport_EventLog_AddReg

[Miniport_EventLog_AddReg]
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll"
HKR,,TypesSupported,%REG_DWORD%,7

[Strings]
;Localizable Strings needed for HBA naming in Windows UI
LSI = "LSI"
DELL = "Dell"
DevDesc1 = "LSI Adapter, SAS2 2116 Meteor ROC(E)"
DevDesc2 = "LSI Adapter, SAS2 2116 Meteor ROC"
DevDesc3 = "LSI Adapter, SAS2 2004 Spitfire"
DevDesc4 = "LSI Adapter, SAS2 2008 Falcon"
DevDesc5 = "LSI Adapter, SAS2 2108 Liberator"
DevDesc6 = "LSI Adapter, SAS2 2108 Liberator ROC(E)"
DevDesc7 = "LSI Adapter, SAS2 2108 Liberator ROC"
DevDescD1 = "6Gbps SAS HBA"
DevDescD2 = "PERC H200 Adapter"
DevDescD3 = "PERC H200 Integrated"
DevDescD4 = "PERC H200 Modular"
DevDescD5 = "PERC H200 Embedded"
DevDescD6 = "PERC H200"
DevDescD7 = "6Gbps SAS"

;*******************************************
;Non-Localizable strings
SPSVCINST_ASSOCSERVICE = 0x00000002
SERVICE_KERNEL_DRIVER  = 1
SERVICE_BOOT_START     = 0
SERVICE_ERROR_NORMAL   = 1
REG_EXPAND_SZ          = 0x00020000
REG_DWORD              = 0x00010001
