[strings.0804]
;Non-Localizable Strings
  MS=				  "Microsoft"
  PROVIDER=                       "Eicon Networks"
  PROVIDERPRODUCT=                "Eicon Networks Diva Server"
  PRIVITEMID_CARD=                "{2CD6D901-506B-11d1-BF23-00A0242DD63F}"
  DRVDIR=                         "disdn"

  DIVA_CT_ST_DISP=         "Eicon Diva Server ISDN+CT S/T (PCI)"
  DIVA_CT_ST_V20_DISP=     "Eicon Diva Server ISDN+CT S/T V2.0 (PCI)"
  DIVA_PRO20_PCI_DISP=     "Eicon DIVA Pro 2.0 S/T (PCI)"
  DIVA_20_PCI_DISP=        "Eicon DIVA 2.0 S/T (PCI)"
  DIVA_202_PCI_DISP=       "Eicon DIVA 2.02 S/T (PCI)"
  DIVA_PRO30_PCI_DISP=     "Eicon Diva Pro 3.0 (PCI)"
  DIVA_PCMCIA_DISP=        "Eicon DIVA/PCM (PCMCIA)"
  DIVA_PCMCIA_V2_DISP=     "Eicon Diva PC Card (PCMCIA)"
  DIVA_____PCMCIA_DISP=    "Eicon Diva PC Card (PCMCIA)"
  DIVA_PRO_PCMCIA_DISP=    "Eicon DIVA Pro (PCMCIA)"
  DIVA_PRO_PCMCIA_V3_DISP= "Eicon Diva Pro 3.0 (PCMCIA)"
  DIVA_LOW_USB_DISP=       "Eicon Diva USB 2.01 S/T"
  TELEDAT_SURF_USB_DISP=   "Teledat Surf USB"
  DIVA_LOW_USBV2_DISP=     "Eicon Diva ISDN USB 2.0"

  ; friendly server names
  DIVA_DISP=                      "Eicon Driver for all DIVA PnP cards"
  DIVACO_DISP=                    "Eicon Connection Oriented Driver for all Diva PnP cards"
  MAINT_DISP=                     "Eicon Maintenance Driver"
  CAPI_DISP=                      "Eicon CAPI 2.0 Driver"
  CAPI20=                         "CAPI20"

  SERVER_DISK_1_LABEL=			  "Diva Client for Windows Setup"


  ; registry data types
  ;     types with NCLOB don't overwrite existing values
  REG_SZ=                         0x00000000
  REG_SZ_NCLOB=                   0x00000002
  REG_MSZ=                        0x00010000
  REG_MSZ_NCLOB=                  0x00010002
;  REG_MSZ_APPEND=                 0x0001000A
;  REG_MSZ_DELVAL=                 0x00010006
  REG_ESZ=                        0x00020000
  REG_DW=                         0x00010001
  REG_DW_NCLOB=                   0x00010003
 
  ; bus types [ USB isn't existing, fake as Internal (or PCI)? ]
  ISA=                            1
  MCA=                            3
  PCI=                            5
  PCMCIA=                         8
  ISAPNP=                         14
  USB=                            15

  ; device characteristics
  NCF_PHYSICAL=                   0x04
  NCF_HAS_UI=                     0x80


;***************************************************
; Supported Switch Types for Server cards:
;  [ISDN_SWITCH_AUTO(0x01)]	| ISDN_SWITCH_ATT(0x02
;  ISDN_SWITCH_NI1(0x04)    | ISDN_SWITCH_NTI(0x08)
;  ISDN_SWITCH_INS64(0x10)  | ISDN_SWITCH_1TR6(0x20)
;  ISDN_SWITCH_VN3(0x40)    | ISDN_SWITCH_DSS1(0x80)
;  ISDN_SWITCH_AUS(0x100)   | ISDN_SWITCH_BEL(0x200)
;  ISDN_SWITCH_SWE(0x1000)  | ISDN_SWITCH_ITA(0x2000)
;  ISDN_SWITCH_TWN(0x4000)
;***************************************************
  GENERIC_ISDNSWITCHTYPES=  0x73DE
  CLIENT_ISDNSWITCHTYPES=  0x73DE

;[strings.0007]

;*** end *********************************************************************

;Localizable Strings
