; Copyright (c) 2006-2009, Microsoft

[version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %MSFT%
DriverVer=04/06/2009,11.0.5.21

[Manufacturer]
%Intel%     = Intel, NTx86.6.0

[ControlFlags]
ExcludeFromSelect = *


[Intel]

[Intel.NTx86.6.0]

; DisplayName                   Section                DeviceID
; -----------                   -------                --------
%E10A7NC.DeviceDesc%            = E10A7,               PCI\VEN_8086&DEV_10A7
%E10A9NC.DeviceDesc%            = E10A9,               PCI\VEN_8086&DEV_10A9
%E10A7DD.DeviceDesc%            = NO_DRV,              PCI\VEN_8086&DEV_10A6
%E10D6NC.DeviceDesc%            = E10D6PM,             PCI\VEN_8086&DEV_10D6&SUBSYS_147A8086
%E10A7NC.DeviceDesc%            = E10A7,               PCI\VEN_8086&DEV_10A7&SUBSYS_10A88086
%E10D3NC.DeviceDesc%            = E10D3,               PCI\VEN_8086&DEV_10D3
%EA01FNC.DeviceDesc%            = E10D3,               PCI\VEN_8086&DEV_10D3&SUBSYS_A01F8086
%E10C9LNC.DeviceDesc%           = E10C9,               PCI\VEN_8086&DEV_10C9
%E10E6LNC.DeviceDesc%           = E10E6,               PCI\VEN_8086&DEV_10E6
%E10E7NC.DeviceDesc%            = E10E6,               PCI\VEN_8086&DEV_10E7
%E10C9NC.DeviceDesc%            = E10C9PM,             PCI\VEN_8086&DEV_10C9&SUBSYS_A01C8086
%E10C9NC.DeviceDesc%            = E10C9PM,             PCI\VEN_8086&DEV_10C9&SUBSYS_A03C8086
%E10E6NC.DeviceDesc%            = E10E6PM,             PCI\VEN_8086&DEV_10E6&SUBSYS_A01F8086
%E10E6NC.DeviceDesc%            = E10E6PM,             PCI\VEN_8086&DEV_10E6&SUBSYS_A02F8086
%E10E8NC.DeviceDesc%            = E10E8PM,             PCI\VEN_8086&DEV_10E8&SUBSYS_A02C8086
%E10D3NC.DeviceDesc%            = E10D3,               PCI\VEN_8086&DEV_10F6







;===============================================================================
;
;
;===============================================================================

;-------------------------------------------------------------------------------
; Intel 82575EB Gigabit Network Connection
;
[E10A7]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
AddReg          = e1q.reg, Copper.reg, Copper1000.reg
AddReg          = JumboPacket.reg
AddReg          = TcpSeg.reg, RSS.reg, RSS4Q.reg, HDSplit.reg
CopyFiles       = winvista.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[E10A7.Services]
AddService = e1qexpress, 2, winvista.Service, winvista.EventLog


[E10A7.HW]
Include=machine.inf
Needs=PciIoSpaceNotRequired
AddReg=MSIX.reg

;-------------------------------------------------------------------------------
; Intel(R) 82575EB Gigabit Backplane Connection
;
[E10A9]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
AddReg          = e1q.reg
AddReg          = JumboPacket.reg
AddReg          = TcpSeg.reg, RSS.reg, RSS4Q.reg, HDSplit.reg
CopyFiles       = winvista.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[E10A9.Services]
AddService = e1qexpress, 2, winvista.Service, winvista.EventLog


[E10A9.HW]
Include=machine.inf
Needs=PciIoSpaceNotRequired
AddReg=MSIX.reg

;-------------------------------------------------------------------------------
; Intel(R) Gigabit VT Quad Port Network Connection
;
[E10D6PM]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
AddReg          = e1q.reg, Copper.reg, Copper1000.reg
AddReg          = JumboPacket.reg
AddReg          = TcpSeg.reg, RSS.reg, RSS4Q.reg, HDSplit.reg
CopyFiles       = winvista.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[E10D6PM.Services]
AddService = e1qexpress, 2, winvista.Service, winvista.EventLog


[E10D6PM.HW]
Include=machine.inf
Needs=PciIoSpaceNotRequired
AddReg=MSIX.reg

;-------------------------------------------------------------------------------
; Intel(R) 82574 Gigabit Network Connection
;
[E10D3]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
AddReg          = e1q.reg, Copper.reg, Copper1000.reg
AddReg          = JumboPacket.reg
AddReg          = TcpSeg.reg, RSS.reg, RSS2Q.reg
CopyFiles       = winvista.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[E10D3.Services]
AddService = e1qexpress, 2, winvista.Service, winvista.EventLog


[E10D3.HW]
Include=machine.inf
Needs=PciIoSpaceNotRequired
AddReg=MSIX3.reg

;-------------------------------------------------------------------------------
; Intel(R) 82576 Gigabit Dual Port Network Connection
;-------------------------------------------------------------------------------
[E10C9]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
AddReg          = e1q.reg, Copper.reg, Copper1000.reg
AddReg          = JumboPacket.reg
AddReg          = TcpSeg.reg, RSS.reg, RSS8Q.reg, HDSplit.reg, IPSec.reg
CopyFiles       = winvista.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[E10C9.Services]
AddService = e1qexpress, 2, winvista.Service, winvista.EventLog


[E10C9.HW]
Include=machine.inf
Needs=PciIoSpaceNotRequired
AddReg=MSIX10.reg

;-------------------------------------------------------------------------------
; Intel(R) 82576 Gigabit Dual Port Network Connection
;-------------------------------------------------------------------------------
[E10E6]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
AddReg          = e1q.reg
AddReg          = JumboPacket.reg
AddReg          = TcpSeg.reg, RSS.reg, RSS8Q.reg, HDSplit.reg, IPSec.reg
CopyFiles       = winvista.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[E10E6.Services]
AddService = e1qexpress, 2, winvista.Service, winvista.EventLog


[E10E6.HW]
Include=machine.inf
Needs=PciIoSpaceNotRequired
AddReg=MSIX10.reg

;-------------------------------------------------------------------------------
; Intel(R) Gigabit ET Dual Port Server Adapter
;-------------------------------------------------------------------------------

[E10C9PM]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
AddReg          = e1q.reg, Copper.reg, Copper1000.reg
AddReg          = JumboPacket.reg
AddReg          = TcpSeg.reg, RSS.reg, RSS8Q.reg, HDSplit.reg, IPSec.reg
CopyFiles       = winvista.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[E10C9PM.Services]
AddService = e1qexpress, 2, winvista.Service, winvista.EventLog


[E10C9PM.HW]
Include=machine.inf
Needs=PciIoSpaceNotRequired
AddReg=MSIX10.reg

;-------------------------------------------------------------------------------
; Intel(R) Gigabit EF Dual Port Server Adapter
;-------------------------------------------------------------------------------
[E10E6PM]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
AddReg          = e1q.reg
AddReg          = JumboPacket.reg
AddReg          = TcpSeg.reg, RSS.reg, RSS8Q.reg, HDSplit.reg, IPSec.reg
CopyFiles       = winvista.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[E10E6PM.Services]
AddService = e1qexpress, 2, winvista.Service, winvista.EventLog

[E10E6PM.HW]
Include=machine.inf
Needs=PciIoSpaceNotRequired
AddReg=MSIX10.reg

;-------------------------------------------------------------------------------
; Intel(R) Gigabit ET Quad Port Server Adapter
;-------------------------------------------------------------------------------
[E10E8PM]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
AddReg          = e1q.reg, Copper.reg, Copper1000.reg
AddReg          = JumboPacket.reg
AddReg          = TcpSeg.reg, RSS.reg, RSS8Q.reg, HDSplit.reg, IPSec.reg
CopyFiles       = winvista.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[E10E8PM.Services]
AddService = e1qexpress, 2, winvista.Service, winvista.EventLog


[E10E8PM.HW]
Include=machine.inf
Needs=PciIoSpaceNotRequired
AddReg=MSIX10.reg

;-------------------------------------------------------------------------------
; Do-nothing section used to avoid "Unknown hardware" installation prompts.
;
[NO_DRV]
Characteristics = 0x01
Include=machine.inf
Needs=NO_DRV

[NO_DRV.Services]
Include=machine.inf
Needs=NO_DRV.Services

;-------------------------------------------------------------------------------
; Registry Settings (decimal)
;
[e1q.reg]

HKR, Ndi\Interfaces,                                    UpperRange,             0, "ndis5"
HKR, Ndi\Interfaces,                                    LowerRange,             0, "ethernet"
HKR, Ndi,                                               Service,                0, "e1qexpress"

HKR, Ndi\Params\*FlowControl,                           ParamDesc,              0, %FlowControl%
HKR, Ndi\Params\*FlowControl,                           default,                0, "3"
HKR, Ndi\Params\*FlowControl\Enum,                      "0",                    0, %Disabled%
HKR, Ndi\Params\*FlowControl\Enum,                      "1",                    0, %FlowControl_TxOnly%
HKR, Ndi\Params\*FlowControl\Enum,                      "2",                    0, %FlowControl_RxOnly%
HKR, Ndi\Params\*FlowControl\Enum,                      "3",                    0, %FlowControl_Full%
HKR, Ndi\Params\*FlowControl,                           type,                   0, "enum"

; *TransmitBuffers
HKR, Ndi\params\*TransmitBuffers,                       ParamDesc,              0, %TransmitBuffers%
HKR, Ndi\params\*TransmitBuffers,                       default,                0, "512"
HKR, Ndi\params\*TransmitBuffers,                       min,                    0, "80"
HKR, Ndi\params\*TransmitBuffers,                       max,                    0, "2048"
HKR, Ndi\params\*TransmitBuffers,                       step,                   0, "8"
HKR, Ndi\params\*TransmitBuffers,                       Base,                   0, "10"
HKR, Ndi\params\*TransmitBuffers,                       type,                   0, "int"

; *ReceiveBuffers
HKR, Ndi\params\*ReceiveBuffers,                        ParamDesc,              0, %ReceiveBuffers%
HKR, Ndi\params\*ReceiveBuffers,                        default,                0, "256"
HKR, Ndi\params\*ReceiveBuffers,                        min,                    0, "80"
HKR, Ndi\params\*ReceiveBuffers,                        max,                    0, "2048"
HKR, Ndi\params\*ReceiveBuffers,                        step,                   0, "8"
HKR, Ndi\params\*ReceiveBuffers,                        Base,                   0, "10"
HKR, Ndi\params\*ReceiveBuffers,                        type,                   0, "int"

; *TCPChecksumOffloadIPv4
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,                ParamDesc,              0, %TCPChksumOffv4%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,                default,                0, "3"
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\Enum,           "0",                    0, %Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\Enum,           "1",                    0, %ChksumOffTx%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\Enum,           "2",                    0, %ChksumOffRx%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\Enum,           "3",                    0, %ChksumOffTxRx%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,                type,                   0, "enum"

; *TCPChecksumOffloadIPv6
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,                ParamDesc,              0, %TCPChksumOffv6%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,                default,                0, "3"
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\Enum,           "0",                    0, %Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\Enum,           "1",                    0, %ChksumOffTx%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\Enum,           "2",                    0, %ChksumOffRx%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\Enum,           "3",                    0, %ChksumOffTxRx%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,                type,                   0, "enum"

; *UDPChecksumOffloadIPv4
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,                ParamDesc,              0, %UDPChksumOffv4%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,                default,                0, "3"
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\Enum,           "0",                    0, %Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\Enum,           "1",                    0, %ChksumOffTx%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\Enum,           "2",                    0, %ChksumOffRx%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\Enum,           "3",                    0, %ChksumOffTxRx%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,                type,                   0, "enum"

; *UDPChecksumOffloadIPv6
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,                ParamDesc,              0, %UDPChksumOffv6%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,                default,                0, "3"
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\Enum,           "0",                    0, %Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\Enum,           "1",                    0, %ChksumOffTx%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\Enum,           "2",                    0, %ChksumOffRx%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\Enum,           "3",                    0, %ChksumOffTxRx%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,                type,                   0, "enum"

; *IPChecksumOffloadIPv4
HKR, Ndi\Params\*IPChecksumOffloadIPv4,                 ParamDesc,              0, %IPChksumOffv4%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,                 default,                0, "3"
HKR, Ndi\Params\*IPChecksumOffloadIPv4\Enum,            "0",                    0, %Disabled%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\Enum,            "1",                    0, %ChksumOffTx%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\Enum,            "2",                    0, %ChksumOffRx%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\Enum,            "3",                    0, %ChksumOffTxRx%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,                 type,                   0, "enum"

; Network Address
HKR, Ndi\params\NetworkAddress,                         ParamDesc,              0, %LAA%
HKR, Ndi\params\NetworkAddress,                         Default,                0, ""
HKR, Ndi\params\NetworkAddress,                         type,                   0, "edit"
HKR, NDI\params\NetworkAddress,                         LimitText,              0, "12"
HKR, NDI\params\NetworkAddress,                         UpperCase,              0, "1"
HKR, NDI\params\NetworkAddress,                         optional,               0, "1"

;Log Link State Event
HKR,Ndi\Params\LogLinkStateEvent,                       ParamDesc,              0, %LogLinkState%
HKR,Ndi\Params\LogLinkStateEvent,                       Type,                   0, "enum"
HKR,Ndi\Params\LogLinkStateEvent,                       Default,                0, "51"
HKR,Ndi\Params\LogLinkStateEvent\Enum,                  "51",                   0, %Enabled%
HKR,Ndi\Params\LogLinkStateEvent\Enum,                  "16",                   0, %Disabled%
; Wait for Link
HKR, Ndi\Params\WaitAutoNegComplete,                    ParamDesc,              0, %WaitAutoNegComplete%
HKR, Ndi\Params\WaitAutoNegComplete,                    default,                0, "2"
HKR, Ndi\Params\WaitAutoNegComplete\Enum,               "0",                    0, %Off%
HKR, Ndi\Params\WaitAutoNegComplete\Enum,               "1",                    0, %On%
HKR, Ndi\Params\WaitAutoNegComplete\Enum,               "2",                    0, %AutoDetect%
HKR, Ndi\Params\WaitAutoNegComplete,                    type,                   0, "enum"


;  Interrupt Throttle Rate
HKR, Ndi\Params\ITR,                                    ParamDesc,              0, %InterruptThrottleRate%
HKR, Ndi\Params\ITR,                                    default,                0, "65535"
HKR, Ndi\Params\ITR\Enum,                               "65535",                0, %Adaptive%
HKR, Ndi\Params\ITR\Enum,                               "3600",                 0, %Extreme%
HKR, Ndi\Params\ITR\Enum,                               "2000",                 0, %High%
HKR, Ndi\Params\ITR\Enum,                               "950",                  0, %Medium%
HKR, Ndi\Params\ITR\Enum,                               "400",                  0, %Low%
HKR, Ndi\Params\ITR\Enum,                               "200",                  0, %Minimal%
HKR, Ndi\Params\ITR\Enum,                               "0",                    0, %Off%
HKR, Ndi\Params\ITR,                                    type,                   0, "enum"
; *InterruptModeration
HKR, Ndi\Params\*InterruptModeration,                   ParamDesc,              0, %InterruptModeration%
HKR, Ndi\Params\*InterruptModeration,                   default,                0, "1"
HKR, Ndi\Params\*InterruptModeration\Enum,              "0",                    0, %Disabled%
HKR, Ndi\Params\*InterruptModeration\Enum,              "1",                    0, %Enabled%
HKR, Ndi\Params\*InterruptModeration,                   type,                   0, "enum"

; *PriorityVLANTag
HKR, Ndi\Params\*PriorityVLANTag,                       ParamDesc,              0, %PriorityVLANTag%
HKR, Ndi\Params\*PriorityVLANTag,                       default,                0, "3"
HKR, Ndi\Params\*PriorityVLANTag\Enum,                  "0",                    0, %PriorityVlanDisabled%
HKR, Ndi\Params\*PriorityVLANTag\Enum,                  "1",                    0, %PriorityEnabled%
HKR, Ndi\Params\*PriorityVLANTag\Enum,                  "2",                    0, %VlanEnabled%
HKR, Ndi\Params\*PriorityVLANTag\Enum,                  "3",                    0, %PriorityVlanEnabled%
HKR, Ndi\Params\*PriorityVLANTag,                       type,                   0, "enum"

; Advanced Power Consumption Features
HKR,,                                          ReduceSpeedOnPowerDown,   0, "1"
HKR,,                                          AutoPowerSaveModeEnabled, 0, "0"
HKR,,                                          SavePowerNowEnabled,      0, "1"


[TcpSeg.reg]
; *LsoV2IPv4 / *LsoV2IPv6
HKR, Ndi\Params\*LsoV2IPv4,                             ParamDesc,              0, %LsoV2IPv4%
HKR, Ndi\Params\*LsoV2IPv4,                             default,                0, "1"
HKR, Ndi\Params\*LsoV2IPv4\Enum,                        "0",                    0, %Disabled%
HKR, Ndi\Params\*LsoV2IPv4\Enum,                        "1",                    0, %Enabled%
HKR, Ndi\Params\*LsoV2IPv4,                             type,                   0, "enum"

HKR, Ndi\Params\*LsoV2IPv6,                             ParamDesc,              0, %LsoV2IPv6%
HKR, Ndi\Params\*LsoV2IPv6,                             default,                0, "1"
HKR, Ndi\Params\*LsoV2IPv6\Enum,                        "0",                    0, %Disabled%
HKR, Ndi\Params\*LsoV2IPv6\Enum,                        "1",                    0, %Enabled%
HKR, Ndi\Params\*LsoV2IPv6,                             type,                   0, "enum"

[HDSplit.reg]
; Header Split capabilities
HKR, Ndi\Params\*HeaderDataSplit,                       ParamDesc,              0, %HeaderDataSplit%
HKR, Ndi\Params\*HeaderDataSplit,                       default,                0, "1"
HKR, Ndi\Params\*HeaderDataSplit\Enum,                  "0",                    0, %Disabled%
HKR, Ndi\Params\*HeaderDataSplit\Enum,                  "1",                    0, %Enabled%
HKR, Ndi\Params\*HeaderDataSplit,                       type,                   0, "enum"

[Copper.reg]
HKR, Ndi\params\*SpeedDuplex,                           ParamDesc,              0, %SpeedDuplex%
HKR, Ndi\params\*SpeedDuplex,                           default,                0, "0"
HKR, Ndi\params\*SpeedDuplex,                           type,                   0, "enum"
HKR, Ndi\params\*SpeedDuplex\enum,                      "0",                    0, %AutoNegotiation%
HKR, Ndi\params\*SpeedDuplex\enum,                      "1",                    0, %10Mb_Half_Duplex%
HKR, Ndi\params\*SpeedDuplex\enum,                      "2",                    0, %10Mb_Full_Duplex%
HKR, Ndi\params\*SpeedDuplex\enum,                      "3",                    0, %100Mb_Half_Duplex%
HKR, Ndi\params\*SpeedDuplex\enum,                      "4",                    0, %100Mb_Full_Duplex%
HKR, PROSetNdi\NdiExt\Params\*SpeedDuplex,              ExposeLevel,            0, "3"
; Adaptive IFS
HKR, Ndi\Params\AdaptiveIFS,                            ParamDesc,              0, %AdaptiveIFS%
HKR, Ndi\Params\AdaptiveIFS,                            default,                0, "0"
HKR, Ndi\Params\AdaptiveIFS,                            type,                   0, "enum"
HKR, Ndi\Params\AdaptiveIFS\Enum,                       "0",                    0, %Disabled%
HKR, Ndi\Params\AdaptiveIFS\Enum,                       "1",                    0, %Enabled%

[Copper1000.reg]
HKR, Ndi\params\*SpeedDuplex\enum,                      "6",                    0, %1000Mb_Full_Duplex%
; Gigabit Master Slave Mode
HKR,Ndi\Params\MasterSlave,                             ParamDesc,              0, %MasterSlaveMode%
HKR,Ndi\Params\MasterSlave,                             Type,                   0, "enum"
HKR,Ndi\Params\MasterSlave,                             Default,                0, "0"
HKR,Ndi\Params\MasterSlave\Enum,                        "0",                    0, %AutoDetect%
HKR,Ndi\Params\MasterSlave\Enum,                        "1",                    0, %GigabitMasterMode%
HKR,Ndi\Params\MasterSlave\Enum,                        "2",                    0, %GigabitSlaveMode%

;-------------------------------------------------------------------------------
; Packet specifics
;

; *JumboPacket
[JumboPacket.reg]
HKR, Ndi\Params\*JumboPacket,                           ParamDesc,              0, %JumboPacket%
HKR, Ndi\Params\*JumboPacket,                           default,                0, "1514"
HKR, Ndi\Params\*JumboPacket\Enum,                      "1514",                 0, %Disabled%
HKR, Ndi\Params\*JumboPacket\Enum,                      "4088",                 0, %Bytes4088%
HKR, Ndi\Params\*JumboPacket\Enum,                      "9014",                 0, %Bytes9014%
HKR, Ndi\Params\*JumboPacket,                           type,                   0, "enum"


[RSS.reg]
; *RSS
HKR, Ndi\Params\*RSS,                                   ParamDesc,              0, %RSS%
HKR, Ndi\Params\*RSS,                                   default,                0, "1"
HKR, Ndi\Params\*RSS,                                   type,                   0, "enum"
HKR, Ndi\Params\*RSS\Enum,                              "0",                    0, %Disabled%
HKR, Ndi\Params\*RSS\Enum,                              "1",                    0, %Enabled%


[RSS2Q.reg]
; NumRssQueues
HKR, Ndi\Params\NumRssQueues,                           ParamDesc,              0, %NumRssQueues%
HKR, Ndi\Params\NumRssQueues,                           default,                0, "1"
HKR, Ndi\Params\NumRssQueues,                           type,                   0, "enum"
HKR, Ndi\Params\NumRssQueues\Enum,                      "1",                    0, %1queue%
HKR, Ndi\Params\NumRssQueues\Enum,                      "2",                    0, %2queues%

[RSS4Q.reg]
; NumRssQueues
HKR, Ndi\Params\NumRssQueues,                           ParamDesc,              0, %NumRssQueues%
HKR, Ndi\Params\NumRssQueues,                           default,                0, "1"
HKR, Ndi\Params\NumRssQueues,                           type,                   0, "enum"
HKR, Ndi\Params\NumRssQueues\Enum,                      "1",                    0, %1queue%
HKR, Ndi\Params\NumRssQueues\Enum,                      "2",                    0, %2queues%
HKR, Ndi\Params\NumRssQueues\Enum,                      "4",                    0, %4queues%

[RSS8Q.reg]
; NumRssQueues
HKR, Ndi\Params\NumRssQueues,                           ParamDesc,              0, %NumRssQueues%
HKR, Ndi\Params\NumRssQueues,                           default,                0, "1"
HKR, Ndi\Params\NumRssQueues,                           type,                   0, "enum"
HKR, Ndi\Params\NumRssQueues\Enum,                      "1",                    0, %1queue%
HKR, Ndi\Params\NumRssQueues\Enum,                      "2",                    0, %2queues%
HKR, Ndi\Params\NumRssQueues\Enum,                      "4",                    0, %4queues%
HKR, Ndi\Params\NumRssQueues\Enum,                      "8",                    0, %8queues%

[IPSec.reg]
; IPSec capabilities
HKR, Ndi\Params\*IPsecOffloadV2,                        ParamDesc,              0, %IPsecOffloadV2%
HKR, Ndi\Params\*IPsecOffloadV2,                        default,                0, "0"
HKR, Ndi\Params\*IPsecOffloadV2\Enum,                   "0",                    0, %Disabled%
HKR, Ndi\Params\*IPsecOffloadV2\Enum,                   "1",                    0, %IPsecAH%
HKR, Ndi\Params\*IPsecOffloadV2\Enum,                   "2",                    0, %IPsecESP%
HKR, Ndi\Params\*IPsecOffloadV2\Enum,                   "3",                    0, %IPsecAHESP%
HKR, Ndi\Params\*IPsecOffloadV2,                        type,                   0, "enum"

[MSIX.reg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 6

[MSIX3.reg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 3

[MSIX10.reg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 10


;-------------------------------------------------------------------------------
; WinVista copy files
;
[winvista.CopyFiles]
e1q6032.sys,,,2

[winvista.Service]
DisplayName     = %E1QExpress.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\e1q6032.sys
LoadOrderGroup  = NDIS

;-------------------------------------------------------------------------------
; Common base for all drivers for Eventlog and TextModeFlags
;

[winvista.EventLog]
AddReg = winvista.AddEventLog.reg

[winvista.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, %EventLogMessageDllPath_6032%
HKR, , TypesSupported,   0x00010001, 7

;-------------------------------------------------------------------------------
; DestinationDirs
;
[DestinationDirs]
DefaultDestDir                = 11
winvista.CopyFiles            = 12

[SourceDisksNames]
;
; diskid = description[, [tagfile] [, <unused>,subdir]]
;
1 = %DISKNAME%,,,

[SourceDisksFiles]
e1q6032.sys  = 1,, ; on distribution disk 1

;-----------------------------------------------------------------------------
; Localizable Strings

[Strings]
;-------------------------------------------------------------------------------
EventLogMessageDllPath_6032     = "%SystemRoot%\System32\netevent.dll;%SystemRoot%\System32\drivers\e1q6032.sys"

;-------------------------------------------------------------------------------
AnsLoaded                       = "ANS Loaded"
AutoDetect                      = "Auto Detect"
AutoNegotiation                 = "Auto Negotiation"

SpeedDuplex                     = "Link Speed & Duplex"
10Mb_Half_Duplex                = "10 Mbps Half Duplex"
10Mb_Full_Duplex                = "10 Mbps Full Duplex"
100Mb_Half_Duplex               = "100 Mbps Half Duplex"
100Mb_Full_Duplex               = "100 Mbps Full Duplex"
1000Mb_Full_Duplex              = "1.0 Gbps Full Duplex"

IPChksumOffv4                   = "IPv4 Checksum Offload"
TCPChksumOffv4                  = "TCP Checksum Offload (IPv4)"
UDPChksumOffv4                  = "UDP Checksum Offload (IPv4)"
TCPChksumOffv6                  = "TCP Checksum Offload (IPv6)"
UDPChksumOffv6                  = "UDP Checksum Offload (IPv6)"

LsoV2IPv4                       = "Large Send Offload (IPv4)"
LsoV2IPv6                       = "Large Send Offload (IPv6)"
HeaderDataSplit                 = "Header Data Split"
IPsecOffloadV2                  = "IPsec Offload"
IPsecAH                         = "Auth Header Enabled"
IPsecESP                        = "ESP Enabled"
IPSecAHESP                      = "Auth Header & ESP Enabled"
ChksumOffTxRx                   = "Rx & Tx Enabled"
ChksumOffTx                     = "Tx Enabled"
ChksumOffRx                     = "Rx Enabled"
FlowControl                     = "Flow Control"
FlowControl_TxOnly              = "Tx Enabled"
FlowControl_RxOnly              = "Rx Enabled"
FlowControl_Full                = "Rx & Tx Enabled"
PriorityVlanDisabled            = "Priority & VLAN Disabled"
PriorityEnabled                 = "Priority Enabled"
VlanEnabled                     = "VLAN Enabled"
PriorityVlanEnabled             = "Priority & VLAN Enabled"
TransmitBuffers                 = "Transmit Buffers"
ReceiveBuffers                  = "Receive Buffers"
NumCoalesceBuffers              = "Coalesce Buffers"
PriorityVLANTag                 = "Priority & VLAN"
RSS                             = "Receive Side Scaling"
NumRssQueues                    = "Receive Side Scaling Queues"
1queue                          = "1 Queue"
2queues                         = "2 Queues"
4queues                         = "4 Queues"
8queues                         = "8 Queues"

On                              = "On"
Off                             = "Off"
Enabled                         = "Enabled"
Disabled                        = "Disabled"
Bytes4088                       = "4088 Bytes"
Bytes9014                       = "9014 Bytes"

LAA                             = "Locally Administered Address"
JumboPacket                     = "Jumbo Packet"
AdaptiveIFS                     = "Adaptive Inter-Frame Spacing"

LogLinkState                    = "Log Link State Event"
InterruptModeration             = "Interrupt Moderation"
InterruptThrottleRate           = "Interrupt Moderation Rate"
Adaptive                        = "Adaptive"
Extreme                         = "Extreme"
Minimal                         = "Minimal"
High                            = "High"
Medium                          = "Medium"
Low                             = "Low"
GigabitMasterMode               = "Force Master Mode"
GigabitSlaveMode                = "Force Slave Mode"
MasterSlaveMode                 = "Gigabit Master Slave Mode"
WaitAutoNegComplete             = "Wait for Link"
Intel                           = "Intel"
MSFT                            = "Microsoft"

E1QExpress.Service.DispName     = "Intel(R) PRO/1000 PCI Express Network Connection Driver Q"
DISKNAME                        = "Intel(R) PRO/1000 Driver Disk"

;; Brandnames.str
;------------------------------------------------------------------------------
E10A7NC.DeviceDesc              = "Intel(R) 82575EB Gigabit Network Connection"
E10A9NC.DeviceDesc              = "Intel(R) 82575EB Gigabit Backplane Connection"
E10D6NC.DeviceDesc              = "Intel(R) Gigabit VT Quad Port Server Adapter"
E10A7DD.DeviceDesc              = "Intel(R) 82575EB Multi-Function Network Device"
E10D3NC.DeviceDesc              = "Intel(R) 82574L Gigabit Network Connection"
EA01FNC.DeviceDesc              = "Intel(R) Gigabit CT Desktop Adapter"
E10C9LNC.DeviceDesc             = "Intel(R) 82576 Gigabit Dual Port Network Connection"
E10C9NC.DeviceDesc              = "Intel(R) Gigabit ET Dual Port Server Adapter"
E150A.DeviceDesc                = "Intel(R) 82576NS Gigabit Ethernet Controller"
E10E6NC.DeviceDesc              = "Intel(R) Gigabit EF Dual Port Server Adapter"
E10E7NC.DeviceDesc              = "Intel(R) 82576 Gigabit Dual Port Server Network Connection"
E10E8NC.DeviceDesc              = "Intel(R) Gigabit ET Quad Port Server Adapter"
E10E6LNC.DeviceDesc             = "Intel(R) 82576 Gigabit Dual Port Network Connection"

;---------------------------------------------------------------------------------------------------
;---------------------------------------------------------------------------------------------------
;---------------------------------------------------------------------------------------------------
;---------------------------------------------------------------------------------------------------
;---------------------------------------------------------------------------------------------------
