;
; Copyright (c) 2008, Microsoft Corporation.
;

[version]
	Signature	= "$Windows NT$"
	Class           = Net
	ClassGUID	= {4d36e972-e325-11ce-bfc1-08002be10318}
	Provider	= %MSFT%
	Compatible	= 1
DriverVer=10/01/2008,4.176.75.21

[Manufacturer]
	%V_BCM% = BROADCOM, NTx86.6.1

[ControlFlags] 
	ExcludeFromSelect = *

[BROADCOM.NTx86.6.1]
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4320&REV_03
	%BCM430G_LNK_SPB_DeviceDesc%    = BCM43XG_NT61, PCI\VEN_14E4&DEV_4320&SUBSYS_43201737&REV_03
	%BCM430G_DELL_DeviceDesc% =  BCM43XGBO_NT61,  PCI\VEN_14E4&DEV_4320&SUBSYS_00011028&REV_03
	%BCM430GC_DeviceDesc% = BCM43XGBO_NT61, PCI\VEN_14E4&DEV_4320&SUBSYS_00021028&REV_03
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4320&SUBSYS_00E70E11&REV_03
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4320&SUBSYS_12F4103C&REV_03
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4320&SUBSYS_12F8103C&REV_03
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4320&SUBSYS_12FA103C&REV_03
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4320&SUBSYS_12FB103C&REV_03
	%BCM1350M_DeviceDesc% = BCM43XGBO_NT61, PCI\VEN_14E4&DEV_4320&SUBSYS_00031028&REV_03
	%BCM1350C_DeviceDesc% = BCM43XGBO_NT61, PCI\VEN_14E4&DEV_4320&SUBSYS_00041028&REV_03
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4320&SUBSYS_000218DE&REV_03
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4320&SUBSYS_00151737&REV_03
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4320&SUBSYS_046614E4&REV_03

	%BCM430A_DeviceDesc% = BCM43XA_NT61, PCI\VEN_14E4&DEV_4321&REV_03
	%BCM430A_DeviceDesc% = BCM43XA_NT61, PCI\VEN_14E4&DEV_4321&SUBSYS_046614E4&REV_03

	%BCM430M_DeviceDesc% = BCM43XM_NT61, PCI\VEN_14E4&DEV_4324&REV_03
	%BCM430M_DeviceDesc% = BCM43XMJ8_NT61, PCI\VEN_14E4&DEV_4324&SUBSYS_03281154&REV_03
	%BCM430M_DeviceDesc% = BCM43XMJ6_NT61, PCI\VEN_14E4&DEV_4324&SUBSYS_033C1154&REV_03
	%BCM430M_DeviceDesc% = BCM43XMJ5_NT61, PCI\VEN_14E4&DEV_4324&SUBSYS_033F1154&REV_03
	%BCM430M_DELL_DeviceDesc% =  BCM43XMBO_NT61,  PCI\VEN_14E4&DEV_4324&SUBSYS_00011028&REV_03
	%BCM430MC_DeviceDesc% = BCM43XMBO_NT61, PCI\VEN_14E4&DEV_4324&SUBSYS_00021028&REV_03
	%BCM1450M_DeviceDesc% = BCM43XMBO_NT61, PCI\VEN_14E4&DEV_4324&SUBSYS_00031028&REV_03
	%BCM1450C_DeviceDesc% = BCM43XMBO_NT61, PCI\VEN_14E4&DEV_4324&SUBSYS_00041028&REV_03
	%BCM430M_DeviceDesc% = BCM43XM_NT61, PCI\VEN_14E4&DEV_4324&SUBSYS_12F9103C&REV_03
	%BCM430M_DeviceDesc% = BCM43XM_NT61, PCI\VEN_14E4&DEV_4324&SUBSYS_12FC103C&REV_03
	%BCM430M_DeviceDesc% = BCM43XM_NT61, PCI\VEN_14E4&DEV_4324&SUBSYS_046614E4&REV_03

	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4325&REV_03
	%BCM430G_MSFT_PC_DeviceDesc%    = BCM43XG_NT61, PCI\VEN_14E4&DEV_4325&SUBSYS_00031414&REV_03
	%BCM430G_MSFT_PCI_DeviceDesc%   = BCM43XG_NT61, PCI\VEN_14E4&DEV_4325&SUBSYS_00041414&REV_03
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4325&SUBSYS_000318DE&REV_03
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4325&SUBSYS_000618DE&REV_03

	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4318
	%BCM430G_USR_PC_DeviceDesc%     = BCM43XG_NT61, PCI\VEN_14E4&DEV_4318&SUBSYS_011916EC&REV_02
	%BCM430G_USR_PCI_DeviceDesc%    = BCM43XG_NT61, PCI\VEN_14E4&DEV_4318&SUBSYS_011A16EC&REV_02
	%BCM430G_LNK_SPB_DeviceDesc%    = BCM43XG_NT61, PCI\VEN_14E4&DEV_4318&SUBSYS_00491737
	%BCM430G_LNK_DeviceDesc%        = BCM43XG_NT61, PCI\VEN_14E4&DEV_4318&SUBSYS_00481737
	%BCM1370M_DeviceDesc% = BCM43XGBO_NT61, PCI\VEN_14E4&DEV_4318&SUBSYS_00051028
	%BCM1370C_DeviceDesc% = BCM43XGBO_NT61, PCI\VEN_14E4&DEV_4318&SUBSYS_00061028
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4318&SUBSYS_1355103C
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4318&SUBSYS_1356103C
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4318&SUBSYS_1357103C
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4318&SUBSYS_00421737
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4318&SUBSYS_03111468
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4318&SUBSYS_03121468
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4318&SUBSYS_046614E4
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4318&SUBSYS_11011A32

	%BCM430M_DeviceDesc% = BCM43XM_NT61, PCI\VEN_14E4&DEV_4319
	%BCM1470M_DeviceDesc% = BCM43XMBO_NT61, PCI\VEN_14E4&DEV_4319&SUBSYS_00051028
	%BCM1470C_DeviceDesc% = BCM43XMBO_NT61, PCI\VEN_14E4&DEV_4319&SUBSYS_00061028
	%BCM430M_DeviceDesc% = BCM43XM_NT61, PCI\VEN_14E4&DEV_4319&SUBSYS_1358103C
	%BCM430M_DeviceDesc% = BCM43XM_NT61, PCI\VEN_14E4&DEV_4319&SUBSYS_1359103C
	%BCM430M_DeviceDesc% = BCM43XM_NT61, PCI\VEN_14E4&DEV_4319&SUBSYS_135A103C
	%BCM430M_DeviceDesc% = BCM43XM_NT61, PCI\VEN_14E4&DEV_4319&SUBSYS_046614E4

	%BCM430A_DeviceDesc% = BCM43XA_NT61, PCI\VEN_14E4&DEV_431A
	%BCM430A_DeviceDesc% = BCM43XA_NT61, PCI\VEN_14E4&DEV_431A&SUBSYS_046614E4

	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4311
	%BCM1390M_DeviceDesc% = BCM43XGBO_NT61, PCI\VEN_14E4&DEV_4311&SUBSYS_00071028
	%BCM1390E_DeviceDesc% = BCM43XGBO_NT61, PCI\VEN_14E4&DEV_4311&SUBSYS_00081028
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4311&SUBSYS_1363103C
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4311&SUBSYS_1364103C
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4311&SUBSYS_1365103C
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4311&SUBSYS_1374103C
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4311&SUBSYS_1375103C
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4311&SUBSYS_1376103C
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4311&SUBSYS_1377103C
	%BCM430G_DeviceDesc% = BCM43XG_NT61,PCI\VEN_14E4&DEV_4311&SUBSYS_04221468
	%BCM430G_DeviceDesc% = BCM43XG_NT61,PCI\VEN_14E4&DEV_4311&SUBSYS_046614E4
	%BCM430G_DeviceDesc% = BCM43XG_NT61,PCI\VEN_14E4&DEV_4311&SUBSYS_11021A32


	%BCM430M_DeviceDesc% = BCM43XM_NT61, PCI\VEN_14E4&DEV_4312
	%BCM1490M_DeviceDesc% = BCM43XMBO_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_00071028
	%BCM1490E_DeviceDesc% = BCM43XMBO_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_00081028
	%BCM430M_DeviceDesc% = BCM43XM_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_1360103C
	%BCM430M_DeviceDesc% = BCM43XM_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_1361103C
	%BCM430M_DeviceDesc% = BCM43XM_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_1362103C
	%BCM430M_DeviceDesc% = BCM43XM_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_135F103C
	%BCM430M_DeviceDesc% = BCM43XM_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_1370103C
	%BCM430M_DeviceDesc% = BCM43XM_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_1371103C
	%BCM430M_DeviceDesc% = BCM43XM_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_1372103C
	%BCM430M_DeviceDesc% = BCM43XM_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_1373103C

	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4313
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4313&SUBSYS_046614E4

	%BCM430N_DeviceDesc% = BCM43XNM_NT61, PCI\VEN_14E4&DEV_4328
	%BCM1500M_DeviceDesc% = BCM43XNMBO_NT61, PCI\VEN_14E4&DEV_4328&SUBSYS_00091028
	%BCM1505M_DeviceDesc% = BCM43XNMBO_NT61, PCI\VEN_14E4&DEV_4328&SUBSYS_000A1028
        %BCM430NM_DeviceDesc% = BCM43XNM_NT61, PCI\VEN_14E4&DEV_4328&SUBSYS_1366103C
        %BCM430NM_DeviceDesc% = BCM43XNM_NT61, PCI\VEN_14E4&DEV_4328&SUBSYS_1367103C
        %BCM430NM_DeviceDesc% = BCM43XNM_NT61, PCI\VEN_14E4&DEV_4328&SUBSYS_1368103C
        %BCM430NM_DeviceDesc% = BCM43XNM_NT61, PCI\VEN_14E4&DEV_4328&SUBSYS_1369103C
        %BCM430NM_DeviceDesc% = BCM43XNM_NT61, PCI\VEN_14E4&DEV_4328&SUBSYS_03191468
        %BCM430NM_DeviceDesc% = BCM43XNM_NT61, PCI\VEN_14E4&DEV_4328&SUBSYS_00661737
        %BCM430NM_DeviceDesc% = BCM43XNM_NT61, PCI\VEN_14E4&DEV_4328&SUBSYS_046614E4
        %BCM430NM_DeviceDesc% = BCM43XNM_NT61, PCI\VEN_14E4&DEV_4328&SUBSYS_05001A32

	%BCM430N_DeviceDesc% = BCM43XNG_NT61, PCI\VEN_14E4&DEV_4329
	%BCM430N_USR_PC_DeviceDesc%     = BCM43XNG_NT61, PCI\VEN_14E4&DEV_4329&SUBSYS_012516EC&REV_01
	%BCM430N_USR_PCI_DeviceDesc%    = BCM43XNG_NT61, PCI\VEN_14E4&DEV_4329&SUBSYS_012416EC&REV_01
	%BCM430N_LNK_DeviceDesc%        = BCM43XNG_NT61, PCI\VEN_14E4&DEV_4329&SUBSYS_00581737
	%BCM430N_NTGR_PC_DeviceDesc%    = BCM43XNG_NT61, PCI\VEN_14E4&DEV_4329&SUBSYS_1385&subdev_7B00WN511B
	%BCM430N_NTGR_PCI_DeviceDesc%   = BCM43XNG_NT61, PCI\VEN_14E4&DEV_4329&SUBSYS_1385&subdev_7D00WN311B
	%BCM430N_DeviceDesc% = BCM43XNG_NT61, PCI\VEN_14E4&DEV_4329&SUBSYS_00601737
	%BCM430N_DeviceDesc% = BCM43XNG_NT61, PCI\VEN_14E4&DEV_4329&SUBSYS_046614E4
	%BCM430N_DeviceDesc% = BCM43XNG_NT61, PCI\VEN_14E4&DEV_4329&SUBSYS_7B001385
	%BCM430N_DeviceDesc% = BCM43XNG_NT61, PCI\VEN_14E4&DEV_4329&SUBSYS_7D001385
	%BCM430N_DeviceDesc% = BCM43XNG_NT61, PCI\VEN_14E4&DEV_4329&SUBSYS_F03014E4

	%BCM430N_DeviceDesc% = BCM43XA_NT61, PCI\VEN_14E4&DEV_432A
	%BCM430N_DeviceDesc% = BCM43XA_NT61, PCI\VEN_14E4&DEV_432A&SUBSYS_046614E4

	%BCM430N_DeviceDesc% = BCM43XNM_NT61, PCI\VEN_14E4&DEV_432B
	%BCM1510HM8L_DeviceDesc% = BCM43XNMBO_NT61, PCI\VEN_14E4&DEV_432b&SUBSYS_000D1028
	%BCM4322NM_DeviceDesc% = BCM43XNM_NT61, PCI\VEN_14E4&DEV_432B&SUBSYS_137F103C
	%BCM4322NM_DeviceDesc% = BCM43XNM_NT61, PCI\VEN_14E4&DEV_432B&SUBSYS_1380103C
	%BCM4322NM_DeviceDesc% = BCM43XNM_NT61, PCI\VEN_14E4&DEV_432B&SUBSYS_1509103C
	%BCM4322NM_DeviceDesc% = BCM43XNM_NT61, PCI\VEN_14E4&DEV_432B&SUBSYS_1510103C

	%BCM430N_DeviceDesc% = BCM43XNG_NT61, PCI\VEN_14E4&DEV_432C

	%BCM430M_DeviceDesc% = BCM43XM_NT61, PCI\VEN_14E4&DEV_4314
	%BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4315
	%BCM1395M_DeviceDesc% = BCM43XGBO_NT61, PCI\VEN_14E4&DEV_4315&SUBSYS_000B1028
	%BCM1397HMG_DeviceDesc% = BCM43XGBO_NT61, PCI\VEN_14E4&DEV_4315&SUBSYS_000C1028
        %BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4315&SUBSYS_137C103C
        %BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4315&SUBSYS_137D103C
        %BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4315&SUBSYS_1507103C
        %BCM430G_DeviceDesc% = BCM43XG_NT61, PCI\VEN_14E4&DEV_4315&SUBSYS_1508103C

	%BCM430A_DeviceDesc% = BCM43XA_NT61, PCI\VEN_14E4&DEV_4316

;-----------------------------------------------------------------
; Win7
;
[BCM43XZ_NT61.NTx86]
	Include=netvwifibus.inf
	Needs=VWiFiBus.CopyFiles
	*IfType		= 71    ; IF_TYPE_IEEE80211
	*MediaType	= 16    ; NdisMediumNative802_11
	*PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
	Characteristics	= 0x84	; NCF_PHYSICAL | NCF_HAS_UI
	BusType		= 5			; PCI bus
	AddReg		= BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, b.options.reg, bg.options.reg, bg.channels.reg
	DelReg          = common.delreg, common.vista.delreg, rate.delreg
	CopyFiles	= BCM43XX_NT60.files.NTx86

[BCM43PCMG_NT61.NTx86]
	Include=netvwifibus.inf
	Needs=VWiFiBus.CopyFiles
	*IfType		= 71    ; IF_TYPE_IEEE80211
	*MediaType	= 16    ; NdisMediumNative802_11
	*PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
	Characteristics	= 0x84	; NCF_PHYSICAL | NCF_HAS_UI
	BusType		= 8		; PCMCIA bus
	AddReg		= BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, g.options.reg, bg.options.reg, bg.channels.reg
	DelReg          = common.delreg, common.vista.delreg, rate.delreg
	CopyFiles	= BCM43XX_NT60.files.NTx86

[BCM43XG_NT61.NTx86]
	Include=netvwifibus.inf
	Needs=VWiFiBus.CopyFiles
	*IfType		= 71    ; IF_TYPE_IEEE80211
	*MediaType	= 16    ; NdisMediumNative802_11
	*PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
	Characteristics	= 0x84	; NCF_PHYSICAL | NCF_HAS_UI
	BusType		= 5			; PCI bus
	AddReg		= BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, g.options.reg, bg.options.reg, bg.channels.reg
	DelReg          = common.delreg, common.vista.delreg, rate.delreg
	CopyFiles	= BCM43XX_NT60.files.NTx86

[BCM43XGBO_NT61.NTx86]
	Include=netvwifibus.inf
	Needs=VWiFiBus.CopyFiles
	*IfType		= 71    ; IF_TYPE_IEEE80211
	*MediaType	= 16    ; NdisMediumNative802_11
	*PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
	Characteristics	= 0x84	; NCF_PHYSICAL | NCF_HAS_UI
	BusType		= 5			; PCI bus
	AddReg		= BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, g.options.reg, bg.options.reg, bg.channels.reg, country.BO.reg
	DelReg          = common.delreg, common.vista.delreg, rate.delreg
	CopyFiles	= BCM43XX_NT60.files.NTx86

[BCM43XA_NT61.NTx86]
	Include=netvwifibus.inf
	Needs=VWiFiBus.CopyFiles
	*IfType		= 71    ; IF_TYPE_IEEE80211
	*MediaType	= 16    ; NdisMediumNative802_11
	*PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
	Characteristics	= 0x84	; NCF_PHYSICAL | NCF_HAS_UI
	BusType		= 5			; PCI bus
	AddReg		= BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, a.options.reg, a.channels.reg
	DelReg          = common.delreg, common.vista.delreg, rate.delreg
	CopyFiles	= BCM43XX_NT60.files.NTx86

[BCM43XM_NT61.NTx86]
	Include=netvwifibus.inf
	Needs=VWiFiBus.CopyFiles
	*IfType		= 71    ; IF_TYPE_IEEE80211
	*MediaType	= 16    ; NdisMediumNative802_11
	*PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
	Characteristics	= 0x84	; NCF_PHYSICAL | NCF_HAS_UI
	BusType		= 5			; PCI bus
	AddReg		= BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.options.reg, a.channels.reg, bg.channels.reg
	DelReg          = common.delreg, common.vista.delreg
	CopyFiles	= BCM43XX_NT60.files.NTx86

[BCM43XMJ8_NT61.NTx86]
	Include=netvwifibus.inf
	Needs=VWiFiBus.CopyFiles
	*IfType		= 71    ; IF_TYPE_IEEE80211
	*MediaType	= 16    ; NdisMediumNative802_11
	*PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
	Characteristics	= 0x84	; NCF_PHYSICAL | NCF_HAS_UI
	BusType		= 5			; PCI bus
	AddReg		= BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.options.reg, a.channels.reg, bg.channels.reg, country.J8.reg
	DelReg          = common.delreg, common.vista.delreg
	CopyFiles	= BCM43XX_NT60.files.NTx86

[BCM43XMJ6_NT61.NTx86]
	Include=netvwifibus.inf
	Needs=VWiFiBus.CopyFiles
	*IfType		= 71    ; IF_TYPE_IEEE80211
	*MediaType	= 16    ; NdisMediumNative802_11
	*PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
	Characteristics	= 0x84	; NCF_PHYSICAL | NCF_HAS_UI
	BusType		= 5			; PCI bus
	AddReg		= BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.options.reg, a.channels.reg, bg.channels.reg, country.J6.reg
	DelReg          = common.delreg, common.vista.delreg
	CopyFiles	= BCM43XX_NT60.files.NTx86

[BCM43XMJ5_NT61.NTx86]
	Include=netvwifibus.inf
	Needs=VWiFiBus.CopyFiles
	*IfType		= 71    ; IF_TYPE_IEEE80211
	*MediaType	= 16    ; NdisMediumNative802_11
	*PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
	Characteristics	= 0x84	; NCF_PHYSICAL | NCF_HAS_UI
	BusType		= 5			; PCI bus
	AddReg		= BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.options.reg, a.channels.reg, bg.channels.reg, country.J5.reg
	DelReg          = common.delreg, common.vista.delreg
	CopyFiles	= BCM43XX_NT60.files.NTx86

[BCM43XMBO_NT61.NTx86]
	Include=netvwifibus.inf
	Needs=VWiFiBus.CopyFiles
	*IfType		= 71    ; IF_TYPE_IEEE80211
	*MediaType	= 16    ; NdisMediumNative802_11
	*PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
	Characteristics	= 0x84	; NCF_PHYSICAL | NCF_HAS_UI
	BusType		= 5			; PCI bus
	AddReg		= BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.options.reg, a.channels.reg, bg.channels.reg, country.BO.reg
	DelReg          = common.delreg, common.vista.delreg
	CopyFiles	= BCM43XX_NT60.files.NTx86

[BCM43XNG_NT61.NTx86]
	Include=netvwifibus.inf
	Needs=VWiFiBus.CopyFiles
	*IfType		= 71    ; IF_TYPE_IEEE80211
	*MediaType	= 16    ; NdisMediumNative802_11
	*PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
	Characteristics	= 0x84	; NCF_PHYSICAL | NCF_HAS_UI
	BusType		= 5			; PCI bus
	AddReg		= BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, gn.options.reg, bg.options.reg, nbg.channels.reg
	DelReg          = common.delreg, common.vista.delreg, rate.delreg
	CopyFiles	= BCM43XX_NT60.files.NTx86

[BCM43XNM_NT61.NTx86]
	Include=netvwifibus.inf
	Needs=VWiFiBus.CopyFiles
	*IfType		= 71    ; IF_TYPE_IEEE80211
	*MediaType	= 16    ; NdisMediumNative802_11
	*PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
	Characteristics	= 0x84	; NCF_PHYSICAL | NCF_HAS_UI
	BusType		= 5			; PCI bus
	AddReg		= BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.options.reg, na.channels.reg, nbg.channels.reg
	DelReg          = common.delreg, common.vista.delreg
	CopyFiles	= BCM43XX_NT60.files.NTx86

[BCM43XNMBO_NT61.NTx86]
	Include=netvwifibus.inf
	Needs=VWiFiBus.CopyFiles
	*IfType		= 71    ; IF_TYPE_IEEE80211
	*MediaType	= 16    ; NdisMediumNative802_11
	*PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
	Characteristics	= 0x84	; NCF_PHYSICAL | NCF_HAS_UI
	BusType		= 5			; PCI bus
	AddReg		= BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.options.reg, na.channels.reg, nbg.channels.reg, country.BO.reg
	DelReg          = common.delreg, common.vista.delreg
	CopyFiles	= BCM43XX_NT60.files.NTx86

[BCM43XNMD_NT61.NTx86]
	Include=netvwifibus.inf
	Needs=VWiFiBus.CopyFiles
	*IfType		= 71    ; IF_TYPE_IEEE80211
	*MediaType	= 16    ; NdisMediumNative802_11
	*PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
	Characteristics	= 0x84	; NCF_PHYSICAL | NCF_HAS_UI
	BusType		= 5			; PCI bus
	AddReg		= BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.options.reg, na.channels.reg, nbg.channels.reg
	DelReg          = common.delreg, common.vista.delreg
	CopyFiles	= BCM43XX_NT60.files.NTx86

[BCM43XZ_NT61.NTx86.Services]
	Include=netvwifibus.inf
	Needs=VWiFiBus.Services
	AddService = BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog

[BCM43PCMG_NT61.NTx86.Services]
	Include=netvwifibus.inf
	Needs=VWiFiBus.Services
	AddService = BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog

[BCM43XG_NT61.NTx86.Services]
	Include=netvwifibus.inf
	Needs=VWiFiBus.Services
	AddService = BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog

[BCM43XGBO_NT61.NTx86.Services]
	Include=netvwifibus.inf
	Needs=VWiFiBus.Services
	AddService = BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog

[BCM43XA_NT61.NTx86.Services]
	Include=netvwifibus.inf
	Needs=VWiFiBus.Services
	AddService = BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog

[BCM43XM_NT61.NTx86.Services]
	Include=netvwifibus.inf
	Needs=VWiFiBus.Services
	AddService = BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog

[BCM43XMJ8_NT61.NTx86.Services]
	Include=netvwifibus.inf
	Needs=VWiFiBus.Services
	AddService = BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog

[BCM43XMJ6_NT61.NTx86.Services]
	Include=netvwifibus.inf
	Needs=VWiFiBus.Services
	AddService = BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog

[BCM43XMJ5_NT61.NTx86.Services]
	Include=netvwifibus.inf
	Needs=VWiFiBus.Services
	AddService = BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog

[BCM43XMBO_NT61.NTx86.Services]
	Include=netvwifibus.inf
	Needs=VWiFiBus.Services
	AddService = BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog

[BCM43XNG_NT61.NTx86.Services]
	Include=netvwifibus.inf
	Needs=VWiFiBus.Services
	AddService = BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog

[BCM43XNM_NT61.NTx86.Services]
	Include=netvwifibus.inf
	Needs=VWiFiBus.Services
	AddService = BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog

[BCM43XNMBO_NT61.NTx86.Services]
	Include=netvwifibus.inf
	Needs=VWiFiBus.Services
	AddService = BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog

[BCM43XNMD_NT61.NTx86.Services]
	Include=netvwifibus.inf
	Needs=VWiFiBus.Services
	AddService = BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog

[BCM43XZ_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[BCM43PCMG_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[BCM43XG_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[BCM43XGBO_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[BCM43XA_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[BCM43XM_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[BCM43XMJ8_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[BCM43XMJ6_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[BCM43XMJ5_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[BCM43XMBO_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[BCM43XNG_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[BCM43XNM_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[BCM43XNMBO_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[BCM43XNMD_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration


;-----------------------------------------------------------------
; NT systems
;

[BCM43XX_NT61.reg]
	; Ndis Info
	; Interfaces
	HKR,	Ndi\Interfaces,	UpperRange,	,	"ndis5"
	HKR,	Ndi\Interfaces,	LowerRange,	,	"ethernet,wlan,vwifi"

[BCM43XX.brcm.reg]
	HKR,	Ndi,	HelpText,		,	%BCM43XX_HELP%
	HKR,	Ndi,	Service,		0,	"BCM43XX"

[common.EventLog]
	AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
	HKR,	,	EventMessageFile,	0x00020000,	"%%SystemRoot%%\System32\netevent.dll"
	HKR,	,	TypesSupported,		0x00010001,	7

;-----------------------------------------------------------------
; service-install-section
;

[BCM43XX_NT60.Service.NTx86]
	DisplayName	= %BCM43XX_Service_DispName%
	ServiceType	= 1			; %SERVICE_KERNEL_DRIVER%
	StartType	= 3			; %SERVICE_DEMAND_START%
	ErrorControl	= 1			; %SERVICE_ERROR_NORMAL%
	ServiceBinary	= %12%\bcmwl6.sys
	LoadOrderGroup	= NDIS

;-----------------------------------------------------------------
; filename for CopyFiles
;
; Flag = 2 is COPYFLG_NOSKIP (2)
; Flag = 33 is COPYFLG_WARN_IF_SKIP (1) | COPYFLG_NO_VERSION_DIALOG (32)

[BCM43XX_NT60.files.NTx86]
	BCMWL6.SYS,,,6

; common for WinVista, but excluded in WinXP and older
[common.vista.delreg]
	HKR,,"MPC"
	HKR, Ndi\params\vlan_mode
	HKR,,vlan_mode
	HKR, Ndi\params\PowerSaveMode

; common for all platform
[common.delreg]
	HKR,,"gpiotimerval"
	HKR,,"gpio3"
	HKR,,"gpio2"
	HKR,,"gpio1"
	HKR,,"gpio0"
	HKR, Ndi\params\RoamPref
        HKR, Ndi\params\AssocPref
	HKR, Ndi\params\Locale
	HKR,,Locale
	HKR, Ndi\params\RoamTrigger
	HKR, Ndi\params\WME
	HKR, Ndi\params\MixedCell
	HKR, Ndi\params\Channel
	HKR,,Channel
	HKR, Ndi\params\IBSSGMode
	HKR,,IBSSGMode
	HKR, Ndi\params\Intolerant
	HKR,,Intolerant
	HKLM,Software\Broadcom\802.11,SupportedApps
	       		       
[rate.delreg]
	HKR,	Ndi\params\Rate
	HKR,	Ndi\params\RateA

[country.J8.reg]
	HKR,,	"Country",		0,	"J8"

[country.J6.reg]
	HKR,,	"Country",		0,	"J6"

[country.J5.reg]
	HKR,,	"Country",		0,	"J5"

[country.BO.reg]
	HKR,,	"Country",		0,	"XX"

; common for WinVista, but excluded in WinXP and older
[common.vista.reg]
	HKR, 	Ndi\params\*PriorityVLANTag, ParamDesc,	0,	%PriorityVLANTag%
	HKR, 	Ndi\params\*PriorityVLANTag, type,	0, 	"enum"
	HKR, 	Ndi\params\*PriorityVLANTag\enum, "0",	0,	%PriorityAndVLANDisabled%
	HKR, 	Ndi\params\*PriorityVLANTag\enum, "1",	0,	%PriorityEnabled%
	HKR, 	Ndi\params\*PriorityVLANTag\enum, "2",	0,	%VLANEnabled%
	HKR, 	Ndi\params\*PriorityVLANTag\enum, "3",	0,	%PriorityAndVLANEnabled%
	HKR,    Ndi\params\*PriorityVLANTag,default,,"0"
	HKR,    Ndi\params\*PriorityVLANTag,optional,,"0"

	HKR,	,"PowerSaveMode",	0,	"0"

; common for WinXP and older, but excluded in WinVista
[common.prevista.reg]
	HKR,					,"assoc_recreate",	0,	"1"
        HKR,,   "IBSSAllowed",          0,      "1"
	HKR,,   "ssid_auto_promote",    0,      "0"

; common for all platform
[common.reg]
	HKR, ,"EnableSoftAP", 0, "0"
	HKR, ,"EnableAutoConnect", 0, "0"

	HKR,,	"RoamTrigger",		0,	"2"
	HKR,,	"RoamDelta",		0,	"1"
        HKR,,   "LOM",                  0,      "0"

	HKR,,	"MPC",			0,	"1" ; 1

	HKR,	Ndi\params\frag, ParamDesc,	0,	%FragmentationThreshold%
	HKR,	Ndi\params\frag,type,0,"dword"
	HKR,	Ndi\params\frag,min,,"256"
	HKR,	Ndi\params\frag,max,,"2346"
	HKR,	Ndi\params\frag,default,,"2346"

	HKR,	Ndi\params\rts, ParamDesc,	0,	%RTSThreshold%
	HKR,	Ndi\params\rts,type,0,"dword"
	HKR,	Ndi\params\rts,min,,"0"
	HKR,	Ndi\params\rts,max,,"2347"
	HKR,	Ndi\params\rts,default,,"2347"

	HKR,	Ndi\params\NetworkAddress, ParamDesc,	0, %LocallyAdministeredMACAddress%
	HKR,	Ndi\params\NetworkAddress, type,	0, "edit"
	HKR,	Ndi\params\NetworkAddress, LimitText,	0, "12"
	HKR,	Ndi\params\NetworkAddress, UpperCase,  0, "1"
	HKR,	Ndi\params\NetworkAddress, default,	0, ""
	HKR,	Ndi\params\NetworkAddress, optional,	0, "1"

	HKR,,	"PwrOut",		0,	"100"

	HKR,,	"FrameBursting",	0,	"0"

	HKR,,	"BTCoexist",		0,	"0"

	HKR,					,"WEP",	0,	""
	HKR,					,"NetworkType",	0,	"-1"
	HKR,					,"SSID",	0,	""

	HKR,					,"ledbh0",	0,	"-1"
	HKR,					,"ledbh1",	0,	"-1"
	HKR,					,"ledbh2",	0,	"-1"
	HKR,					,"ledbh3",	0,	"-1"
	HKR,					,"ledblinkslow",	0,	"-1"
	HKR,					,"ledblinkmed",	0,	"-1"
	HKR,					,"ledblinkfast",	0,	"-1"
	HKR,					,"leddc",	0,	"0"

	HKR,					,"scan_channel_time",	0,	"-1"
	HKR,					,"scan_unassoc_time",	0,	"-1"
	HKR,					,"scan_home_time",		0,	"-1"
	HKR,					,"scan_passes",			0,	"-1"

	HKR,					,"BadFramePreempt",		0,	"0"

	HKR,					,"Interference_Mode",		0,	"3"

	HKR,					,"ccx_rm",			0,	"1"
	HKR,					,"ccx_rm_limit",		0,	"300"

	HKR,					,"EFCEnable",		0,	"0"

	HKR,,	"antdiv",		0,	"-1"
	HKR,,	"WME",			0,	"-1"

	HKR,,	"MixedCell", 		0,	"0"

[bg.channels.reg]
	; 2G-band, 20MHz channels supported
	HKR,	Ndi\params\Chanspec\enum, "1",   0, "  1"
	HKR,	Ndi\params\Chanspec\enum, "2",   0, "  2"
	HKR,	Ndi\params\Chanspec\enum, "3",   0, "  3"
	HKR,	Ndi\params\Chanspec\enum, "4",   0, "  4"
	HKR,	Ndi\params\Chanspec\enum, "5",   0, "  5"
	HKR,	Ndi\params\Chanspec\enum, "6",   0, "  6"
	HKR,	Ndi\params\Chanspec\enum, "7",   0, "  7"
	HKR,	Ndi\params\Chanspec\enum, "8",   0, "  8"
	HKR,	Ndi\params\Chanspec\enum, "9",   0, "  9"
	HKR,	Ndi\params\Chanspec\enum, "10",   0, " 10"
	HKR,	Ndi\params\Chanspec\enum, "11",   0, " 11"
	HKR,	Ndi\params\Chanspec\enum, "12",   0, " 12"
	HKR,	Ndi\params\Chanspec\enum, "13",   0, " 13"
	HKR,	Ndi\params\Chanspec\enum, "14",   0, " 14"

[nbg.channels.reg]
	; Chanspec parameters
	; 2G-band, 20MHz channels supported
	HKR,	Ndi\params\Chanspec\enum, "1",   0, "  1(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "2",   0, "  2(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "3",   0, "  3(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "4",   0, "  4(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "5",   0, "  5(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "6",   0, "  6(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "7",   0, "  7(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "8",   0, "  8(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "9",   0, "  9(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "10",   0, " 10(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "11",   0, " 11(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "12",   0, " 12(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "13",   0, " 13(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "14",   0, " 14(20MHz)"

	; 2G-band, 40MHz channels supported
	HKR,	Ndi\params\Chanspec\enum, "1bl",   0, "  1(40MHz-L)"
	HKR,	Ndi\params\Chanspec\enum, "6bl",   0, "  6(40MHz-L)"
	HKR,	Ndi\params\Chanspec\enum, "6bu",   0, "  6(40MHz-U)"
	HKR,	Ndi\params\Chanspec\enum, "11bu",  0, " 11(40MHz-U)"

[a.channels.reg]
	; 5G-band, 20MHz channels supported
	; USA Low Band
	HKR,	Ndi\params\Chanspec\enum, "36",   0, " 36"
	HKR,	Ndi\params\Chanspec\enum, "40",   0, " 40"
	HKR,	Ndi\params\Chanspec\enum, "44",   0, " 44"
	HKR,	Ndi\params\Chanspec\enum, "48",   0, " 48"
	HKR,	Ndi\params\Chanspec\enum, "52",   0, " 52"
	HKR,	Ndi\params\Chanspec\enum, "56",   0, " 56"
	HKR,	Ndi\params\Chanspec\enum, "60",   0, " 60"
	HKR,	Ndi\params\Chanspec\enum, "64",   0, " 64"
	; Europe
	HKR,	Ndi\params\Chanspec\enum, "100",   0, "100"
	HKR,	Ndi\params\Chanspec\enum, "104",   0, "104"
	HKR,	Ndi\params\Chanspec\enum, "108",   0, "108"
	HKR,	Ndi\params\Chanspec\enum, "112",   0, "112"
	HKR,	Ndi\params\Chanspec\enum, "116",   0, "116"
	HKR,	Ndi\params\Chanspec\enum, "120",   0, "120"

	HKR,	Ndi\params\Chanspec\enum, "124",   0, "124"
	HKR,	Ndi\params\Chanspec\enum, "128",   0, "128"
	HKR,	Ndi\params\Chanspec\enum, "132",   0, "132"
	HKR,	Ndi\params\Chanspec\enum, "136",   0, "136"
	HKR,	Ndi\params\Chanspec\enum, "140",   0, "140"

; 	Additional channels supported only on SPROM map version 2
;	HKR,	Ndi\params\Chanspec\enum, "149",   0, "149"
;	HKR,	Ndi\params\Chanspec\enum, "153",   0, "153"
;	HKR,	Ndi\params\Chanspec\enum, "157",   0, "157"
;	HKR,	Ndi\params\Chanspec\enum, "161",   0, "161"
;	HKR,	Ndi\params\Chanspec\enum, "165",   0, "165"

[na.channels.reg]
	; Chanspec parameters
	; USA Low Band
	HKR,	Ndi\params\Chanspec\enum, "36",   0, " 36(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "40",   0, " 40(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "44",   0, " 44(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "48",   0, " 48(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "52",   0, " 52(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "56",   0, " 56(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "60",   0, " 60(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "64",   0, " 64(20MHz)"
	; Europe
	HKR,	Ndi\params\Chanspec\enum, "100",   0, "100(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "104",   0, "104(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "108",   0, "108(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "112",   0, "112(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "116",   0, "116(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "120",   0, "120(20MHz)"

	HKR,	Ndi\params\Chanspec\enum, "124",   0, "124(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "128",   0, "128(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "132",   0, "132(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "136",   0, "136(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "140",   0, "140(20MHz)"

	HKR,	Ndi\params\Chanspec\enum, "149",   0, "149(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "153",   0, "153(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "157",   0, "157(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "161",   0, "161(20MHz)"
	HKR,	Ndi\params\Chanspec\enum, "165",   0, "165(20MHz)"

	; 5G-band, 40MHz channels supported
	HKR,	Ndi\params\Chanspec\enum, "36al",   0, " 36(40MHz-L)"
	HKR,	Ndi\params\Chanspec\enum, "44al",   0, " 44(40MHz-L)"
	HKR,	Ndi\params\Chanspec\enum, "52al",   0, " 52(40MHz-L)"
	HKR,	Ndi\params\Chanspec\enum, "60al",   0, " 60(40MHz-L)"
	; Europe
	HKR,	Ndi\params\Chanspec\enum, "100al",   0, "100(40MHz-L)"
	HKR,	Ndi\params\Chanspec\enum, "108al",   0, "108(40MHz-L)"
	HKR,	Ndi\params\Chanspec\enum, "116al",   0, "116(40MHz-L)"

	HKR,	Ndi\params\Chanspec\enum, "124al",   0, "124(40MHz-L)"
	HKR,	Ndi\params\Chanspec\enum, "132al",   0, "132(40MHz-L)"

	HKR,	Ndi\params\Chanspec\enum, "149al",   0, "149(40MHz-L)"
	HKR,	Ndi\params\Chanspec\enum, "157al",   0, "157(40MHz-L)"

[b.options.reg]
	HKR,,	"PLCPHeader",		0,	"0"

	HKR,	Ndi\params\Rate, ParamDesc,	0,	%Rate%
	HKR,	Ndi\params\Rate, type,		0,	"enum"
	HKR,	Ndi\params\Rate\enum, "0",	0,	%Usebestrate%
	HKR,	Ndi\params\Rate\enum, "2",	0,	" 1"
	HKR,	Ndi\params\Rate\enum, "4",	0,	" 2"
	HKR,	Ndi\params\Rate\enum, "11",	0,	" 5.5"
	HKR,	Ndi\params\Rate\enum, "22",	0,	"11"
	HKR,	Ndi\params\Rate,default,,"0"

[g.options.reg]
	HKR,,	"PLCPHeader",		0,	"0"

	HKR,    Ndi\params\IBSSMode, ParamDesc,	   0,      %IBSS54gtmMode%
	HKR,    Ndi\params\IBSSMode, type,         0,      "enum"
	HKR,    Ndi\params\IBSSMode\enum, "0",     0,      %80211bOnly%
	HKR,    Ndi\params\IBSSMode\enum, "2",     0,      %54gAuto%
	HKR,    Ndi\params\IBSSMode\enum, "4",     0,      %54gPerformance%
	HKR,    Ndi\params\IBSSMode,default,,"0"

	HKR,    Ndi\params\IBSSGProtection, ParamDesc,	0,      %IBSS54gtmProtectionMode%
	HKR,    Ndi\params\IBSSGProtection, type,       0,      "enum"
	HKR,    Ndi\params\IBSSGProtection\enum, "0",   0,      %Disabled%
	HKR,    Ndi\params\IBSSGProtection\enum, "2",   0,      %Auto%
	HKR,    Ndi\params\IBSSGProtection,default,,"2"

	HKR,	Ndi\params\Rate, ParamDesc,	0,	%Rate%
	HKR,	Ndi\params\Rate, type,		0,	"enum"
	HKR,	Ndi\params\Rate\enum, "0",	0,	%Usebestrate%
	HKR,	Ndi\params\Rate\enum, "2",	0,	" 1"
	HKR,	Ndi\params\Rate\enum, "4",	0,	" 2"
	HKR,	Ndi\params\Rate\enum, "11",	0,	" 5.5"
	HKR,	Ndi\params\Rate\enum, "12",	0,	" 6"
	HKR,	Ndi\params\Rate\enum, "18",	0,	" 9"
	HKR,	Ndi\params\Rate\enum, "22",	0,	"11"
	HKR,	Ndi\params\Rate\enum, "24",	0,	"12"
	HKR,	Ndi\params\Rate\enum, "36",	0,	"18"
	HKR,	Ndi\params\Rate\enum, "48",	0,	"24"
	HKR,	Ndi\params\Rate\enum, "72",	0,	"36"
	HKR,	Ndi\params\Rate\enum, "96",	0,	"48"
	HKR,	Ndi\params\Rate\enum, "108",0,	"54"
	HKR,	Ndi\params\Rate,default,,"0"

	HKR,,	"Afterburner",		0,      "0"

[gn.options.reg]
	HKR,,	"PLCPHeader",		0,	"0"

	HKR,    Ndi\params\IBSSMode, ParamDesc,	0,      %IBSSMode%
	HKR,    Ndi\params\IBSSMode, type,         0,      "enum"
	HKR,    Ndi\params\IBSSMode\enum, "0",     0,      %80211abOnly%
	HKR,    Ndi\params\IBSSMode\enum, "2",     0,      %80211abgAuto%
	HKR,    Ndi\params\IBSSMode\enum, "4",     0,      %80211abgPerf%
	HKR,    Ndi\params\IBSSMode\enum, "5",     0,      %80211abgnAuto%
	HKR,    Ndi\params\IBSSMode,default,,"0"

	HKR,    Ndi\params\IBSSGProtection, ParamDesc,	0,      %IBSS54gtmProtectionMode%
	HKR,    Ndi\params\IBSSGProtection, type,       0,      "enum"
	HKR,    Ndi\params\IBSSGProtection\enum, "0",   0,      %Disabled%
	HKR,    Ndi\params\IBSSGProtection\enum, "2",   0,      %Auto%
	HKR,    Ndi\params\IBSSGProtection,default,,"2"

	HKR,	Ndi\params\Rate, ParamDesc,	0,	%Rate%
	HKR,	Ndi\params\Rate, type,		0,	"enum"
	HKR,	Ndi\params\Rate\enum, "0",	0,	%Usebestrate%
	HKR,	Ndi\params\Rate\enum, "2",	0,	" 1"
	HKR,	Ndi\params\Rate\enum, "4",	0,	" 2"
	HKR,	Ndi\params\Rate\enum, "11",	0,	" 5.5"
	HKR,	Ndi\params\Rate\enum, "12",	0,	" 6"
	HKR,	Ndi\params\Rate\enum, "18",	0,	" 9"
	HKR,	Ndi\params\Rate\enum, "22",	0,	"11"
	HKR,	Ndi\params\Rate\enum, "24",	0,	"12"
	HKR,	Ndi\params\Rate\enum, "36",	0,	"18"
	HKR,	Ndi\params\Rate\enum, "48",	0,	"24"
	HKR,	Ndi\params\Rate\enum, "72",	0,	"36"
	HKR,	Ndi\params\Rate\enum, "96",	0,	"48"
	HKR,	Ndi\params\Rate\enum, "108",0,	"54"
	HKR,	Ndi\params\Rate,default,,"0"

	HKR,,	"Afterburner",		0,      "0"
        
	HKR,    Ndi\params\Intolerant, ParamDesc,	0,      %Intolerant%
	HKR,    Ndi\params\Intolerant, type,         0,      "enum"
	HKR,    Ndi\params\Intolerant\enum, "0",     0,      %Disabled%
	HKR,    Ndi\params\Intolerant\enum, "1",     0,      %Enabled%
	HKR,    Ndi\params\Intolerant,default,,"0"

	; option to override antenna selection, -1: no override, 0: no selection
	HKR,					,"mimo_antsel",	0,	"-1"

; options common to both b and g
[bg.options.reg]
	HKR,,	"Chanspec",		0, 	"11"
	HKR,,	"ApCompatMode",		0,	"0"
	  
[a.options.reg]
	HKR,,	"Afterburner",		0,      "0"

	HKR,	Ndi\params\RateA, ParamDesc,	0,	%Rate_802_11a%
	HKR,	Ndi\params\RateA, type,		0,	"enum"
	HKR,	Ndi\params\RateA\enum, "0",	0,	%Usebestrate%
	HKR,	Ndi\params\RateA\enum, "12",	0,	" 6"
	HKR,	Ndi\params\RateA\enum, "18",	0,	" 9"
	HKR,	Ndi\params\RateA\enum, "24",	0,	"12"
	HKR,	Ndi\params\RateA\enum, "36",	0,	"18"
	HKR,	Ndi\params\RateA\enum, "48",	0,	"24"
	HKR,	Ndi\params\RateA\enum, "72",	0,	"36"
	HKR,	Ndi\params\RateA\enum, "96",	0,	"48"
	HKR,	Ndi\params\RateA\enum, "108",0,	"54"
	HKR,	Ndi\params\RateA,default,,"0"

	HKR,,	"Chanspec",		0,	"36"

[bag.options.reg]
	HKR,,	"Afterburner",		0,      "0"

	HKR,, 	"11HNetworks", 		0, 	"1"
	HKR,,	"PLCPHeader",		0,	"0"
	HKR,,	"band",			0,	"0"
	HKR,,	"BandPref",		0,	"0"
	HKR,,	"AssocRoamPref",	0,	"0"

	HKR,    Ndi\params\IBSSMode, ParamDesc,	   0,      %IBSS54gtmMode%
	HKR,    Ndi\params\IBSSMode, type,         0,      "enum"
	HKR,    Ndi\params\IBSSMode\enum, "0",     0,      %80211bOnly%
	HKR,    Ndi\params\IBSSMode\enum, "2",     0,      %54gAuto%
	HKR,    Ndi\params\IBSSMode\enum, "4",     0,      %54gPerformance%
	;default from bcmwl5[ei].inf

	HKR,    Ndi\params\IBSSGProtection, ParamDesc,	0,      %IBSS54gtmProtectionMode%
	HKR,    Ndi\params\IBSSGProtection, type,       0,      "enum"
	HKR,    Ndi\params\IBSSGProtection\enum, "0",   0,      %Disabled%
	HKR,    Ndi\params\IBSSGProtection\enum, "2",   0,      %Auto%
	HKR,    Ndi\params\IBSSGProtection,default,,"2"


	HKR,	Ndi\params\RateA, ParamDesc,	0,	%Rate_802_11a%
	HKR,	Ndi\params\RateA, type,		0,	"enum"
	HKR,	Ndi\params\RateA\enum, "0",	0,	%Usebestrate%
	HKR,	Ndi\params\RateA\enum, "12",	0,	" 6"
	HKR,	Ndi\params\RateA\enum, "18",	0,	" 9"
	HKR,	Ndi\params\RateA\enum, "24",	0,	"12"
	HKR,	Ndi\params\RateA\enum, "36",	0,	"18"
	HKR,	Ndi\params\RateA\enum, "48",	0,	"24"
	HKR,	Ndi\params\RateA\enum, "72",	0,	"36"
	HKR,	Ndi\params\RateA\enum, "96",	0,	"48"
	HKR,	Ndi\params\RateA\enum, "108",0,	"54"
	HKR,	Ndi\params\RateA,default,,"0"


	HKR,	Ndi\params\Rate, ParamDesc,	0,	%Rate_802_11bg%
	HKR,	Ndi\params\Rate, type,		0,	"enum"
	HKR,	Ndi\params\Rate\enum, "0",	0,	%Usebestrate%
	HKR,	Ndi\params\Rate\enum, "2",	0,	" 1"
	HKR,	Ndi\params\Rate\enum, "4",	0,	" 2"
	HKR,	Ndi\params\Rate\enum, "11",	0,	" 5.5"
	HKR,	Ndi\params\Rate\enum, "12",	0,	" 6"
	HKR,	Ndi\params\Rate\enum, "18",	0,	" 9"
	HKR,	Ndi\params\Rate\enum, "22",	0,	"11"
	HKR,	Ndi\params\Rate\enum, "24",	0,	"12"
	HKR,	Ndi\params\Rate\enum, "36",	0,	"18"
	HKR,	Ndi\params\Rate\enum, "48",	0,	"24"
	HKR,	Ndi\params\Rate\enum, "72",	0,	"36"
	HKR,	Ndi\params\Rate\enum, "96",	0,	"48"
	HKR,	Ndi\params\Rate\enum, "108",0,	"54"
	HKR,	Ndi\params\Rate,default,,"0"

	HKR,,	"Chanspec",		0,	"11"
	HKR,,	"ApCompatMode",		0,	"0"

[bagn.options.reg]
	HKR,,	"Afterburner",		0,      "0"

	HKR,, 	"11HNetworks", 		0, 	"1"
	HKR,,	"PLCPHeader",		0,	"0"
	HKR,,	"band",			0,	"0"
	HKR,,	"BandPref",		0,	"0"
	HKR,,	"AssocRoamPref",	0,	"0"

	HKR,    Ndi\params\IBSSMode, ParamDesc,	0,      %IBSSMode%
	HKR,    Ndi\params\IBSSMode, type,         0,      "enum"
	HKR,    Ndi\params\IBSSMode\enum, "0",     0,      %80211abOnly%
	HKR,    Ndi\params\IBSSMode\enum, "2",     0,      %80211abgAuto%
	HKR,    Ndi\params\IBSSMode\enum, "4",     0,      %80211abgPerf%
	HKR,    Ndi\params\IBSSMode\enum, "5",     0,      %80211abgnAuto%
	HKR,    Ndi\params\IBSSMode,default,,"0"

	HKR,    Ndi\params\IBSSGProtection, ParamDesc,	0,      %IBSS54gtmProtectionMode%
	HKR,    Ndi\params\IBSSGProtection, type,       0,      "enum"
	HKR,    Ndi\params\IBSSGProtection\enum, "0",   0,      %Disabled%
	HKR,    Ndi\params\IBSSGProtection\enum, "2",   0,      %Auto%
	HKR,    Ndi\params\IBSSGProtection,default,,"2"

	HKR,	Ndi\params\RateA, ParamDesc,	0,	%Rate_802_11a%
	HKR,	Ndi\params\RateA, type,		0,	"enum"
	HKR,	Ndi\params\RateA\enum, "0",	0,	%Usebestrate%
	HKR,	Ndi\params\RateA\enum, "12",	0,	" 6"
	HKR,	Ndi\params\RateA\enum, "18",	0,	" 9"
	HKR,	Ndi\params\RateA\enum, "24",	0,	"12"
	HKR,	Ndi\params\RateA\enum, "36",	0,	"18"
	HKR,	Ndi\params\RateA\enum, "48",	0,	"24"
	HKR,	Ndi\params\RateA\enum, "72",	0,	"36"
	HKR,	Ndi\params\RateA\enum, "96",	0,	"48"
	HKR,	Ndi\params\RateA\enum, "108",0,	"54"
	HKR,	Ndi\params\RateA,default,,"0"

	HKR,	Ndi\params\Rate, ParamDesc,	0,	%Rate_802_11bg%
	HKR,	Ndi\params\Rate, type,		0,	"enum"
	HKR,	Ndi\params\Rate\enum, "0",	0,	%Usebestrate%
	HKR,	Ndi\params\Rate\enum, "2",	0,	" 1"
	HKR,	Ndi\params\Rate\enum, "4",	0,	" 2"
	HKR,	Ndi\params\Rate\enum, "11",	0,	" 5.5"
	HKR,	Ndi\params\Rate\enum, "12",	0,	" 6"
	HKR,	Ndi\params\Rate\enum, "18",	0,	" 9"
	HKR,	Ndi\params\Rate\enum, "22",	0,	"11"
	HKR,	Ndi\params\Rate\enum, "24",	0,	"12"
	HKR,	Ndi\params\Rate\enum, "36",	0,	"18"
	HKR,	Ndi\params\Rate\enum, "48",	0,	"24"
	HKR,	Ndi\params\Rate\enum, "72",	0,	"36"
	HKR,	Ndi\params\Rate\enum, "96",	0,	"48"
	HKR,	Ndi\params\Rate\enum, "108",0,	"54"
	HKR,	Ndi\params\Rate,default,,"0"

	HKR,,	"Chanspec",		0,	"11"
	HKR,,	"ApCompatMode",		0,	"0"

	HKR,    Ndi\params\Intolerant, ParamDesc,	0,      %Intolerant%
	HKR,    Ndi\params\Intolerant, type,         0,      "enum"
	HKR,    Ndi\params\Intolerant\enum, "0",     0,      %Disabled%
	HKR,    Ndi\params\Intolerant\enum, "1",     0,      %Enabled%
	HKR,    Ndi\params\Intolerant,default,,"0"

	HKR, 	Ndi\params\11NPreamble, ParamDesc,  0, 	"802.11n Preamble"
	HKR, 	Ndi\params\11NPreamble, type, 		0, "enum"
	HKR, 	Ndi\params\11NPreamble\enum, "-1", 	0, %Green_Field_Mode%
	HKR, 	Ndi\params\11NPreamble\enum, "0", 	0, %Mixed_Mode%
	HKR, 	Ndi\params\11NPreamble,default,,"-1"

[DestinationDirs]
	DefaultDestDir=11
	BCM43XX.sys.files=11
	BCM43XX.files.NT = 12
	BCM43XX_NT60.files.NTx86 = 12

[SourceDisksNames]
	1=%BCM43XX_DiskName%,,

; for WinVista specify BCMWL6.SYS
[SourceDisksFiles.x86]
	bcmwl6.sys=1

; for WinVista specify BCMWL6.SYS
[SourceDisksFiles]
	bcmwl6.sys=1

[strings]
; Non-Localizable strings
MSFT= "Microsoft"
V_BCM="Broadcom"

; Localizable strings
BCM430G_DeviceDesc="Broadcom 802.11g Network Adapter"
BCM430A_DeviceDesc="Broadcom 802.11a Network Adapter"
BCM430N_DeviceDesc="Broadcom 802.11n Network Adapter"
BCM430M_DeviceDesc="Broadcom 802.11 Multiband Network Adapter"
BCM430G_USR_PC_DeviceDesc="U.S. Robotics Wireless 802.11g PC Card Adapter"
BCM430G_USR_PCI_DeviceDesc= "U.S. Robotics Wireless 802.11g PCI Adapter"
BCM430N_USR_PC_DeviceDesc="USRobotics Wireless MAXn PC Card"
BCM430N_USR_PCI_DeviceDesc="USRobotics Wireless MAXn PCI Adapter" 
BCM430G_LNK_SPB_DeviceDesc="Linksys Wireless-G Notebook Adapter with SpeedBooster"
BCM430G_LNK_DeviceDesc="Linksys Wireless-G Notebook Adapter WPC54G V3"
BCM430N_LNK_DeviceDesc="Linksys Wireless-N Notebook Adapter WPC300N"
BCM430N_NTGR_PC_DeviceDesc="RangeMax Next Wireless Notebook Adapter"
BCM430N_NTGR_PCI_DeviceDesc="RangeMax Next Wireless PCI Adapter"
BCM430G_MSFT_PC_DeviceDesc="Microsoft Wireless Notebook Adapter MN-720"
BCM430G_MSFT_PCI_DeviceDesc="Microsoft Wireless Notebook Adapter MN-730"
BCM430G_DELL_DeviceDesc="Dell TrueMobile 1300 WLAN Mini-PCI Card"
BCM430GC_DeviceDesc="Dell TrueMobile 1300 WLAN PC Card"
BCM430M_DELL_DeviceDesc="Dell TrueMobile 1400 Dual Band WLAN Mini-PCI Card"
BCM430MC_DeviceDesc="Dell TrueMobile 1400 Dual Band WLAN PC Card"
BCM1350M_DeviceDesc="Dell Wireless 1350 WLAN Mini-PCI Card"
BCM1370M_DeviceDesc="Dell Wireless 1370 WLAN Mini-PCI Card"
BCM1450M_DeviceDesc="Dell Wireless 1450 Dual Band WLAN Mini-PCI Card"
BCM1470M_DeviceDesc="Dell Wireless 1470 Dual Band WLAN Mini-PCI Card"
BCM1350C_DeviceDesc="Dell Wireless 1350 WLAN PC Card"
BCM1370C_DeviceDesc="Dell Wireless 1370 WLAN PC Card"
BCM1450C_DeviceDesc="Dell Wireless 1450 Dual Band WLAN PC Card"
BCM1470C_DeviceDesc="Dell Wireless 1470 Dual Band WLAN PC Card"
BCM1390M_DeviceDesc="Dell Wireless 1390 WLAN Mini-Card"
BCM1390E_DeviceDesc="Dell Wireless 1390 WLAN ExpressCard"
BCM1490M_DeviceDesc="Dell Wireless 1490 Dual Band WLAN Mini-Card"
BCM1490E_DeviceDesc="Dell Wireless 1490 Dual Band WLAN ExpressCard"
BCM1500M_DeviceDesc="Dell Wireless 1500 Draft 802.11n WLAN Mini-Card"
BCM1505M_DeviceDesc="Dell Wireless 1505 Draft 802.11n WLAN Mini-Card"
BCM1395M_DeviceDesc="Dell Wireless 1395 WLAN Mini-Card"
BCM1397HMG_DeviceDesc="Dell Wireless 1397 WLAN Mini-Card"
BCM1510HM8L_DeviceDesc="Dell Wireless 1510 Wireless-N WLAN Mini-Card"
BCM430NM_DeviceDesc="Broadcom 4321AG 802.11a/b/g/draft-n Wi-Fi Adapter"
BCM4322NM_DeviceDesc="Broadcom 4322AG 802.11a/b/g/draft-n Wi-Fi Adapter"
BCM43XX_HELP="The Broadcom 802.11 Network Adapter provides wireless local area networking."
BCM43XX_Service_DispName="Broadcom 802.11 Network Adapter Driver"
PriorityVLANTag="Priority & VLAN"
PriorityAndVLANDisabled="Priority & VLAN Disabled"
PriorityAndVLANEnabled="Priority & VLAN Enabled"
PriorityEnabled="Priority Enabled"
VLANEnabled="VLAN Enabled"
FragmentationThreshold="Fragmentation Threshold"
RTSThreshold="RTS Threshold"
LocallyAdministeredMACAddress="Locally Administered MAC Address"
Rate="Rate"
Usebestrate="Best Rate"
IBSS54gtmMode="IBSS 54g(tm) Mode"
80211bOnly="802.11b Only"
54gAuto="54g - Auto"
54gPerformance="54g - Performance"
IBSS54gtmProtectionMode="IBSS 54g(tm) Protection Mode"
Disabled="Disabled"
Auto="Auto"
IBSSMode="IBSS Mode"
80211abOnly="802.11a/b Only"
80211abgAuto="802.11a/b/g Auto"
80211abgPerf="802.11a/b/g Performance"
80211abgnAuto="802.11a/b/g/n Auto"
Intolerant="40MHz Intolerant"
Enabled="Enabled"
Rate_802_11a="Rate (802.11a)"
Rate_802_11bg="Rate (802.11b/g)"
Green_Field_Mode="Green Field Mode"
Mixed_Mode="Mixed Mode"
BCM43XX_DiskName="802.11 Network Adapter Install Disk"
