;                     
; Remote NDIS template device setup file
; Copyright (c) Microsoft Corporation
;
; This is the template for the INF installation script 
; for the RNDIS-over-USB host driver.
; This INF works for Windows XP SP2, Windows XP x64, 
; Windows Server 2003 SP1 x86, x64, and ia64, and 
; Windows Vista x86 and x64.
; This INF will work with Windows XP, Windows XP SP1, 
; and Windows 2003 after applying specific hotfixes.

[Version]
Signature           = "$Windows NT$"
Class               = Net
ClassGUID           = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider            = %Microsoft%
DriverVer=06/21/2006,6.1.7600.16385
;CatalogFile        = device.cat

[Manufacturer]
%Microsoft%         = RndisDevices,NTx86,NTamd64,NTia64

; Decoration for x86 architecture
[RndisDevices.NTx86]
;when MSID is used for RNDIS Ethernet devices over USB transport 
%RndisDevice%    = RNDIS.NT.6.0, USB\MS_COMP_RNDIS&MS_SUBCOMP_5162001
;when CompatID is used for RNDIS Ethernet devices over USB transport 
%RndisDevice%    = RNDIS.NT.6.0, USB\Class_EF&SubClass_04&Prot_01

; Decoration for x64 architecture
[RndisDevices.NTamd64]
;when MSID is used for RNDIS Ethernet devices over USB transport 
%RndisDevice%    = RNDIS.NT.6.0, USB\MS_COMP_RNDIS&MS_SUBCOMP_5162001
;when CompatID is used for RNDIS Ethernet devices over USB transport 
%RndisDevice%    = RNDIS.NT.6.0, USB\Class_EF&SubClass_04&Prot_01

; Decoration for ia64 architecture
[RndisDevices.NTia64]
;when MSID is used for RNDIS Ethernet devices over USB transport 
%RndisDevice%    = RNDIS.NT.6.0, USB\MS_COMP_RNDIS&MS_SUBCOMP_5162001
;when CompatID is used for RNDIS Ethernet devices over USB transport 
%RndisDevice%    = RNDIS.NT.6.0, USB\Class_EF&SubClass_04&Prot_01

;@@@ This is the common setting for setup
[ControlFlags]
ExcludeFromSelect=*

; DDInstall section
; References the in-build Netrndis.inf
[RNDIS.NT.6.0]
Characteristics = 0x84   ; NCF_PHYSICAL + NCF_HAS_UI
BusType         = 15
; NEVER REMOVE THE FOLLOWING REFERENCE FOR NETRNDIS.INF
include            = netrndis.inf
needs              = usbrndis6.ndi
AddReg             = Rndis_AddReg_Vista
*IfType            = 6    ; IF_TYPE_ETHERNET_CSMACD.
*MediaType         = 0   ; NdisMediumNative802_3
*PhysicalMediaType = 14   ; NdisPhysicalMedium802_3

; DDInstal.Services section
[RNDIS.NT.6.0.Services]
include     = netrndis.inf
needs       = usbrndis6.ndi.Services


; Optional registry settings. You can modify as needed.
[RNDIS_AddReg_Vista] 
HKR, NDI\params\VistaProperty, ParamDesc,  0, %Vista_Property%
HKR, NDI\params\VistaProperty, type,       0, "edit"
HKR, NDI\params\VistaProperty, LimitText,  0, "12"
HKR, NDI\params\VistaProperty, UpperCase,  0, "1"
HKR, NDI\params\VistaProperty, default,    0, " "
HKR, NDI\params\VistaProperty, optional,   0, "1"

; No sys copyfiles - the sys files are already in-build 
; (part of the operating system).

; Modify these strings for your device as needed.
[Strings]
Microsoft             = "Microsoft Corporation"
RndisDevice           = "Remote NDIS Compatible Device"
Vista_Property        = "Optional Vista Property"
